{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":20,"n_cols":13,"rows_kept":20,"merged":[[0,0,0,8],[1,0,1,12],[16,0,16,8],[17,0,17,8],[18,0,18,8],[19,0,19,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2024年6月机械备件采购项目                   项目编号：HG JY-G2024081"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,5800200112,"拖链","TL125-Ⅱ;200*420*3125","铝型材支撑板II型;两侧长孔70*100;中间长孔70*150","件",5,"JB/T6608-1993","炼钢厂部","2024-08-26"]
[2,7102100013,"气动控制阀门","D376XE72",null,"只",3,"ISO5211","89热轧","2024-08-26"]
[3,7001200350,"除磷环喷嘴紫铜垫","MQL-CLH-01","材质：紫铜；重量：0.02kg","只",100,"审核图纸","89管加工热处理","2024-08-26"]
[4,7502500119,"冷却塔;风叶总成","LF-50","Q=45×104m3/h，与Φ5000风筒及NGW-L-F61-22KW减速箱配套，","套",1,"Q/YB01-2009","89管加工热处理","2024-08-26"]
[5,5601500003,"自预热高速燃烧器","WD-GZYS-200H","1Cr18Ni9Ti和Cr25Ni20,85Kg;焊缝无夹杂、气孔等缺陷;法兰面不能有焊渣;保证法兰面平整;所有位置满焊;不能出现漏气的焊孔。","只",2,"JB/T10697-2007","炼钢厂部","2024-08-26"]
[6,5502000041,"一极出灰刮板输送机","YD250G","输送物料:粉尘;输送长度:25.8m;输灰量:6.5立方/h;机槽宽度:25㎝;链条节距:15厘米;传动方式:链条传动;减速机型号:BWY3332-187-5.5-4;电机功率:5.5kw;电机防护等级:IP54;电源:380v;50HZ","套",1,"审核图纸","高辅工段","2024-08-26"]
[7,7502300037,"双介质气雾喷枪","621072303-03-00-2","P=0.6MP;Qmax3.7T/H;＜120°;￠3500;H~3000;枪长1600;开孔273;316L护板","把",2,"GB/T4213-1992","炼钢厂部","2024-08-26"]
[8,4201200045,"火焰清理枪","QLQ-2","总长2m;枪头长280mm;氧气接头螺纹M18*1.5;燃气接头螺纹M16*1.5反丝;材质;手柄铜（H59-1);枪头材质耐热钢","把",10,"GB5108-1985","炼钢厂部","2024-08-26"]
[9,4201200046,"清理嘴","QLZ-2","长度280mm;氧气接头螺纹M16*1.5;燃气接头螺纹M16*1","个",20,"GB5108-1985","炼钢厂部","2024-08-26"]
[10,5800100035,"压缩弹簧","d=22;D=210;H0=900;有效圈数10;两段并紧磨平","65Si2MnA","根",2,"GB/T1972-1992","720厂部","2024-08-26"]
[11,5704900004,"内磨机磨杆","M52型","长度6.9m,直径52mm,内轴20mm,80kg","根",2,"JB/T3715-2016","180热轧","2024-08-26"]
[12,5400100162,"离心式空压机 后冷却器","S050 1006","\"FS-ELLIOTT 260 传热面积：46.27㎡\n，外壳最大工作压力:0.6Mpa、最大工作温度：104℃，换热器最大工作压力：1.0Mpa、最大工作温度248℃\"","台",1,"GB151-1999","能源厂部","2024-08-26"]
[13,6600200826,"电动执行器","E110","执行器旋转90°用时12s;扭矩400Nm;额定电流1.0A;启动电流1.8A;功率0.2275Kw;额定电压380VAC;频率50Hz;工作循环等级C;防护等级IP67","台",1,"JB/T10391-2002","炼钢厂部","2024-08-26"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2024年6月机械备件采购项目          项目编号：HG JY-G2024081"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]