{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":48,"n_cols":13,"rows_kept":48,"merged":[[0,0,0,11],[1,0,1,11],[44,0,44,8],[45,0,45,8],[46,0,46,8],[47,0,47,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2024年7月至2025年6月机电备件年度采购项目                    项目编号：HG JY-G2024079"]
["序号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,6400100009,"热金属检测器探头","OSA6747.18G","2米电缆 订货号6136A","CNS12081-1987","件",8,"各二级厂","按合同计划交货期交货"]
[2,6400200066,"热金属检测器","LOS-R2-4ZC1","反光板型 直流24V 输出形式pnp和继电器一常开一常闭 快速接头10芯引出线 带反光板SP-17/N 环境温度-25℃-+120℃","Q/3204BCK010-2013","台",30,"各二级厂","按合同计划交货期交货"]
[3,6400600114,"激光测距传感器","LTF-12-I-C2-LD-Q 德国DIN","12-30VDC:4-20MA","德国DIN","只",13,"各二级厂","按合同计划交货期交货"]
[4,6400600338,"位移传感器","DG-155P-L605;带磁头","精度5um，测量范围155mm,SONY",null,"个",12,"各二级厂","按合同计划交货期交货"]
[5,6100100160,"全相双安全保护装置","EAT-2.5D-13.5/600","直流电压不小于18.6 额定电压10.5，残压31","GB/T208001-2001","台",1,"各二级厂","按合同计划交货期交货"]
[6,6100100031,"交流电焊机","BX3-500-2","380V","GB/T8118-1995","台",33,"各二级厂","按合同计划交货期交货"]
[7,6200100036,"停电保护控制系统 蓄电池","LC-P12100 100Ah/12V XK06-006-00420","规格型号：LC-P12100 100Ah/12V","XK06-006-00420","组",128,"各二级厂","按合同计划交货期交货"]
[8,6400600240,"位移传感器","BTL7-E100-M0225-B-KA05;","含磁环","GB/T14048","只",9,"各二级厂","按合同计划交货期交货"]
[9,6200200658,"风机","D4E225-CC01-39;ebmpast","电压:230V;频率:50/60HZ;电流:2.4/2.75A;功率:540/625W;转速;1210/1300min-1;电容:16uF(P2) 400VDB;效率:40.2%;生产厂家:ebmpast",null,"台",1,"各二级厂","按合同计划交货期交货"]
[10,6100700015,"电流互感器","LDJ6-35","户内50Hz;额定绝缘水平40.5/95/185KV;额定电流比400/5;额定输出15VA;准确级次0.5;短时热电流1S 54KA;额定动稳定电流120KA","GB1208-2006","台",1,"各二级厂","按合同计划交货期交货"]
[11,6100900095,"120/45 通用车控电气控制柜","LC8911","含电机断路器（GV2ME14C+GV AE-11)1台、直流接触器（LC1D12BDC DC24V)1台、可编程控制器（14IN-10 OUT)1台、继电器模组（MZ-16A 4路DC24V）1只、红色指示灯（DC24V)3只、绿色指示灯（DC24V)1只、熔断器（RT28N 2A)2只、端子排（30*3+15*30）一组",null,"台",1,"各二级厂","按合同计划交货期交货"]
[12,6100400371,"无触点控制器","TDF-200A-3PJ","电源380V无触点通断，HMI编程面板，正反转延时保护，缺相保护，过流保护，偏流保护，宽电压设计，带有输出辅助触点，，故障报警可储存，通断无火花，实时电流监视。",null,"只",1,"各二级厂","按合同计划交货期交货"]
[13,6400600245,"位移传感器","CI43-6-1BH04T40135XA4201A","量程135mm；电源24VDC;输出4-20mA，测量起始端以外保持4mA输出；超出测量末端保持20mA输出。5米屏蔽电缆直接；带磁环。Q/JT01-2011","Q/JT01-2011","台",5,"各二级厂","按合同计划交货期交货"]
[14,6600300046,"全电子式电动执行器","LSDZ-2000","电源220VAC输出4-20mA 反馈4-20mA 动作时间50S 转角90度 输出力矩2000N.m","JB/T8219-1999","台",1,"各二级厂","按合同计划交货期交货"]
[15,6400600201,"压力继电器","EDS345-1-250+ZBM300","精度等级正负0.5% 过载压力400Bar 测量范围0-250Bar 测量介质温度-25℃ - +80℃ PNP晶体管输出 1路开关输出 耐振≤10g/0..500HZ 耐冲击≤50g/11ms","DIN16086-2006","只",4,"各二级厂","按合同计划交货期交货"]
[16,6400300121,"限位开关","FTSB4 0.066387.B 8.117729.C DP 15301261 德国IEC947","触头1NO+1NC","德国IEC947","只",1,"各二级厂","按合同计划交货期交货"]
[17,6400400149,"轴型PN绝对值型编码器","8.5868.12C2.C212","库伯勒 夹紧法兰，?58mm 轴10x20mm 电源10-30VDC 接口PROFINET IO  防护等级IP67","2002/95/EG","台",1,"各二级厂","按合同计划交货期交货"]
[18,5300300685,"车载台","GM3688 MOTORLA 军标MIL810C.D.E","军标MIL810C.D.E","军标MIL810C.D.E","台",10,"各二级厂","按合同计划交货期交货"]
[19,6600400045,"流量开关","DW182/A/C/C043/F/A/1/0/1","量程 1.2-10t/h.报警下限5t/h","JB/T 5493-1991","台",1,"各二级厂","按合同计划交货期交货"]
[20,6400100008,"热金属检测器","SHB10-B2D","一体型 金属外壳 高温型 光纤 供电电压24VDC PNP 常开点 接线端子 IP67","GB/T21706-200","台",17,"各二级厂","按合同计划交货期交货"]
[21,6400200067,"热探","HMD2-4ZC1","DC 24V:检测方式 漫反射：使用环境温度-20—70°","GB/T23110-2008","只",8,"各二级厂","按合同计划交货期交货"]
[22,6100400374,"行车切电阻接触器","SDM-1J0100","工作电源220/380VAC;额定电流100A;控制电压220/380VAC;2NO","GB8871-2001","台",1,"各二级厂","按合同计划交货期交货"]
[23,6400600419,"激光测距仪","OSM160-RPL40PN6L","电源16-30VDC/max200mA:测量范围0.2-40m:精度±2mm:重复精度0.3mm;测量输出时间2ms:分辨率可调整:profibus预设1mm,SSI预设0.1mm","IEC 60947-5-1","台",1,"各二级厂","按合同计划交货期交货"]
[24,4100400213,"耐热套管","直径35mm","30m/卷","FDA标准","卷",15,"各二级厂","按合同计划交货期交货"]
[25,6100400390,"行车切电阻无触点接触器","SEM-1J0200","工作电源220/380VAC;额定电流200A;控制电压220/380V;中文液晶显示","GB8871-2001","台",2,"各二级厂","按合同计划交货期交货"]
[26,6100100080,"数字式电动机保护测控装置","PDS-766 整组动作时间(包括出口继电器动作时间)电流速断保护：≤35ms 带时限保护动作时间与整定值的误差:?≤+20ms",null,"GB/T21705-2008","台",1,"各二级厂","按合同计划交货期交货"]
[27,4100800122,"感应控制器","HYCX-5/10A","一级动作角度：12，二级动作角度：30；极限角度：70；触点数量：2常开、2常闭；触点容量：380vAC；电流：10A；防护等级：ⅠP67；环境温度：-30一+70；相对湿度：不大于85%","GB/T13978-2008","套",10,"各二级厂","按合同计划交货期交货"]
[28,5714100033,"气体弹簧","90.10.00500.160 PED","进口件 进口件，90.10.00500.160","PED","只",100,"各二级厂","按合同计划交货期交货"]
[29,5702200032,"线性导轨滑座","SRG65LV5QZZZC0","SRG65LV5QZZZC0;末端密封垫片;带油嘴。","THK","件",26,"各二级厂","按合同计划交货期交货"]
[30,7501300081,"波纹补偿器","自由高度705mm，法兰内径770，外径980,螺孔数量24个，螺孔直径26mm（改）","内侧采用耐磨堆焊工艺，堆焊层厚度12mm","审核图纸","只",1,"各二级厂","按合同计划交货期交货"]
[31,5712300077,"混合煤气直焰烧嘴芯嘴","LBT1500Kw","586m3/h 嘴前压力4KPa 煤气管外径108mm","GB/T3098.6-2000","只",10,"各二级厂","按合同计划交货期交货"]
[32,5500300105,"铁水取样器","SAF12/TC900-JN","试样尺寸：35*12mm，饱满，表面平整，无毛刺，无缩孔，测成率：96%，纸管长度：900mm","Q/C005-2016","只",2000,"各二级厂","按合同计划交货期交货"]
[33,5712300074,"混合煤气直焰烧嘴芯","SBT260Kw","112m3/h 嘴前压力3.5KPa","GB/T3098.6-2000","只",8,"各二级厂","按合同计划交货期交货"]
[34,5712300075,"混合煤气直焰烧嘴芯","SBT780Kw","335m3/h 嘴前压力3.5KPa","GB/T3098.6-2000","只",8,"各二级厂","按合同计划交货期交货"]
[35,5712300076,"混合煤气直焰烧嘴芯嘴","LBT1000Kw","405m3/h 嘴前压力4KPa 煤气管外径108mm","GB/T3098.6-2000","只",10,"各二级厂","按合同计划交货期交货"]
[36,6400600030,"测温枪前节","KZ-888CQN-604","1.2米 与测温枪配套使用","Q/CYKHL0003-2012","只",20,"各二级厂","按合同计划交货期交货"]
[37,6400600181,"无线测温枪","KZ-888CQN-604-SH","整长4.5米 前节1.2米 配线测温枪机芯 S分度号，测温范围：600-1769℃ 通信范围70m","Q/CYKHL0003-2012","把",12,"各二级厂","按合同计划交货期交货"]
[38,6600100086,"无线测温枪 机芯","KZ-888CQN2","S分度号","Q/CYKHL0003-2012","支",37,"各二级厂","按合同计划交货期交货"]
[39,7500300001,"板式换热器","BR02-20 散热面积20㎡","20㎡，1MPa","JB/T4715-1992","台",3,"各二级厂","按合同计划交货期交货"]
[40,7500300003,"板式换热器","YBRM0.23 冷却面积15m3 工作压力1.6MPa",null,"JB/T4715-1992","台",5,"各二级厂","按合同计划交货期交货"]
[41,7500300004,"板式冷却器","BR30 冷却面积30平方米",null,"JB/T4715-1992","台",16,"各二级厂","按合同计划交货期交货"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2024年7月至2025年6月机电备件年度采购项目                    \n项目编号：HG JY-G2024079"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}