{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":46,"n_cols":12,"rows_kept":46,"merged":[[0,0,0,11],[1,0,1,11],[42,0,42,8],[43,0,43,8],[44,0,44,8],[45,0,45,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2024年6月电气备件采购项目                  项目编号：HG JY-G2024080"]
["序号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家"]
[1,6100500432,"电磁吸盘电压检测板","FV1-FV2","输入电压DC170V-260V","IEC97-1991","套",1,"物流中心","2024-08-27"]
[2,4100700196,"晶闸管","MTC110A/2200V","额定电流110A;耐压2200V","GB/T17761-2018","个",5,"89管加工热处理","2024-08-27"]
[3,6300500286,"无触点继电器","YHP-WKG04","正逻辑输入，输入电压10-30VDC，正逻辑输出，输出电源电压20-30VDC，输出电流4A,带短路保护功能，双通道","JB/T2785-2010","只",30,"89管加工热处理","2024-08-27"]
[4,6200200959,"变频器","VFD037E43A","INPUT:3PH 380-480V 50/60Hz;11.2A;OUTPUT:3PH00480V;8.5A;6.8KVA;3.7Kw","GB/T12668.2-2002","台",2,"219厂部","2024-08-27"]
[5,6600300196,"阀门回讯器","TXP-M20GNPM","2xSPDT无源干接点;触点容量10A;250VAC;隔爆型Ex d II C T4;IP67防护等级","GB/T12237","个",6,"炼钢厂部","2024-08-27"]
[6,4000300030,"接线端子盒","NO:01.10 16 08;带10节菲尼克斯端子和DN15电缆缩紧头2个)","100*160*80mm","GB/T30402-2013","只",10,"炼钢厂部","2024-08-27"]
[7,6100100251,"故障录波装置","SH-DFR-G","1．采样指标　采样频率 最大 10KHz（9.6KHz）　谐波分辨率 最大 99 次，谐波误差＜ 5%　采样精度 25℃时，额定值下，电流误差＜ 0.2%　25℃时，额定值下，电压误差＜ 0.1%　开关事件分辨率 0.1ms A/D 分辨率 16 位","\"GB/T 22386\t\"","台",1,"能源厂部","2024-08-27"]
[8,6100400407,"行车用（一体化无触点）正反转装置","TDE-300A-3PJ-2N","电源AC380V；无触点通断；正反转延时保护，缺相、过流保护；智能风扇散热，电流实时显示。","GB14048.4-2003","只",1,"炼钢厂部","2024-08-27"]
[9,6600200826,"电动执行器","E110","执行器旋转90°用时12s;扭矩400Nm;额定电流1.0A;启动电流1.8A;功率0.2275Kw;额定电压380VAC;频率50Hz;工作循环等级C;防护等级IP67","JB/T10391-2002","台",2,"炼钢厂部","2024-08-27"]
[10,6100900167,"专用电器箱","HTOW380-15N","最大控制电流35A;额定电压380V;频率50Hz","GB14048.4-2003","台",1,"炼钢厂部","2024-08-27"]
[11,6100900168,"控制专用电器箱","WBQL-380/25/50","最大控制电流60A;额定电压380V;频率50Hz","GB14048.4-2003","台",1,"炼钢厂部","2024-08-27"]
[12,6100100249,"电动机保护器","I3DM-WRDUHZ","控制电压Ue100-240VAC/DC;50/60Hz;Uimp4KV;Aux.contact;OL(1NC+1NO);AL（1NO）;UL:Ie 0.5-60A/CCC;Ie 0.5-80A","德国IEC947","只",2,"炼钢厂部","2024-08-27"]
[13,6300500280,"不间断电源","3C10KS(6G)","容量10KVA/9Kw;电池输入192VDC;旁路输入220VAC;50Hz;63A;输出220VAC;50Hz;5.5A","GB/T9813-2000","台",1,"炼钢厂部","2024-08-27"]
[14,6100100246,"三相输出电抗器","LP-ACR40020V-0120F-550","额定电流120A;额定电感0.055mH;绝缘等级F级","GB/T1094.6-2011","台",2,"炼钢厂部","2024-08-27"]
[15,6100100247,"三相输出电抗器","LP-ACR40020V-0090F-151","额定电流90A;额定电感0.15mH;绝缘等级F级","GB/T1094.6-2011","台",4,"炼钢厂部","2024-08-27"]
[16,6100100248,"三相输出电抗器","LP-ACR40020V-0220F-320","额定电流220A;额定电感0.032mH;绝缘等级F级","GB/T1094.6-2011","台",2,"炼钢厂部","2024-08-27"]
[17,6100100236,"进线电抗器","DRLE-SL01-3.5","额定电流3.5A;电压降5.77V;频率50/60Hz","GB/T1094.6-2011","台",2,"炼钢厂部","2024-08-27"]
[18,6100100237,"出线电抗器","SDK-80A","工作电压400V;额定电流80A;绝缘等级F级;防护等级IP00;耐压3000V;工作频率50Hz","GB/T1094.6-2011","台",2,"炼钢厂部","2024-08-27"]
[19,4100400300,"重载连接器套装","HDC-HE-016-2","16芯;顶出开孔;套装","GB/T26846-2011","套",10,"炼钢厂部","2024-08-27"]
[20,4100400301,"重载连接器套装","HDC-HE-010-2","10芯;顶出开孔;套装","GB/T26846-2011","套",10,"炼钢厂部","2024-08-27"]
[21,4100400302,"重载连接器套装","HDC-HE-006-2","6芯;顶出开孔;套装","GB/T26846-2011","套",20,"炼钢厂部","2024-08-27"]
[22,6100600309,"熔断器","RS30C 100A","Ar100a;690V-50kA","GB/T13539.4","只",10,"炼钢厂部","2024-08-27"]
[23,6100600310,"熔断器","RS30C 63A","Ar63a;690V-50kA","GB/T13539.4","只",10,"炼钢厂部","2024-08-27"]
[24,6100300331,"万能式断路器","CW3-4000M","Cat.B;额定绝缘电压Ui=1250V;额定冲击耐受电压12KV;Icu85KA,Ics85KA;Icw 1s 85KA,分励脱扣器电压AC230V;电操机构AC230V;合闸电磁铁电压AC230V;智能控制器电压AC230V;额定电流4000A","GB/T14048.2","台",1,"炼钢厂部","2024-08-27"]
[25,6400600589,"压力传感器","S-20","螺纹类型G1/4A;信号输出类型4～20mA;量程0～40Mpa;精度0.5％;ED密封;带M12X1圆形接头","IEC601071-2007","只",4,"炼钢厂部","2024-08-27"]
[26,4100500407,"万能转换开关","LW39-16A","Ui690V;Ith16A","GB/T14048.5","个",30,"炼钢厂部","2024-08-27"]
[27,6200200973,"步进驱动器","HN-GZ-01","输入电压80-265VAC;输出电流0.4-8.0amps;步进信号频率2-2MHz;欠压保护80VAC;过压保护295VAC;输入电压信号4.0-28V","GB/T17215.2-2009","台",3,"炼钢厂部","2024-08-27"]
[28,6400500947,"PWM信号转换器","HN-PMW01","电源DC24V;输出1-10KHz;输入4-20mA55","GB/T43061-2023","台",3,"炼钢厂部","2024-08-27"]
[29,4100500406,"可编程计时器","TM5645E-1J-W","计时范围10ms-999H59m;工作电压DC5V或DC7-30V;显示方式;5位红色LED显示","GB22773-2008","个",6,"炼钢厂部","2024-08-27"]
[30,6400400183,"旋变编码器","J63XFW975","极对数：1;励磁电压7.0V;励磁频率：10KHz；变压比0.5±0.05；电气误差≤±10Max;相位移≤±25度；绝缘电阻：250MΩ；最大转速：8000rpm;工作温度范围：-30℃~+95℃；厂家：上海赢双电机科技股份有限公司","EN 60947-5-2","个",1,"340热轧","2024-08-27"]
[31,6200200987,"逆变器","DPD395T43A-00","重载200kw，额定输出电流395A，直流540v输入，内置预充电回路，输出频率0-599HZ，带DP通讯卡CMC-PD01","IEC/EN60068-2-27","台",3,"720厂部","2024-08-27"]
[32,6100500433,"电流继电器","DL-33；6A","动作电流1.5~3A","GB/T22387-2008","个",6,"能源厂部","2024-08-27"]
[33,6100500063,"时间继电器","ST3P A-F","AC220V 时间范围2小时","GB 10963.1","只",10,"89管加工热处理","2024-08-27"]
[34,6100600060,"熔断器","RT14,6A,直径10.3mm长38mm",null,"JB3368-83","只",5,"能源厂部","2024-08-27"]
[35,6100900078,"动力箱（壳体）","6.14.100.4；尺寸：宽350*深260*高280；","采用2mm钢板制作；下进线(下方开孔）；配接地柱；表面刷漆，冰灰GY09","图纸审核","个",10,"炼钢厂部","2024-08-27"]
[36,6100900005,"不修钢辊道开关箱","530*500*400 非标","非标 不锈钢制作",null,"台",10,"炼钢厂部","2024-08-27"]
[37,6100100062,"控制变压器","BK-150VA","输入 380V 220V输出 36V 75VA 27V 75VA JB/T 5553-2006","JB/T 5553-2006","台",2,"340热轧","2024-08-27"]
[38,6100100097,"整流控制柜变压器","ZSG-30KVA/170+190","GB/T18494.1-2001 30KVA 输入380V 输出170+190V","JB4315-1986","台",1,"340热轧","2024-08-27"]
[39,6100700025,"电流互感器","CP62/20.80/0.1A","CLASS:1.0  2.5VA; 50/60HZ; 0.72/3KW",null,"只",5,"180热轧","2024-08-27"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2024年6月电气备件采购项目         项目编号：HG JY-G2024080"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]