{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":29,"n_cols":14,"rows_kept":29,"merged":[[0,0,0,12],[1,0,1,12],[25,0,25,9],[26,0,26,9],[27,0,27,9],[28,0,28,9]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2024年8月电气备件采购项目                  项目编号：HG JY-G2024111"]
["序号","子项号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,"A2247000440050",4000200381,"拉绳跑偏开关","HFKPT1-12-30","防护等级IP65;极限角度30度;动作角度12度;触点数量2常开2常闭;触点容量380VAC;2.6A","GB/T14048.5-2017","个",2,"炼钢厂部","2024-09-26"]
[2,"A2247000650002",6100100254,"变压器风机","DBF-8.5Q8  1.5KW","720r/min，风叶直径850mm；（电机底座尺寸安装孔距140*190mm）","JB/T9008.1-2004","台",1,"能源厂部","2024-09-26"]
[3,"A2247000490028",6100900083,"BCM数字式吸盘控制装置","BCM 140A 220BS","140A  220V","GB/T3235-1999","台",2,"炼钢厂部","2024-09-26"]
[4,"A2247000750106",6100900183,"行车大小车防尘控制柜","YEKG-QRY/100D2+30X1","1600*1200*450(H8*W*D)","审核图纸","台",1,"720厂部","2024-09-26"]
[5,"A2247000490050",6100900186,"遥控控制柜","控制柜尺寸1350*700*350","行车加装AUTEC无线遥控器;要求配套遥控器AUTEC;接收机电源AC~220V;双遥杆式四方位四挡操作手柄(左手柄大、小车，右手柄主、副钩);带急停、起动、电锁、声光报警器、大梁照明灯等按钮;操作手柄要有零位保护;遥控器控制输出中间继电器采用施耐德RXM4AB2P7","GB3797-1983","台",3,"炼钢厂部","2024-09-26"]
[6,"A1247000510045",6300400097,"稳压电源","S-350-36","输入电压110/220V,输出电压DC36V，输出电流9.7A,功率350W,尺寸：215*215*50mm","GB/T 15184-1994","只",2,"89管加工热处理","2024-09-26"]
[7,"A2247000490036",6300600090,"智能转子控制器","SEM-1J0150","SN1;1JE1521007A;工作电源165-440VAC;控制电压220/380VAC;主回路电压500VAC;主回路额定电流150A","QYQJ0301004-2019","台",2,"炼钢厂部","2024-09-26"]
[8,"A2247000440054",6400500965,"火焰检测探头","C7027A1049","环境温度-18℃-102℃;最大耐压5ps(34.5kPa);电路连接2根2.44米长耐热温度105℃的NEC CLSAA1导线","GB12791-2006","只",3,"炼钢厂部","2024-09-26"]
[9,"A2247000440038",6400600583,"激光检测器","LOS-T4-4ZC1","AC220V;PNP常开;检测距离0~50m;（光纤10m、10m）;（成对使用）","Q/3204BCK010-2013","台",1,"炼钢厂部","2024-09-26"]
[10,"A2247000440039",6400600585,"位移传感器","BTL7-E501-M0600-PB-S32","量程600mm;电源24VDC;输出4-20mA;测量起始端以外保持4mA输出;超出测量末端保持20mA输出;插头BKS-S32M-15;带磁环","德国IEC947","台",2,"炼钢厂部","2024-09-26"]
[11,"A1247000540016",6400600623,"激光测距传感器开关安装角撑架","E21120","适合O1D100-O1DLF3KG传感器安装万向调节角撑架，并附带两套螺丝。","IEC 61131-2","个",15,"219厂部","2024-09-26"]
[12,"A1246000360139",6100900173,"辊道开关箱","600*500*200","304不锈钢箱体，板厚不小于1.5mm,配GV2ME14C 6-10A电动机断路器20只","审核图纸","只",4,"219厂部","2024-09-26"]
[13,"A2246000820038",6100900173,"辊道开关箱","600*500*200","304不锈钢箱体，板厚不小于1.5mm,配GV2ME14C 6-10A电动机断路器20只","审核图纸","只",4,"340热轧","2024-09-26"]
[14,"A1245000450031",6400600183,"限位开关","LX44-20 AC380V 20A","GB/T14048,电动葫芦限位开关","GB/T14048","只",5,"89管加工热处理","2024-09-26"]
[15,"A1246000360114",6200200864,"变频器","MD480T280P","负载类型，风机泵类；交流输入电压380V;标准应用输出功率280kw，输出电流520A;重载输出功率250kw，输出电流465A",null,"台",1,"219厂部","2024-09-26"]
[16,"A2245000440062",4000100154,"指示灯","AD16-22B","220VDC （红）","EN60947-511EC337","只",20,"炼钢厂部","2024-09-26"]
[17,"A2246000820037",6100900160,"变频控制柜","柜体尺寸：宽*深*高为800mm*600mm*2150mm;","风机水泵负荷；每台变频器柜为2台功率为75Kw风机水泵提供动力；具体配置：2套进线电源开关；带配套进出线电抗器；2套变频器型号为：MD480T55G-PLUS（品牌为汇川）；变频器与AB公司Logix5000PLC通过EIP通讯卡进行通讯（型号：MD500-EN1）；供货方负责变频控制柜及与PLC的现场通讯调试","GB/T12668.2-1989","套",1,"340热轧","2024-09-26"]
[18,"A1246000310003",6400600612,"栏杆机红外对射","DS436i-chi,","工作电压：12V，警戒距离60米，射束距离650米。","GB/T27664.2-2010","对",2,"物流中心","2024-09-26"]
[19,"A2244000310046",6600300196,"阀门回讯器","TXP-M20GNPM","2xSPDT无源干接点;触点容量10A;250VAC;隔爆型Ex d II C T4;IP67防护等级","GB/T12237","个",6,"炼钢厂部","2024-09-26"]
[20,null,6100900189,"变频器成套控制柜","BSC-280/380","柜体尺寸：800（宽）*800（深）*2200（高）；内附：变频器IPE300-0280-4；制动单元DBU100H-320-4；中文面板安装套件IPE300-LCD；DP 总线卡EC-TX503D；断路器CVS600F /600A；接触器CJ20-630J/220V/630A；输入电抗器GDL-ACL0580-4AL 580A；输出电抗器GDL-OCL0660-4AL 660A；铜排60*6","EN61000-6-2","套",1,"180厂部","2024-09-26"]
[21,null,6200200993,"变频器","MD480T55G-PLUS","重载应用，输入电压：380V，输入电流106A，输出电流112A，输出功率55KW","EN IEC 61800-3","台",1,"180厂部","2024-09-26"]
[22,"A2247000440036",6000200465,"真空断路器","3AH4305-4 Ur=36KV/Isc=31.5KA/Ir=2000A/屏柜NX-40.5 带小车 德国IEC947","德国IEC947","德国IEC947","台",1,"炼钢厂部","2024-10-11"]
["注：1、投标报价含税，税率13%                                                                                     \n2、生产厂家要求全称填写准确无误\n3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2024年8月电气备件采购项目     项目编号：HG JY-G2024111"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]