{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Macro1","附件表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"附件表","index":1,"n_rows":42,"n_cols":9,"rows_kept":42,"merged":[[0,0,0,8],[41,0,41,8]],"flags":["formulas_cached_only"]}
["附件1    "]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","交货时间","使用部门"]
[1,"7200400015","G4225带锯床；锯架升降油缸","锯架升降油缸","耐压16MPa；无故障工作循环次数65万次；带性能可靠磁性开关","台","2","2021-10-30","管加工厂部"]
[2,"7200600086","液压缸","CDH1MP5/160/110-650A1X/D1CSEMWW+CGAS80","缸径Φ160,杆径Φ110,行程650 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台","1","2021-10-30","340热轧"]
[3,"7200100329","新开口机挂钩油缸","YYZ3030.02.03","φ125/φ90-98.5，工作压力16MPa","台","1","2021-10-30","高炉"]
[4,"7200100330","新开口机回转油缸","YYZ3030.01.07","φ140/φ100-474,油缸前后两腔带节流缓冲，工作压力25MPa","台","1","2021-10-30","高炉"]
[5,"7200100331","新开口机夹钳油缸","YZG5050.04.01.03.02","φ50/φ28-140，工作压力16MPa","台","1","2021-10-30","高炉"]
[6,"7200600039","冷床横移液压缸","180-125-280","缸径Φ180,杆径Φ125,行程280 带缓冲 伸缩防护套耐温150度 工作环境温度-20℃~100℃ 工作压力15MPa,试验压力25MPa 活塞及活塞杆采用V型组合耐高温密封 工作介质聚酯抗燃液压油","台","2","2021-10-30","炼钢厂部"]
[7,"7200100040","液压缸","CD250B125/90-255A10/02CADMA","缸径Φ125,杆径Φ90,行程255 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台","2","2021-10-30","炼钢厂部"]
[8,"7502000060","液压缸耳环","GAS60",null,"件","2","2021-10-30","炼钢厂部"]
[9,"7200400071","摆动液压缸","80/78-422.806,422度",null,"台","1","2021-10-30","管加工厂部"]
[10,"7200100335","液压缸","CD250B100/70-105A10/02CGDMA；","缸径Φ100,杆径Φ70,行程105 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台","1","2021-10-30","管加工厂部"]
[11,"7200400069","液压缸","100/56-250","17MPa;带连接耳环;带MTS传感器","台","1","2021-10-30","管加工厂部"]
[12,"7200600202","液压缸","CDH1/MP3/50/28/250A1X+GAS30 带耳环;","带耳环;缸径Φ50,杆径Φ28,行程250 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台","3","2021-10-30","管加工厂部"]
[13,"7200100189","液压缸","CD250E125/90-250A10/02CADMA",null,"台","1","2021-10-30","管加工厂部"]
[14,"7200100218","液压缸","CDH2MT4/80/50-400A1X/B1CFDMWV,XV=480","缸径Φ80,杆径Φ50,行程400 ,工作压力25MPa","台","2","2021-10-30","管加工厂部"]
[15,"7200100206","液压缸","CD250E100/56-340A10/01CADMA;","L10=405，压力21MPa","个","2","2021-10-30","管加工厂部"]
[16,"7200400076","液压缸","CD250E125/70-340A10/01CADMA370",null,"台","2","2021-10-30","管加工厂部"]
[17,"7200100322","液压缸","CD250E100/56-460A10/01CADMA；","L10=440；带耳环；JB2162-1991","台","2","2021-10-30","管加工厂部"]
[18,"7200400024","液压缸","YG63/28-25",null,"台","2","2021-10-30","管加工厂部"]
[19,"7201300018","液压缸活塞杆","H250-01","2Cr13调质","件","4","2021-10-30","340热轧"]
[20,"7200100023","液压缸","CD250B/140/100-340A10/01CGDMA+GAK65",null,"台","1","2021-10-30","720厂部"]
[21,"7200100005","液压缸","268.27SB030105-78 CD250B160/100-360ADMLR+GAS80",null,"台","1","2021-10-30","720厂部"]
[22,"7200100030","液压缸","CD250B100/70-160A10/02CGDMA+GAK45","缸径Φ100,杆径Φ70,行程160 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台","1","2021-10-30","340热轧"]
[23,"7200100126","液压缸","CD250F63/36-485A10/02CADMA","缸径Φ63,杆径Φ36,行程485 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台","2","2021-10-30","340热轧"]
[24,"7200100309","液压缸;","CDH1MP5/100/56-90A1X/D1CSEMWW;带耳环CGAS50","缸径Φ100,杆径Φ56,行程90 工作环境温度-20℃~70℃ 工作压力16MPa,试验压力20MPa 活塞及活塞杆采用V型组合密封","台","2","2021-10-30","340热轧"]
[25,"7200600088","液压缸","CG250F63/36-485A10/02CADMA","缸径Φ63,杆径Φ36,行程485 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台","2","2021-10-30","340热轧"]
[26,"7201300019","液压缸活塞","H250-10 MERJER之P6,HUNGER之AI","2Cr13","件","4","2021-10-30","340热轧"]
[27,"7200400009","液压缸","WG01CD250B63/45-225A10/01.1CADMA","额定压力25MPa JB/T 5000","台","2","2021-10-30","180厂部"]
[28,"7502000060","液压缸耳环","GAS60",null,"件","10","2021-10-30","180厂部"]
[29,"7200400098","翻车机新压车液压缸","GGK1-φ125/φ70-2531-420-1360","密封确保12个月以上无内外泄漏；缸底、缸头带节流缓冲。油缸耳环关节轴承要求SKF品牌，且带锁紧装置；活塞杆顶端外丝M64*2.0-100","台","2","2021-10-30","原料工段"]
[30,"7200500079","液压缸","KZ2102.01.01.02","规格125/90-240;带关节轴承GE80ES；耐压250bar;活塞杆与耳环整体锻造","台","4","2021-10-30","180厂部"]
[31,"7200100370","液压缸","CD250A80/56-100A10/02CADMA","缸径80；杆径56；行程100；耐压等级25MPA；连接螺栓12.9级","台","1","2021-10-30","180厂部"]
[32,"7200500078","液压缸","KZ2102.01.01.01","规格125/90-135;不带位移传感器；需留有位移传感器接口；带磁环；带关节轴承；耐压等级250bar；耳环与活塞杆整体锻造","台","4","2021-10-30","180厂部"]
[33,"7200100369","液压缸","CD250F125/90-250A10/02CADMA","缸径125；杆径90；行程250；耐压等级25MPA；连接螺栓12.9级","台","1","2021-10-30","180厂部"]
[34,"7200100371","液压缸","CD250E100/56-120A10/02CADMAL10=230","缸径100；杆径56；行程120；耐压等级250bar；不带位移传感器；留位移传感器接口；需带磁环；带耳环","台","2","2021-10-30","180厂部"]
[35,"7200600162","液压缸","HYZ02345","直径90/80-130","台","2","2021-10-30","89热轧"]
[36,"7200600209","液压缸(三)","02680014DR5005ME013-35","20Kg；其它参数见图纸上的技术要求","件","4","2021-10-30","89热轧"]
[37,"7200100288","液压缸","02680014DR5005ME035-54","CD250B63/45-380A10/01CADMA","台","2","2021-10-30","89热轧"]
[38,"7200200087","液压缸","HY89G43-680C；100/45-680","缸径100mm,杆径45mm,行程680mm,额定压力20Mpa","台","2","2021-10-30","89热轧"]
[39,"7200100267","液压缸","CD250E63/36-380A10/02CADMA+GAS35 L10=350","缸径Φ63,杆径Φ36,行程380 ,工作压力25MPa 活塞及活塞杆采用V型组合密封，带球铰耳环","台","1","2021-10-30","89油管车丝委外"]
["注：1、投标报价含税，税率13% ；                                                                                                 2、生产厂家要求全称填写准确无误 ；                                                                                          3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]