{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Macro1","附 件清单"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"附 件清单","index":1,"n_rows":50,"n_cols":10,"rows_kept":50,"merged":[[0,0,0,9]],"flags":["formulas_cached_only"]}
["附 件"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","交货时间","使用部门","备注   "]
[1,"6000400011","探伤机 磁化线圈","CXT-20001AT 管端纵向",null,"只","1","2021-10-30","管加工厂部"]
[2,"6400500234","超声波探伤仪","HS600","HS600附合格证 附性能测试报告","台","1","2021-10-30","720厂部"]
[3,"6400500803","探伤机；减速机","型号：V 065 2:1 JO-5+6.1+2-500/0000","厂家：ATEK","台","1","2021-10-30","180厂部"]
[4,"6400600142","双激光红外测温仪","TN435","测温范围: -60~1500℃","台","8","2021-10-30","炼钢厂部"]
[5,"6400600331","红外测温仪","ST21-SI","300-1300℃;4-20MA输出;带水;气冷却及护罩","台","1","2021-10-30","管加工厂部"]
[6,"6400600367","探伤机;漏磁探头","JJTZ-16T   3358310010  SHOE ASSY，AMALOG 16CH MILL","长度200mm, 两端带耐磨钉，16个通道","只","1","2021-10-30","管加工厂部"]
[7,"6400600371","差压变送器","EJA110E-DMS5J-712NN/NF2/K1","0-40KPa","台","2","2021-10-30","炼钢厂部"]
[8,"6500300073","电信级光纤跳线","SC-FC","多模；双芯；陶瓷插芯；长度3米","根","6","2021-10-30","720厂部"]
[9,"6500300089","华为交换机","S1700-24GR","442*220*43.6  功耗 14.2W  包转发率 36Mpps   交换容量 48Gbps  固定端口 24个10 /100/1000Base-T","台","2","2021-10-30","保卫处"]
[10,"6500400190","拼接屏","TC-P4664","46寸三星面板，额定电源：100-240VAC，50/60Hz，2A，亮度值500cd/m2，拼缝3.5mm，最大分辨率1920*1080，功耗200W.","台","1","2021-10-30","物流中心"]
[11,"6500400191","网络硬盘录像机","DS-7816NB-K2","电源:12V 序列号:D91682229","台","2","2021-09-30","炼钢厂部"]
[12,"6500400192","海康威视硬盘录像机","DS-8832N-R8  445*470*90mm    重量8kg","接入数  32  输入带宽  256M   输出带宽 160M  录像分辨率  8MP/7MP/6MP/1080P/720P/VGA/4CIF/DCIF/2CIF   VGA 输出 与HDMI异源  1920*1080/60Hz   1600*1200/ 60Hz 同步回放 16  视频解码 H265，Smart265 硬盘管理 8*8T SATA 预览分屏1-36网络接口 2*RJ45","台","1","2021-09-30","保卫处"]
[13,"6500400193","海康威视云台型摄像机","DS-2CD3646F(D)WD-IPZS  400W 221*213*105  1150克","主码流 H264/H265  最大画面尺寸 2560*1440  传感器  1/2.7\"  动态范围  120DB  防护等级  IP 67  接口协议  ONVIF,ISAPI,GB28181 支持协议 TCP/IP ICMP  HTTP  FTP DNS DDNS  通讯接口 1个RJ4510M/100M","台",3,"2021-09-30","保卫处、89热轧"]
[14,"6500400194","海康威视全彩枪形摄像机","DS-2CD3T47E(D)WD-L  400W像素  1/ 1.8\"大靶面传感器  186.6*93.5*92.9MM","主码流 H264/H265  最大画面尺寸 2560*1440  传感器  1/1.8\"  动态范围  120DB  防护等级  IP 67  接口协议  ONVIF,ISAPI,GB28181 支持协议 TCP/IP ICMP  HTTP  FTP DNS DDNS  通讯接口 1个RJ4510M/100M","台","1","2021-09-30","保卫处"]
[15,"6500400195","海康威视枪形摄像机（普通型）","DS-2CD3T56DWD-I5  500W像素  93.9*93.5*194.1  850克","主码流 H264/H265  最大画面尺寸 2560*1920  传感器  1/2.7\"  动态范围  120DB  防护等级  IP 67  接口协议  ONVIF,ISAPI,GB28181 支持协议 TCP/IP ICMP  HTTP  FTP DNS DDNS  通讯接口 1个RJ4510M/100M","台","10","2021-09-30","保卫处"]
[16,"6500400196","热成像防爆筒型摄像机","DS-2TD26ZYL-H/Y","热成像:分辨率384x288;焦距10mm;视场角:36\"x27;可见光:分辨率:2688*1520;焦距:4mm;红外照射距离:30米;人员最远报警距离(以18米*0.5米为准):100m;火点最远报警距离(以0.1米*0.1米为准):50m;吸烟检测最远报警距离:15m;温度异常报警功能，测温精度:±8C或量程的±8%℃(取量大值）;测温范围:-20C~150C;帧率:50Hz50fps(可见光)50Hz50fps(384x288)(热成像);电源:AC24V/DC12V/POE;功率:MAX9.5W;工作温度和湿度：-40℃-400℃，湿度小于90%;机芯品牌：海康威视","台","1","2021-09-30","340热轧"]
[17,"6600100236","三角规","Micrometer Screw for 3 Point Inside Measure;","测量范围:140-240mm","套","1","2021-11-30","180厂部"]
[18,"6600100386","电子位置变送器","ELECTRONIC POSITION TRANSMITTER  TYPE 4211","OUTPUT 4-20mADC AMB TEMP -40℃-70℃ MAX VOLTAGE 30VDC ENCLOSURE IP66（FISHER Emerson ）","台","1","2021-10-30","高炉"]
[19,"6600100405","智能涡轮流量计","LWQ-50Z-G100+EVC300-1.0-1.6/0.5","介质：天然气，10--160m3/h，防爆","台","4","2021-10-30","720厂部"]
[20,"6600200008","称重数据传送器","YH3128SA-1",null,"只","2","2021-10-30","炼钢厂部"]
[21,"6600200011","称重显示器","YH3128S(W)","0-100t","台","2","2021-10-30","炼钢厂部"]
[22,"6600200012","称重显示器(发)","YH3128WBH",null,"台","1","2021-10-30","炼钢厂部"]
[23,"6600200013","称重显示器(收)","YH3128W",null,"台","1","2021-10-30","炼钢厂部"]
[24,"6600200020","高温称重传感器","CZL-YH-8805-50T","50T 带高温称重电缆和接头","只","2","2021-10-30","炼钢厂部"]
[25,"6600200021","高温称重传感器","CZL-YH-8815-100T","100T 带电缆和接头","只","2","2021-10-30","炼钢厂部"]
[26,"6600200036","电子秤","Z6FD1","100Kg","台","2","2021-10-30","烧结"]
[27,"6600200243","SAT专用双芯铂铑铂工作热电偶","SAT-S2-4-25/8-1300-Ⅱ","1650/1500mm φ25刚玉套管 固定法兰 SAT孔径φ8 刚玉管绝缘 丝径φ0.5±0.015mm 二级精度 测温范围0-1300℃ 工作温度800-1100℃ 24个月内温度不超±0.75%","支","2","2021-10-30","89热轧"]
[28,"6600200322","电磁流量计","IFM4080K(40)11441122310","0-12m3/h IP67 DN40 PN16Bar","台","3","2021-10-30","炼钢厂部","KROHNE（科隆）、金湖苏能"]
[29,"6600200679","数字式高精度称重传感器","SLC820-50t","1、制造商: 梅特勒-托利（常州）精密仪器有限公司；2、结构:压式柱型,DWP,不锈钢材材料外壳，焊接密封；3、额定容量: 50T；4、蠕变(30分钟):±0.013%F.S；5、非线性:±0.010%F.S；6、滞后:±0.016%F.S；7、重复性：±0.005%F.S；8、防雷击能力（最大测试指标）： 80000A；9、IP防护等级： IP68/IP69K；10、使用温度范围 -40C~+55C；11、最大安全过载: 200%F.S","个","1","2021-09-30","物流中心"]
[30,"6600200680","PDX称重专用仪表","IND880 PDX高级版","1、显示器：5.7” LCD显示器, 320 x 240点阵带背光的TFT彩色显示器; 显示刷新率: 10 Hz；2、尺寸(h x w x d): 200 x 299 x 235 mm (台式)； 3、具有统一的Mettler Toledo图形菜单风格的设置界面；4、键盘：有触感的轻触隔膜按键，可以输入字母和数字。主要功能键: 清零, 去皮, 清除, 打印, 秤台切换；数字键: 0～9, 小数点；软键: 3组共15个可自定义软键（可输入英文字符）；应用功能键: 4个可编程功能键；5、外壳：不锈钢304L，符合EHEDG和NSF卫生标准；6、防护等级: IP69K，防水，防尘，可用高温高压水冲洗；7、","台","1","2021-09-30","物流中心"]
[31,"6600200691","称重显示控制器","IND880","全不锈钢外壳，抗干扰能力强； 6.5’’工业级高亮TFT彩色液晶显示屏；仪表支持触控与按键两种方式的操作； 支持梅特勒-托利多公司的各种模拟及数字式传感器","台","1","2021-09-30","物流中心"]
[32,"6600200699","高速高温激光测距仪","ZYT-405G","测量范围0.1-30m任何物体表面0.1-50mm选择物体表面;测量精度±1mm(+15℃...,+30℃);重复率≤±0.5mm;分辨率0.01mm SF100;测量频率10Hz;激光等级≤1mw安全等级2级;防护等级IP66;供电10-30VDC;外形尺寸255*90*110mm;测量物体最高温度1200度","个","1","2021-10-30","炼钢厂部"]
[33,"6600200709","智能涡轮流量计","JHBL-065N05SNBL","介质:软水;DN50;PN1.6MPa;工作电压24V;0-50m3/h;防护等级IP65;精度0.5级;HART协议","台","2","2021-10-30","炼钢厂部"]
[34,"6600200714","称重显示控制器","METTLER TOLEDO XK3141(IND331)","托利多；   产品编号：33P100000000001； 电源：AC100-240V/50-60Hz；有RS485通讯；规格：（0-6000）d；","台",3,"2021-10-30","180厂部、340热轧"]
[35,"6600200731","数码显示表","CMD4A","4 Bit BCD Input;DC24V/30mA","块","3","2021-10-30","炼钢厂部"]
[36,"6600200757","地下电缆寻线仪","NF-826","断点、短路故障检测。耐压400V，内置交直流电压表，USB锂电直充。","台","1","2021-10-30","检验检测中心"]
[37,"6600200764","示波器","DS1302CA;2通道\\带宽300MHz","普源RIGOL;64K色 TFT彩色液晶显示;实时采样率2 GSa/s（单通道）1 GSa/s（双通道）;存储深度：200Mpts","台","1","2021-10-30","219厂部"]
[38,"6600200765","分体型电磁流量计","RPmag62F-0600-21110","0-3000m3/h;DN600;PN10;-20mA;DC0.5%","台","1","2021-10-30","340热轧"]
[39,"6600200771","全隔离智能温度变送器","NHR-214","电压：12~40V DC，输出电流：4~20mA（dc）；热电偶：pt100，温度：0~200℃","个","5","2021-10-30","能源厂部"]
[40,"6600200772","智能压力变送器","T350","两线制；精度0.2级，输出4-20mA，量程0-1600KPa，电气接口：M20*1.5；防爆","台","1","2021-10-30","能源厂部"]
[41,"6600400085","其他自动化仪表","工业电视;高温数字摄像机配套录像机:JXJ-NVR16P",null,"台","4","2021-10-30","管加工厂部"]
[42,"6700400228","shaft+ballbearing assembly for cap","帕纳科Axios专用，备件号5322 784 00711","备件号5322 784 00711","套","1","2021-10-30","检验检测中心"]
[43,"6700400229","焦炭反应器盖子","HXFQ-6S-FYQGZ","反应器盖子为耐高温合金钢，材质为GH3044,热电偶管壁厚不小于1.5mm，拖料筛片直径78±1mm，其上均匀钻3mm圆孔，孔间距5mm，筛片厚度1.5mm","套",2,"2021-10-30","检验检测中心"]
[44,"6700400231","高温拉伸试验炉","SUST(GWLD-1200F）","高400mm，直径320mm的圆柱形；温度范围：200～1100℃；均热带长：180mm；炉膛尺寸：Φ120×350mm；温度波动度：≤600℃ ±2℃， 600～900℃  ±3℃， 900～1100℃   ±4℃；温度均匀度：≤600℃ ±2℃， 600～900℃  ±3℃， 900～1100℃   ±4℃；电炉丝采用铁铬铝电热合金丝（OCr27Al7Mo2），保温层采用含锆型硅酸铝纤维，保温层厚度达80mm，产品外壳采用厚度为3mm的304不锈钢。","台","1","2021-10-30","检验检测中心"]
[45,"6700400232","全自动金相镶嵌机","ixiang5","镶嵌方式： 全自动电动液压、自动制冷，设置好参数后全过程自动完成镶嵌。压力：至少包括1~20MPa(200kgf-4000kgf)可选,每次可选增减1MPa。加热温度：至少包括90℃~200℃，每次可选增减10℃。镶嵌时间：最快6分钟镶嵌1次。多重安全保护，温度过热会自动断电。镶嵌模具尺寸：30mm。","台","1","2021-10-30","检验检测中心"]
[46,"7000300044","探伤齿轮泵，国产化","XJC-20L-C63-NNNN0001","转速：3000转/分，输出压力：12MPa,输出流量：25ml/r","个","2","2021-10-30","管加工厂部"]
[47,"7502900151","流量计","S070","流量15－550LPM；通径50mm；最高压力1800Ka；最高温度80度；不带显示模块；burkert;","套","1","2021-11-30","180厂部"]
[48,"9800400017","多参数水质分析仪","XZ-0178",null,"台","1","2021-10-30","检验检测中心"]