{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Macro1","附件"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"附件","index":1,"n_rows":15,"n_cols":9,"rows_kept":15,"merged":[[0,0,0,8]],"flags":["formulas_cached_only"]}
["附件"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","交货时间","使用部门"]
[1,"5700700406","刀杆(卡刀体)","0107067-10.400.03：φ50-φ60","VALENITE-D-03.94；G42Z-A1-0416：DW50-60 42CrMo;6Kg","件","1","2021-09-30","89热轧"]
[2,"4201000242","双开肩铣床刀片","YBC301/LPEX1912-WR25","LPEX1912-WR25","片","20","2021-09-30","检验检测中心"]
[3,"6700100460","光谱标样","YSBS11388-04","Ti:0.544；∮35x35；带证书","块","1","2021-09-30","检验检测中心"]
[4,"6700100461","光谱标样","YSBS35152","弹簧钢60Si2Mn，B:0.017；带证书","块","1","2021-09-30","检验检测中心"]
[5,"6700100462","光谱标样","YSBS11091-2009","稀土镁铸铁 Sb:0.039；∮32x19mm；带证书","块","1","2021-09-30","检验检测中心"]
[6,"6700100463","光谱标样","YSBS35232c-2019","中低合金钢Ca：0.0031；Φ38x40mm；带证书","块","1","2021-09-30","检验检测中心"]
[7,"6700100464","光谱标样","YSBS451073-13","纯铁P:0.0037；39*35mm；带证书","块","1","2021-09-30","检验检测中心"]
[8,"6700100465","光谱标样","YSBS112102-2015","硅钢50W600.P:0.074,Ti：0.0007；Φ37x40mm；带证书","块","1","2021-09-30","检验检测中心"]
[9,"6700100466","光谱标样","YSBS35417-2020","模具钢：B：0.0003，C:0.575；φ38×40mm；带证书","块","1","2021-09-30","检验检测中心"]
[10,"6300500223","压线钳","订货号K97 51 10","工业以态网线专用压线钳 用于RJ45 RJ11插头压接","把","2","2021-09-30","炼钢厂部"]
[11,"6700400205","表面粗糙度比较样板","共32块，车，刨，平铣，端铣，镗0.8μm、1.6μm、3.2μm、6.4μm各一块。平磨，外磨0.1μm、0.2μm、0.4μm、0.8μm各一块。研磨0.012μm、0.0025μm、0.05μm、0.1μm。","要求准确度小于5%","块","1","2021-09-30","340热轧"]
[12,"7300500012","高温耐磨软密封装置","Dinfn-THCC/90*150","耐550°以上高温，耐磨，高硅复合材料，长度1米","套","2","2021-09-30","340热轧"]
[13,"7501300016","避震喉","KXT-III DN50，PN2.5","公称直径：DN50，压力等级：≤2.5Mp，长度：105mm","只","5","2021-09-30","炼钢厂部"]