{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["附件"],"read":"whole","date_system":"1900"}

{"sheet":"附件","index":0,"n_rows":79,"n_cols":11,"rows_kept":79}
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","备注"]
[1,7101700057,"不锈钢闸阀","Z45W-10P-200",null,"个",5,"GB/T3955-2004","炼钢厂部","2021-09-15"]
[2,7101600093,"涡轮传动法兰式手动蝶阀 D341X-10 DN300 工作压力≤1.0MPa","D341X-10 DN300 PN1.0","GB/T12221-2005,公称直径：DN300，压力等级：P≤1.0Mp，阀体长度：270mm","只",4,"GB/T12238-1989","炼钢厂部","2021-09-15"]
[3,7101800141,"液控快开快闭偏心半球阀","DYQ740H(X)-400-25","DN400 P=2.5MPa","只",1,"GB/T122202-1980","720厂部","2021-09-15"]
[4,7101600193,"电动调节型耐磨蝶阀","TD943SH-6C;DN2100","阀体材质：Q235，阀板材质16Mn，阀杆材质2Cr13，泄漏率：2%，电动执行器为智能一体化产品，工作电源：380VAC,50Hz，保护等级IP68，有限行程、限力矩机构；含安装螺栓及密封垫片","台",1,"GB/T12238-1989","高炉","2021-09-15"]
[5,6600300132,"气动单座调节阀","HZHY647Y-25C","介质:氧气;DN25/PN25;等百分比;阀体/阀芯材质:CF8;阀座材质:304 防护等级:IP65 泄漏等级:ANSI Class Ⅳ 带西门子阀门定位器:6DR5010-ONG-0AAO","台",1,"GB/T4213-2008","炼钢厂部","2021-09-15"]
[6,7101600195,"电动调节型耐磨蝶阀","TD943SH-6C;DN900","阀体材质：Q235，阀板材质16Mn，阀杆材质2Cr13，泄漏率：2%，电动执行器为智能一体化产品，工作电源：380VAC,50Hz，保护等级IP68，有限行程、限力矩机构；含安装螺栓及密封垫片","台",1,"GB/T12238-1989","高炉","2021-09-15"]
[7,7101600077,"手动控制阀门","S31","DN50 PN16 带手动蜗轮机构","只",3,"GB/T9001:2000","180厂部","2021-09-15"]
[8,6600300133,"气动单座调节阀","HZTRQ647Y-25C","介质:天然气 DN50 PN25 等百分比 阀体/阀芯材质:WCB 阀座材质:304 防护等级:IP65 泄漏等级:ANSI Class Ⅳ 带西门子阀门定位器:6DR5010-ONG-0AAO","台",1,"GB/T4213-2008","炼钢厂部","2021-09-15"]
[9,7101600196,"电动调节型耐磨蝶阀","TD943SH-6C;DN1500","阀体材质：Q235，阀板材质16Mn，阀杆材质2Cr13，泄漏率：2%，电动执行器为智能一体化产品，工作电源：380VAC,50Hz，保护等级IP68，有限行程、限力矩机构；含安装螺栓及密封垫片","台",1,"GB/T12238-1989","高炉","2021-09-15"]
[10,7101600070,"手动控制阀门","S31","DN100 PN16 带手柄","只",4,"GB/T9001:2000","180厂部","2021-09-15"]
[11,6600300007,"电动蝶阀","D943X-10ZB","工作压力 1.0MPa DN300，配现场操作箱","只",5,"DL/T1068-2007","炼钢厂部","2021-09-15"]
[12,7101600071,"手动控制阀门","S31","DN80 PN16 带手柄","只",5,"GB/T9001:2000","180厂部","2021-09-15"]
[13,7101600194,"电动调节型耐磨蝶阀","TD943SH-6C;DN1000","阀体材质：Q235，阀板材质16Mn，阀杆材质2Cr13，泄漏率：2%，电动执行器为智能一体化产品，工作电源：380VAC,50Hz，保护等级IP68，有限行程、限力矩机构；含安装螺栓及密封垫片","台",1,"GB/T12238-1989","高炉","2021-09-15"]
[14,6600300131,"气动单座调节阀","HZYQ647Y-25P","介质:氧气 DN50 PN25 等百分比 阀体/阀芯材质:CF8 阀座材质:304 防护等级:IP65 泄漏等级:ANSI Class Ⅳ 带西门子阀门定位器:6DR5010-ONG-0AAO","台",1,"GB/T4213-2008","炼钢厂部","2021-09-15"]
[15,7101600192,"电动调节型耐磨蝶阀","TD943SH-6C;DN2200","阀体材质：Q235，阀板材质16Mn，阀杆材质2Cr13，泄漏率：2%，电动执行器为智能一体化产品，工作电源：380VAC,50Hz，保护等级IP68，有限行程、限力矩机构；含安装螺栓及密封垫片","台",1,"GB/T12238-1989","高炉","2021-09-15"]
[16,7101800012,"不锈钢浮球阀","DN25",null,"只",4,"JB/T8764-1998","炼钢厂部","2021-09-15"]
[17,7101600073,"手动控制阀门","S31","DN65 PN16 带手柄","只",5,"GB/T9001:2000","180厂部","2021-09-15"]
[18,7101800011,"不锈钢法兰式球阀","Q41F-25P-50，DN50,PN2.5","GB/T12221-2005,公称直径：DN50，压力等级：P≤2.5Mp，阀体长度：216mm，阀体不锈钢","只",20,null,"炼钢厂部","2021-09-15"]
[19,7101800011,"不锈钢法兰式球阀","Q41F-25P-50，DN50,PN2.5","GB/T12221-2005,公称直径：DN50，压力等级：P≤2.5Mp，阀体长度：216mm，阀体不锈钢","只",5,null,"炼钢厂部","2021-09-15"]
[20,7101800149,"气动球阀","V634412","DN125 PN1.6","只",2,"GB/T8100-2009","管加工厂部","2021-09-15"]
[21,7101800132,"气动球阀","Q641H-25P-25","GB/T 12230-2005，含气动三联件","只",4,"GB12237-1989","炼钢厂部","2021-09-15"]
[22,6600300138,"自力式调压阀","ZZYP-16P-25","DN25;PN1.6MPa;调节范围1.1-10bar;介质:压缩空气;阀后型;材质:304不锈钢","只",5,"JB/T11049-2010","炼钢厂部","2021-09-15"]
[23,7101800216,"球阀","Q41F-16-125","DN125,PG16,法兰长度330，法兰安装螺孔中心孔∮210，8孔","只",2,"GB/T 12230-2005","管加工厂部","2021-09-15"]
[24,7101900027,"不锈钢截止阀","J41H-25P-20","铸造","只",5,null,"能源厂部","2021-09-15"]
[25,6600300137,"自力式调压阀","ZZYP-16P-20","DN20;PN1.6MPa;调节范围1.1-10bar;介质:压缩空气;阀后型;材质:304不锈钢","只",5,"JB/T11049-2010","炼钢厂部","2021-09-15"]
[26,7100100191,"切割氧减压阀","ZJD16-Q","进出连接螺纹G3/4''(外螺纹);密封形式为球面密封;两个压力输出点的螺纹为M14*1.5(内螺纹);外形尺寸230*175*128;输出压力0-0.6MPa","只",5,"GB/T12244-2006","炼钢厂部","2021-09-15"]
[27,7102000006,"静音式止回阀","DRVZ-16-250","PN1.6MPa DN250","只",3,"JB/T10365-2002","340热轧","2021-09-15"]
[28,7101800136,"气动球阀:","Q641H-25P-50","带电磁阀及回迅器","只",4,"GB/T12237","炼钢厂部","2021-09-15"]
[29,7101800003,"PPR全塑双活接头球阀","∮40","PPR GBT18742.3-2002，接外径∮40PPR管道","个",20,"GB/T50349-2005","能源厂部","2021-09-15"]
[30,7101700055,"双金属耐磨闸阀","WZ644P-10","DN200","只",1,"GB/T122202-1980","烧结","2021-09-15"]
[31,7101700081,"不锈钢闸阀","Z45W-25-200","PN25;DN200;阀芯、阀杆、阀体为不锈钢材质","只",1,"GB/T12234","炼钢厂部","2021-09-15"]
[32,7101700014,"弹性座封闸阀","RVHX-0100","PG16 DN100 连接形式法兰 DN100 压力:1.0～2.5MPa","只",3,"GB/T12221-1989","340热轧","2021-09-15"]
[33,6600300007,"电动蝶阀","D943X-10ZB","工作压力 1.0MPa DN300，配现场操作箱","只",4,"DL/T1068-2007","炼钢厂部","2021-09-15"]
[34,7101800157,"气动球阀","Q641PPL-16C","DN125;带电磁阀及回迅器","只",2,"GB12237-1989","高辅工段","2021-09-15"]
[35,7101600189,"电动法兰蝶阀","D943SH-2.5C","DN2000;阀体材质Q235;阀板材质：16Mn，阀杆材质：2Cr13；带电动装置：Z90-5000","台",2,null,"高炉","2021-09-15"]
[36,7102000002,"多功能止回阀","DY30AX DN250；压力10",null,"只",1,"GB/T12235-89","炼钢厂部","2021-09-15"]
[37,5501500008,"气动陶瓷出料阀","SZ674TC","公称通径DN200MM，公称压力PN1.0-2.5MPa，铸钢衬陶瓷，双作用，质保3年","个",4,null,"烧结","2021-09-15"]
[38,7101800010,"不锈钢法兰式球阀","Q41F-25P-25 DN25,PN2.5","GB/T12221-2005,公称直径：DN25，压力等级：P≤2.5Mp，阀体长度：165mm，阀体不锈钢","只",5,"GB/T12237","炼钢厂部","2021-09-15"]
[39,7102000052,"持压泄压阀","500X-25;DN250","DN250;PN2.5MPa;出厂时请调整为1.0～1.3MPA泄压","只",1,null,"180厂部","2021-09-15"]
[40,7101800009,"不锈钢法兰式球阀","Q41F-25P-DN32",null,"只",5,"GB/T12224-1989","炼钢厂部","2021-09-15"]
[41,7101700056,"弹性座封闸阀","RVHX-0125；PN16；",null,"只",2,"GB/T12237","炼钢厂部","2021-09-15"]
[42,7102600006,"底阀","H45X-10","DN350 阀体铸铁 阀板球墨铸铁 轴材不锈钢","只",2,"GB/T12235-2007","720厂部","2021-09-15"]
[43,7101700049,"弹性座封闸阀","RVHX-0150","PG16 DN150","只",4,"GB/T28776-2012","炼钢厂部","2021-09-15"]
[44,7101800036,"二片式不锈钢球阀","Q211F-16P-DN15","压力1.6MPa DN15","只",80,"GB/T12237-2007","炼钢厂部","2021-09-15"]
[45,7102000048,"消声止回阀","H41X-10;DN500","铸钢","只",1,"GB/T2100-1980","管加工厂部","2021-09-15"]
[46,5711100106,"步进炉风机入口调节阀","9-19-14D；左90°","风量：25916m3/h；全压：11771Pa；转速：1450n/m","件",1,"GB/T19232-2003","340热轧","2021-09-15"]
[47,7102700001,"快开排污阀","Z44H-25-25","铸造 GB/T13927","只",5,"GB/T13927","能源厂部","2021-09-15"]
[48,7101600174,"电动蝶阀","D971X","公称直径:DN150;耐压等级:1.0Mpa,带电动装置;电压等级:380V","台",16,"JB/T308-2004","能源厂部","2021-09-15"]
[49,7101800262,"二片式不锈钢球阀","Q11F-16P-DN65","压力1.6MPa DN65，螺纹连接ZG2 1/2，不锈钢316","只",4,"GB/T12237-2007","管加工厂部","2021-09-15"]
[50,7101800036,"二片式不锈钢球阀","Q211F-16P-DN15","压力1.6MPa DN15","只",30,"GB/T12237-2007","炼钢厂部","2021-09-15"]
[51,7102000043,"止回阀","H44W-10-400",null,"只",2,null,"管加工厂部","2021-09-15"]
[52,7101800206,"球阀","Q41H   DN100   PN16",null,"只",6,null,"219厂部","2021-09-15"]
[53,7101800149,"气动球阀","V634412","DN125 PN1.6","只",1,"GB/T8100-2009","89油管车丝委外","2021-09-15"]
[54,7101800157,"气动球阀","Q641PPL-16C","DN125;带电磁阀及回迅器","只",1,"GB12237-1989","89油管车丝委外","2021-09-15"]
[55,7101700084,"弹性座封闸阀","RVHX-0200;PG25;DN200","压力2.5MPa","只",2,"GB/T28776-2012","89热轧","2021-09-15"]
[56,7101700014,"弹性座封闸阀","RVHX-0100","PG16 DN100 连接形式法兰 DN100 压力:1.0～2.5MPa","只",5,"GB/T12221-1989","89热轧","2021-09-15"]
[57,7101800104,"气动球阀","Q641PPL-16C DN100 带电磁阀及回迅器",null,"只",1,"GB12237-1989","89热轧","2021-09-15"]
[58,7101800024,"不锈钢球阀","Q11F-64P-50",null,"只",10,"GB/T 21385-2008","219厂部","2021-09-15"]
[59,7101600109,"气动蝶阀","D641X-10;DN250;","L=250;带执行器","只",2,"GB/T28776-2012","89热轧","2021-09-15"]
[60,7102700014,"双层卸灰阀","XJY-30","铸造 GB16490-1996驱动方式重锤式，高度1260mm,法兰300*300mm,阀体宽度700*500mm,阀板材质45Mn 阀体承受负压≥20kPa,阀体材料厚度10mm,输送量15m?/h 300*300,Hs＝1200适用温度≤300℃ 电机功率0.75KW 重量≥0.45吨","只",1,"GB16490-1996","烧结","2021-09-15"]
[61,7101800069,"高压球阀","KHB-G3/4-1212-01X",null,"只",5,null,"高炉","2021-09-15"]
[62,5500800011,"气动卸灰耐磨硬密封球阀","QM647Y-1.6","DN150,双气缸 阀体WCB.球体1Cr18Ni9Ti+硬铬 1.6MPa 介质:高炉含尘埃 WCB QM647Y-1.6 双气缸 介质:高炉含尘埃,总长度390mm 硬密封 全球阀 耐温≥250℃ 球体1Cr18Ni9Ti+硬铬,工作压力1.6MPa","只",2,"GB12237-1989","高炉","2021-10-11"]
[63,5500800002,"电动金属硬密封耐磨蝶阀","DN600","铸钢 型号：防爆型 DN600 D943P-2.5 带电动装置 JB/T8527-1997 含硅胶密封条，耐温400℃ 启闭时间20S 金属垫600*670*10 电动装置型号 Z30-18B 电机功率 0.55KW 电压 380V 输出转矩 300N.m 输出转速 18r/min。","只",5,"JB/T18527-1997","高辅工段","2021-10-11"]
[64,5500800003,"电动扇型耐磨盲板阀","DN600","铸钢 型号 防爆型 F943X-2.5,工作压力0.25MPa,带电动装置,密封条材质氟橡胶246,工作温度-20℃-300℃;法兰JB/T8527-1997， 配2片金属缠绕垫600*670*10;电动装置型号 Z39-18B, 电机功率 0.5KW 电压 380V ,输出转矩 300N.m ,输出转速 18r/min,启闭时间20S；双层不锈钢金属波纹管材质为254SMo,厚度1.2mm*2;密封槽尺寸及电装联结结构尺寸需按技术规格书要求标准制造。","只",10,"JB/T18527-1997","高辅工段","2021-10-11"]
[65,7001600001,"气动开关蝶阀","Z011-A-10-400","对夹式;通径400;压力1MPa","台",1,"GB/T8100-2006","炼钢厂部","2021-09-26"]
[66,7101600202,"气动开关蝶阀","Z011-A-10-80","对夹式;通径80;压力1MPa","台",1,"GB/T8100-2006","炼钢厂部","2021-09-26"]
[67,7101600203,"气动开关蝶阀","Z011-A-10-250","对夹式;通径250;压力1MPa","台",1,"GB/T8100-2006","炼钢厂部","2021-09-26"]
[68,7101600204,"气动开关蝶阀","Z011-A-10-300","对夹式;通径300;压力1MPa","台",1,"GB/T8100-2006","炼钢厂部","2021-09-26"]
[69,7101600205,"气动开关蝶阀","Z011-A-10-900","对夹式;通径900;压力1MPa","台",1,"GB/T8100-2006","炼钢厂部","2021-09-26"]
[70,7101800100,"气动球阀","Q641H-25P-80","铸钢 GB12237-1989","只",20,null,"高辅工段","2021-10-11"]
[71,7101600032,"气动控制阀门","D376XE74",null,"只",2,"JB/T6375-1992","720厂部","2021-09-26"]
[72,7102100010,"气动控制阀门","D376XE69",null,"只",2,"ISO5211","720厂部","2021-09-26"]
[73,7102800009,"内螺纹旋塞阀","X13T-10","DN32","只",4,"GB/571-1986","炼钢厂部","2021-09-26"]
[74,7101600201,"手柄传动对夹式手动蝶阀","D71XJ-10","DN50","只",2,"GB/T12230-2005","炼钢厂部","2021-09-26"]
[75,7101600197,"气力输灰气动耐磨合金陶瓷阀DN200","GLS-HG20-200B2","公称通径：200MM,公称压力1.0-2.5MPa,，阀体铸钢陶瓷，阀板双面全陶瓷耐磨，侧阀座和阀门接触面为耐磨陶瓷材料 .","台",2,null,"烧结","2021-09-26"]
[76,7101600198,"气力输灰气动耐磨合金陶瓷阀DN80","GLS-HG20-80C3","公称通径：80MM,公称压力1.0-2.5MPa,，阀体铸钢陶瓷，阀板双面全陶瓷耐磨，侧阀座和阀门接触面为耐磨陶瓷材料","台",2,null,"烧结","2021-09-26"]
[77,7101600199,"气力输灰气动耐磨合金陶瓷阀DN65","GLS-HG20-65C2","公称通径：65MM,公称压力1.0-2.5MPa,，阀体铸钢陶瓷，阀板双面全陶瓷耐磨，侧阀座和阀门接触面为耐磨陶瓷材料","台",2,null,"烧结","2021-09-26"]
[78,7101600200,"气力输灰气动耐磨合金陶瓷阀DN50","GLS-HG20-50C1","公称通径：50MM,公称压力1.0-2.5MPa,，阀体铸钢陶瓷，阀板双面全陶瓷耐磨，侧阀座和阀门接触面为耐磨陶瓷材料","台",1,null,"烧结","2021-09-26"]