{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":27,"n_cols":11,"rows_kept":27,"merged":[[0,0,0,10],[1,0,1,10],[23,0,23,10],[24,0,24,10],[25,0,25,10],[26,0,26,10]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2021年8月液压备件采购项目Ⅱ                             项目编号：HGZB21423"]
["序号","资材编号","资材名称","规格型号","技术参数","单位","数量","使用部门","交货时间","含税单价（元）","生产厂家\n（品牌）"]
[1,7000300008,"齿轮泵","KV1P/3.8-D-CO-001 3/8\" No.114865","工作介质水乙二醇","台",1,"炼钢厂部","2022-02-08"]
[2,7100400089,"插装式溢流阀","VMD1.040.SV.000","100-350bar No.148373","只",1,"炼钢厂部","2021-10-11"]
[3,7100600011,"伺服换向阀","YJ741-100/100-L","YJ74型电液伺服阀 1系列 额定流量100L 额定电流100mA 电炉用 工作介质乳化液压油","只",1,"炼钢厂部","2021-10-11"]
[4,7000700005,"油泵电机组","40SCY-Y180M-4-B3","排量40ml/r 手动变量泵 压力等级31.5MPa 带电机","台",1,"炼钢厂部","2021-10-11"]
[5,7100300411,"手动换向阀","HV-03","G3/8螺纹;压力0.8MPa","只",8,"炼钢厂部","2021-09-27"]
[6,6100500342,"压力继电器","EDS 3446-1-0250-Y00+ZBE06+ZBM3000","HYDAC","只",2,"720厂部","2021-09-26"]
[7,6100500342,"压力继电器","EDS 3446-1-0250-Y00+ZBE06+ZBM3000","HYDAC","只",3,"340热轧","2021-09-26"]
[8,4000300222,"金属带锯条","HSS-M42;WIKUS  5080*41*1.3","HSS-M42;WIKUS  5080*41*1.3；最大切削规格400*400（晨龙G4240/50金属带锯床使用）","条",20,"340热轧","2021-10-27"]
[9,7100100139,"直动溢流阀","DBDS10P-10/315",null,"只",4,"高炉","2021-10-11"]
[10,7200500076,"电液推杆","DYTZ1750-300/60","推力17.5KN,推速60mm/s,行程300mm,电机型号Y100L-4-B5。功率2.2Kw","台",2,"高辅工段","2021-10-06"]
[11,7100300393,"液控单向阀","SL10PB2-6X","DN6,31.5MPa","个",4,"炼钢厂部","2021-09-26"]
[12,7100400097,"电液换向阀","DG5V-10-H-2C-M-U-H-10","介质:水乙二醇液压油;底板安装,P/T/A/B油口压力额定值350bar;阀规格 CETOP 10,ISO4401-10,NFP A D10;带手动操作;先导阀型式CETOP 3安装型式,高性能;阀芯型式闭式中位（全部油口）;阀芯弹簧对中;线圈型式ISO4400(DIN 43650);VICKERS","台",2,"炼钢厂部","2021-10-26"]
[13,7500400048,"过滤器","ZUI.BH-H250*5DFP","纸质滤芯;带旁通阀;工作介质水乙二醇液压油;公称压力32MPa;公称流量250L/min;过滤精度5um;倒装法兰式;带CMS式发讯器","台",1,"炼钢厂部","2021-09-26"]
[14,7201100021,"水冷式压下辊气缸","B206G20-15改","工作介质：净化压缩空气，工作压力： 0.1—1.5MPa。工作温度：0-60℃","台",2,"炼钢厂部","2021-09-26"]
[15,7500600055,"蓄能器组","Z0745.90.00.01","按图纸要求；含油路块、蓄能器、蓄能器控制阀组、油盆、阀台架及其它附件","套",4,"180厂部","2021-09-26"]
[16,7100100237,"溢流截止阀","YZF-F20L","DN20;315bar","只",4,"炼钢厂部","2021-10-11"]
[17,7100300401,"单向阀","HC41X-16C DN125","DN125 ","只",4,"炼钢厂部","2021-10-26"]
[18,7501400003,"避震喉","KXT-Ⅲ","DN200,三层，材质：橡胶","只",6,"180厂部","2021-09-26"]
[19,4201700123,"超轻型硫化机","BW=1000;ALEX-YHG3448","尺寸：1000*830mm，智能数字仪表控温系统，可“水压、气压、油压”通用切换打压，电压380伏","台",1,"原料工段","2021-09-26"]
[20,3301000055,"切削液","Master马思特 TRIM  SC310，每桶量：204L","水溶液推荐使用浓度： 3.0% - 10.0%","桶",20,"管加工厂部","2021-10-12"]
["注：1、投标报价含税，税率13% ；                                                                                                                          2、生产厂家要求全称填写准确无误 ；                                                                                                                     3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2021年8月液压备件采购项目Ⅱ                             项目编号：HGZB21423"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]