{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":46,"n_cols":11,"rows_kept":46,"merged":[[0,0,0,10],[1,0,1,10],[42,0,42,10],[43,0,43,10],[44,0,44,10],[45,0,45,10]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2022年1月液压备件采购项目                            项目编号：HGCGD22003"]
["序号","资材编号","资材名称","规格型号","技术参数","单位","数量","使用部门","交货时间","含税单价\n(元）","生产厂家\n（品牌）"]
[1,7000500005,"石墨泵","TBKP-80/110","GRACO,GBT10886-2002","台",1,"180厂部","2022-03-28"]
[2,7200700005,"液压马达","BM4-400PAY","1008N.M 6-305r/min GB/T20421.3-2006","台",8,"180厂部","2022-05-12"]
[3,7200800004,"气缸","FD10W44","直径100 H40,Pmax=10bar ISO 4401","台",4,"180厂部","2022-03-28"]
[4,7200900015,"气缸","DNC-80-25-PPV-A","80-25,163433,A908 ISO3320-2013","台",4,"180厂部","2022-03-28"]
[5,7201100009,"气缸","100/25-195 268.01SB0065-100",null,"台",2,"180厂部","2022-03-28"]
[6,7201100018,"气缸","QHR-3T250","80*250, 高温,JB/T7371-1994","只",25,"180厂部","2022-03-28"]
[7,7200800045,"气缸","SC100*180","缸径100；杆径180；工作压力0.6MPa。","台",4,"180厂部","2022-03-28"]
[8,7000700009,"油泵电机组","YB1叶片泵 6ml/R 6.3MPa 1450r/min 电机Y90S-4/1.1Kw",null,"台",2,"219厂部","2022-03-28"]
[9,7200800012,"气缸","QGB直径160*400MT4",null,"台",5,"219厂部","2022-03-28"]
[10,5712000039,"气缸","DNG-250-80-PPV-A 151892 FESTO",null,"台",2,"340热轧","2022-04-12"]
[11,7000700016,"液压泵电机组;","YCB1.6-0.6","流量26.6L/min;压力0.6MPa;功率0.75KW;转速910r/min;电机型号Y90S-6","台",5,"340热轧","2022-03-28"]
[12,7000700017,"圆孤齿轮泵组[带电机];","YCB8/0.6压力0.6MPA流量8立方米/小时",null,"台",2,"340热轧","2022-03-28"]
[13,7200700014,"液压马达","MR7000M-P2E1F1N1N RIVA CALZONI OLEODINAMICA",null,"台",1,"340热轧","2022-07-11"]
[14,7200900003,"气缸","QGB100-100F","安装方式:前法兰式","台",1,"340热轧","2022-03-28"]
[15,7201000007,"气缸","TGC100*50-TC","100*50 ISO15552","台",4,"340热轧","2022-03-28"]
[16,7000200013,"螺杆泵","HSNH280-43",null,"台",1,"720厂部","2022-03-28"]
[17,7100300419,"叠加式开关阀","AV700-6-AA-700-S-V-A*00;Bieri","DN6，耐压等级70Mpa","只",1,"720厂部","2022-03-28"]
[18,7100500105,"三通比例减压阀","3DREE16P-7X/200YG24K31F1V","DN16,内置放大器，4-20mA，0-20MPa","台",2,"720厂部","2022-03-28"]
[19,7100500117,"电液比例换向阀","4WRKE35W6-1000L-3X/6EG24K31/F1D3M","35通径；J型中位机能；控制油外控外排；电流输出","只",1,"720厂部","2022-03-28"]
[20,7100500118,"比例换向阀","KBFDG4V-5-2C50N25-Z-M2-PE7-H7-12","10通径；E型中位机能；电流控制","只",2,"720厂部","2022-03-28"]
[21,7100500119,"比例换向阀","4WRKE32W6-600L-3X/6EG24EK31/F1D3M","32通径；J型中位机能；内控外排；电流给定","只",1,"720厂部","2022-03-28"]
[22,7100500120,"比例换向阀","KBFDG4V-5-2C75N45-Z-M2-PE7-H7-12","10通径；E型中位机能；耐压等级31.5Mpa；电流型控制输入","只",2,"720厂部","2022-03-28"]
[23,7100500121,"比例换向阀","4WRTE16V1-125L-4X/6EG24ETK31/F1M","16通径；J型中位机能；控制油外控外","只",2,"720厂部","2022-03-28"]
[24,7000600007,"液压泵","PVH098R01AD30A250000002001AB010A PartNo:02-334632 VICKERS",null,"台",1,"89包装","2022-07-11"]
[25,7000100032,"液压泵","63PCY14-1B","排量63ml/r，定量泵，顺时针，平键安装","台",2,"89热轧","2022-03-28"]
[26,7200700015,"液压马达","OMS400 输出轴∮32,长67,E=1/2\" DEFOSS",null,"台",2,"89热轧","2022-03-28"]
[27,7000600007,"液压泵","PVH098R01AD30A250000002001AB010A PartNo:02-334632 VICKERS",null,"台",1,"管加工厂部","2022-07-11"]
[28,7000700011,"S非C三相电泵","DB-100","流量100l/min H=4米 250w","台",10,"管加工厂部","2022-03-28"]
[29,7200800023,"气缸","QGBⅡ-R125*750-MS1",null,"台",2,"管加工厂部","2022-03-28"]
[30,7200800029,"气缸","RA/8050/M/125",null,"台",4,"管加工厂部","2022-03-28"]
[31,7201100040,"气缸","SC-63X500-S-CA;","Max press:10MPa;SNS Pneumatic Co.LTD","台",4,"管加工厂部","2022-03-28"]
[32,7100800040,"换向阀阀块DN10","GJ02GYL-01-03","按图纸要求，含油路块、换向阀及其它附件","台",4,"管加工厂部","2022-03-28"]
[33,5501000048,"电液推杆","DYTZ1750-670/110","行程670","台",1,"炼钢厂部","2022-03-28"]
[34,6000200711,"电力液压推动器","ED-80/6","额定推力800N;电压380V;行程60MM;额定功率330W","套",2,"炼钢厂部","2022-03-28"]
[35,7000100068,"轴向柱塞泵","40MCY14-1B","排量40ml/r;定量泵;顺时针;平键安装","台",2,"炼钢厂部","2022-03-28"]
[36,7201100077,"气缸","SDA63X20-B-V","MAX.PRESS:1.00MPa","台",2,"炼钢厂部","2022-03-28"]
[37,6000400069,"主吹电磁阀","VXP2380-14-5D","工作压力：0.4～0.6MPa；调节气流大小，调整容器运行速度；使用流体：空气； 最高使用压力：1.0MPa，设定压力范围；0.1～0.7MPa;耐冲击/耐振动  150/30m/s;线圈电压；24v","台",1,"烧结","2022-03-28"]
[38,5501000048,"电液推杆","DYTZ1750-670/110","行程670","台",1,"原料工段","2022-03-28"]
[39,5501800025,"电液推杆","UPG20XL54B2050X25X750GC1AW5","推力1500KN;行程300mm,推速60mm/s;电机功率1.5Kw","台",1,"原料工段","2022-03-28"]
["注：1、投标报价含税，税率13% ；                                                                                                                          2、生产厂家要求全称填写准确无误 ；                                                                                                                     3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2022年1月液压备件采购项目                       项目编号：HGCGD22003"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]