{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":80,"n_cols":11,"rows_kept":80,"merged":[[0,0,0,10],[1,0,1,10],[76,0,76,10],[77,0,77,10],[78,0,78,10],[79,0,79,10]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2022年1月液压缸采购项目                             项目编号：HGCGD22002"]
["序号","资材编号","资材名称","规格型号","技术参数","单位","数量","使用部门","交货时间","含税单价","生产厂家\n（品牌）"]
[1,7200600225,"钢包加盖横移液压缸(二)","90/60-600","缸径Φ90,杆径Φ60,行程600;工作环境温度≤200℃;工作压力25MPa;试验压力31.5MPa;活塞及活塞杆采用V型组合密封;工作介质水乙二醇液压油;配GAS50耳环;图号:GBJG-HGL-02-3","台",2,"炼钢厂部","2022-03-26"]
[2,7200600226,"钢包加盖横移液压缸（三)","90/60-800","缸径Φ90,杆径Φ60,行程800;工作环境温度≤200℃;工作压力25MPa;试验压力31.5MPa;活塞及活塞杆采用V型组合密封;工作介质水乙二醇液压油;配GAS50耳环;图号:GBJG-HGL-02-4","台",3,"炼钢厂部","2022-03-26"]
[3,7200600227,"钢包加盖提升液压缸","140/100-1000","缸径Φ140,杆径Φ100,行程1000;工作环境温度≤200℃;工作压力25MPa;试验压力31.5MPa;活塞及活塞杆采用V型组合密封;工作介质水乙二醇液压油;配GAS80耳环;图号:GBJG-HGL-02-10","台",3,"炼钢厂部","2022-03-26"]
[4,7501800019,"液压缸铰接吊环头","CGKD160","M125*4","件",2,"炼钢厂部","2022-03-30"]
[5,7200600149,"中间包倾翻锁紧液压缸","250/170-80/50-150","进口密封 缸径Φ80,杆径Φ50,行程150 压紧伸缩煅件钢套Φ160,外固定钢套Φ250 工作环境温度-20℃~60℃ 工作压力17MPa,试验压力25MPa 活塞及活塞杆采用V型组合耐高温密封 工作介质水乙二醇液压油","台",2,"炼钢厂部","2022-03-30"]
[6,7200400025,"液压缸","CD250B50/28-325A10/02CGDMA","06.457-6","台",1,"炼钢厂部","2022-05-28"]
[7,7200600222,"1#炉倾动油缸","250/180-1300","双作用缸;缸径Φ250;杆径Φ180;行程1300;带缓冲;工作环境温度-20℃~70℃;工作压力20MPa;试验压力30MPa;活塞及活塞杆采用V型组合耐高温密封;工作介质水乙二醇液压油","台",1,"炼钢厂部","2022-03-26"]
[8,7200600093,"液压缸","HG-MFL-250.040.185-2-4# 40/28-600","缸径Φ40,杆径Φ28,行程600 工作环境温度-20℃~70℃ 工作压力16MPa,试验压力20MPa 活塞及活塞杆采用格莱圈加U型密封圈","台",2,"340热轧","2022-05-28"]
[9,7200600096,"液压缸","HYZ021745 80/45-425","缸径Φ80,杆径Φ45,行程425 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"340热轧","2022-05-28"]
[10,7200600118,"液压缸","PBA03DA00000 CYH2MT4/140/100/420A1X/B1CXDAWWD",null,"台",4,"340热轧","2022-05-28"]
[11,7201300053,"液压缸活塞杆","*","EC03J0000","件",6,"340热轧","2022-04-12"]
[12,7200100303,"液压缸","液压缸;CD250E160/110-400A10/02CADMA;L10=490.5","缸径Φ160,杆径Φ110,行程400 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"340热轧","2022-03-28"]
[13,7200100307,"液压缸;","CGH1MT4/180/110/430A1X/D1CSEMWW+CGAS90  XV=546;活塞杆内做防松动处理","缸径Φ180,杆径Φ110,行程430 工作环境温度-20℃~70℃ 工作压力16MPa,试验压力20MPa 活塞采用格莱圈密封 活塞杆采用格莱圈密封+USH密封组合 活塞杆与活塞做防松处理","台",1,"340热轧","2022-03-28"]
[14,7200400023,"液压缸","140/100-610+GE70CS-2Z","L10=600 268.01SB0048","台",1,"340热轧","2022-05-28"]
[15,7200400036,"液压缸","HYZ076-45;50/32-25",null,"台",2,"340热轧","2022-03-30"]
[16,7200600063,"推钢机液压缸","CD250B63/36-40A10/01.1CADMA","缸径Φ63,杆径Φ36,行程40 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"340热轧","2022-03-30"]
[17,7200200046,"液压缸","CD250E100/70-80A10/02CGDMA","额定压力25MPa JB/T 5000","台",2,"340热轧","2022-03-30"]
[18,7200600195,"液压缸;","1.MFL.008.00;50/28-350","缸径Φ50,杆径Φ28,行程350 工作环境温度-20℃~70℃ 工作压力16MPa,试验压力21MPa 活塞采用TPM196157-50/40*11.3*4密封;活塞杆密封采用OMS-MR28/35.3*3.2加通用密封;USH00280+挡圈;28*35.5*34.5*8.7","台",4,"340热轧","2022-03-30"]
[19,7200100128,"液压缸","CD250F80-45-400B10-01CADMT","额定压力25MPa JB/T 5000","台",1,"340热轧","2022-05-28"]
[20,7200100211,"液压缸","CD250B160/110-115A10/02CGDMA+GAK80",null,"台",1,"340热轧","2022-05-28"]
[21,7200100358,"液压缸","CD250E100/56-130A10/02CGDMT",null,"台",1,"219厂部","2022-03-28"]
[22,7200100058,"液压缸","CD250B100/56-490A10/02CGDMA","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",1,"219厂部","2022-05-28"]
[23,7200100229,"液压缸","CD250B125/90-320A10/02CGDMA+GKA58",null,"台",1,"219厂部","2022-05-28"]
[24,7200100406,"喷标后升降装置液压缸","CD250C5680150","活塞杆直径56，缸径80，行程150，压力25Mpa","台",2,"219厂部","2022-03-28"]
[25,7200400103,"液压缸","HSGL01-125/70E-1510-300","缸径125，杆径70，行程300，压力等级：25Mpa","台",1,"219厂部","2022-03-26"]
[26,7200400104,"液压缸","HSGL01-80/50E-1510-200","缸径80，活塞杆直径50，行程200，压力等级250Mpa","台",1,"219厂部","2022-03-26"]
[27,7200100258,"液压缸","PB21S000;125/90-1840","CD250C125/90-1840A10/01CADMA","台",2,"89热轧","2022-05-12"]
[28,7200100297,"液压缸","02680014DR5005ME044-35","CD250E100/70-927A10/01CGDMA,L10=630","套",2,"89热轧","2022-03-26"]
[29,7200100054,"液压缸","CD250B63/36-220A10/02CGDMA","额定压力25MPa JB/T 5000","台",2,"89包装","2022-05-28"]
[30,7200600162,"液压缸","HYZ02345","直径90/80-130","台",4,"89热轧","2022-05-28"]
[31,7200600207,"液压缸","PB16Y000G","缸径80杆径56行程234压力等级25MPa","台",3,"89热轧","2022-04-12"]
[32,7200600215,"液压缸组件","Z0202.03.02.03.00g1-7","油缸CD250E80/56-115A10/01CGDMA;L10=200;带耳环、铜套、碰块等附件","台",2,"89热轧","2022-03-26"]
[33,7201300033,"液压缸耳环","GAK22",null,"件",10,"89包装","2022-04-12"]
[34,7200400044,"液压缸","PBICM000","80/56-100;","台",2,"89热轧","2022-05-28"]
[35,7502000051,"液压缸耳环","GAK35",null,"件",10,"89包装","2022-04-12"]
[36,7502000059,"液压缸耳环","GAS40",null,"件",15,"89热轧","2022-04-12"]
[37,7200500065,"充液阀液压缸","TYG-07.08",null,"台",1,"89油管","2022-03-30"]
[38,7200400039,"液压缸","YG80/45-270",null,"台",1,"89油管","2022-03-30"]
[39,7200100372,"液压缸","YG63/45-100","缸径63mm，杆径45mm，行程100mm，压力等级25MPa，符合JB/T10205-2000","台",2,"89油管","2022-03-30"]
[40,7200200090,"液压缸","CDH2MF3/63/45/410A1X/B1CHDMWW","油口G3/4 压力等级：25MPa  行程410","台",3,"89油管","2022-03-30"]
[41,7200100351,"液压缸","CD250B50/36-70A10/01.1CADMA","压力25MPa","台",2,"89热轧","2022-03-28"]
[42,7200200086,"液压缸","PB65KSGWGG1125/90-1850双耳轴轴加粗为70","双耳轴轴加粗为70,缸体材料40Cr,原厂家韶关伟光","台",1,"89热轧","2022-03-26"]
[43,7200400005,"靠车液压缸","HSGK01-100/70E-1521-250-670","带耳环，密封材质：聚氨酯+丁晴橡胶，工作压力25MPa","台",2,"原料工段","2022-05-28"]
[44,7200400006,"平衡液压缸","HSGK01-125/70-5101-200-290","密封材质：聚氨酯+丁晴橡胶，工作压力25MPa","台",1,"原料工段","2022-05-28"]
[45,7200400007,"四辊破碎同步液压缸","125*90-120","密封材质：聚氨酯+丁晴橡胶，工作压力25MPa","台",2,"烧结","2022-05-28"]
[46,7200500006,"氮气吹扫阀液压缸","63/32-153","带耳环，密封材质：聚氨酯+丁晴橡胶，工作压力25MPa","台",2,"高炉","2022-05-28"]
[47,7200500022,"热风阀液压缸","WG01CD250C/100/70-1530","带耳环，密封材质：尼龙夹布V组，工作压力25MPa","台",1,"高炉","2022-05-28"]
[48,7200500084,"新开口机抬头油缸","XKKJTT-01","φ150/φ65-98.5，工作压力25MPa","台",2,"高炉","2022-03-26"]
[49,5721700016,"液压缸","YG80/45*230-F","审核图纸","台",1,"管加工厂部","2022-04-12"]
[50,7200400040,"液压缸","YG80/45*330-F",null,"台",1,"管加工厂部","2022-05-28"]
[51,7200100221,"液压缸","CD250B100/56-200A10/02CADMA+GAS50","进口密封","台",1,"管加工厂部","2022-05-28"]
[52,7200400105,"液压缸","HSGL01-100/50-135-E4011","缸径Φ100,杆径Φ50,行程135 工作环境温度-20℃~70℃ 工作压力16MPa,试验压力21MPa","台",1,"管加工厂部","2022-03-26"]
[53,7200400060,"液压缸","YG100/55-300-F改","不锈钢;带磁环及感应开关","台",1,"管加工厂部","2022-05-28"]
[54,7200400096,"液压缸","SDH2MP5/125/70/480A1XM1CGDMTC{含球铰耳环GAK58)","带球铰耳环;  内置防水型位移传感器RS-M0500-S1-DT05-A01","台",2,"管加工厂部","2022-03-26"]
[55,7200400098,"翻车机新压车液压缸","GGK1-φ125/φ70-2531-420-1360","密封确保12个月以上无内外泄漏；缸底、缸头带节流缓冲。油缸耳环关节轴承要求SKF品牌，且带锁紧装置；活塞杆顶端外丝M64*2.0-100","台",2,"原料工段","2022-03-26"]
[56,7200500024,"液压缸","0107119-36.101","额定压力25MPa JB/T 5000","台",5,"180厂部","2022-05-28"]
[57,7200600077,"液压缸","09401301.02.10 125/90-800",null,"台",2,"720厂部","2022-05-28"]
[58,7200100382,"液压缸","02690045DR5005ME028-4;CDH1MS2320/200/41002X/CSDMWW","缸径320；活塞杆直径200；行程4100；许用压力25Mpa","台",1,"720厂部","2022-03-26"]
[59,7200100383,"液压缸","02690045DR5005ME027-20；SDH1MT4/80/45-320A1X/B1CSDMTC；带位移传感器","缸径80；活塞杆直径45；行程320；位移传感器型号：RHM0340MR031A01","台",2,"720厂部","2022-03-26"]
[60,7200100384,"液压缸","02690045DR5005ME020-32；CD250E125/90-420A10/01CGDMA；L10=370；带位移传感器","缸径125；活塞杆直径90；行程420；位移传感器型号：RHM0440MR031A01","台",2,"720厂部","2022-03-26"]
[61,7200100385,"液压缸","02690045DR5005ME019-3；SDH2MT4/160/110-265；带位移传感器","缸径160；活塞杆直径110；行程265；位移传感器型号：RHM0285MR031A01","台",1,"720厂部","2022-03-26"]
[62,7200100386,"液压缸","02690045DR5005ME019-8；SDH2MT4/140/100-580；活塞杆与杆头整体锻造","缸径140；活塞杆直径100；行程580；活塞杆材质：42CrMo4","台",2,"720厂部","2022-03-26"]
[63,7200100387,"液压缸","02690045DR5005ME021-9；CD250B100/70-320A10/01CADMA","缸径100；活塞杆直径70；行程320","台",1,"720厂部","2022-03-26"]
[64,7200100389,"液压缸","02690045DR5005ME004-6；SDH1MT4/250/160/360A2X/B1CSDMWW","缸径250；活塞杆直径160；行程360；许用压力25Mpa","台",1,"720厂部","2022-03-26"]
[65,7200100390,"液压缸","02690045DR5005ME010-4；CD250B250/140-400A10/01CGDMA","缸径250；活塞杆直径140；行程400","台",1,"720厂部","2022-03-26"]
[66,7200100391,"液压缸","02690045DR5005ME011-4；CD250C200/140-360A10/01CGDMA；带位移传感器","缸径200；活塞杆直径140；行程360；位移传感器型号：RHM0380MR101A01","台",1,"720厂部","2022-03-26"]
[67,7200100392,"液压缸","02690045DR5005ME004-32；180/7.5；带碟型弹簧复位机构","缸径180；行程7.5；许用压力25Mpa","台",2,"720厂部","2022-03-26"]
[68,7200100395,"液压缸","02690045DR5005ME036-5；CD250E140/90-280A10/01CGDMA；L10=380；带位移传感器","缸径140；活塞杆直径90；行程280；位移传感器型号：RHM0300MR031A01","台",1,"720厂部","2022-03-26"]
[69,7200100396,"液压缸","02690045DR5005ME037-25；CD250B125/90-280A10/01CADMA","缸径125；活塞杆90；行程280；许用压力25Mpa","台",2,"720厂部","2022-03-26"]
[70,7200100397,"液压缸","02690045DR5005ME035-3；CD250E125/90-450A10/01CADMA；带位移传感器","缸径125；活塞杆直径90；行程450；位移传感器型号：RHM0470MR031A01","台",2,"720厂部","2022-03-26"]
[71,7200100398,"液压缸","02690045DR5005ME033-12；CD250C125/90-200A10/01CGDMA；带位移传感器","缸径125；活塞杆直径90；行程200，位移传感器型号：RHM0220MR031A01","台",1,"720厂部","2022-03-26"]
[72,7200100399,"液压缸","02690045DR5005ME032-13；CD250B80/56-160A10/01CADMA","缸径80；活塞杆直径56；行程160；许用压力25Mpa","台",1,"720厂部","2022-03-26"]
[73,5715100030,"推拉液压缸活塞杆","CD250C280/200-5250A10/02CAD型液压缸活塞杆","缸径280mm;活塞杆200mm;行程5250mm;工作压力25Mpa;头部安装","根",2,"720厂部","2022-03-26"]
["注：1、投标报价含税，税率13% ；                                                                                                                          2、生产厂家要求全称填写准确无误 ；                                                                                                                     3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2022年1月液压缸采购项目                             项目编号：HGCGD22002"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]