{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":35,"n_cols":11,"rows_kept":35}
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","备注"]
[1,5501000065,"焦炭筛聚氨酯筛板","GY20220127-CX","介质：焦炭，材质：聚氨酯，使用寿命3个月处理能力300吨/小时。包含整套焦炭筛所用聚氨酯HW筛板和聚氨酯HW筛板托架。槽下全套筛板由16块高弹悬浮面小筛板","套",6,"审核图纸","高辅工段","2022-03-09"]
[2,5501000066,"焦炭筛聚氨酯筛框架","GY20220127-ST","\"为安装在槽下焦炭聚氨酯筛板所需框架和辅助配件。每套具体包括侧板1套,3852mm*1764mm*523mm。1件，Q235B；入料口耐磨衬板882*17641块；出料口加强耐磨筋板,1块706*1764；轨座1764mm*2852mm*10mm，16件，聚氨酯；压木100mm*40mm*1764mm，16件，聚氨酯；楔子233mm*50mm*40mm，16件，聚氨酯；不锈钢螺栓M16*35，8.8级，50套；防松不锈钢螺栓M16*50（双帽），8.8级，50套。\n，聚氨酯；压木100mm*40mm*1525mm，1套。\"","套",4,"审核图纸","高辅工段","2022-03-09"]
[3,7001900024,"喷印机油漆","1件4瓶，1瓶4升。","DMJ-1/P","件",35,"GB/T1723-1993","180/340厂部","2022-04-13"]
[4,7001900025,"油漆清洗剂","1件4瓶，1瓶4升。","DMJ-1/R","件",65,"GB/T6743-1986","180/340厂部","2022-04-13"]
[5,7001900057,"油漆喷印机","MJPH-16-I（CPMH-16-I）","油漆喷印机;CPMH-16-I;16个点阵","件",1,"GB/T14885-1994","340热轧","2022-04-13"]
[6,6400100035,"免烘烤型连续测温管","HFC-G-IV-C-1100-95B","测 量 范 围:800～1800℃;测量不确定度:±3℃;测温管寿命:≥30小时;响应时间:热态响应时间≤ 75s","根",60,null,"炼钢厂部","2022-04-13"]
[7,7102700027,"液动组合式矿浆阀","YZKF-10C，DN400","阀体：耐磨钢  阀体内衬陶瓷  闸板：45#钢，表面硬化处理后镀铬；  介质：矿浆  闸板两侧各有两道密封；结构长度：460mm   铸造 带油缸、带密封组件，氟橡胶","台",1,"GB/571-1986","高炉","2022-04-13"]
[8,7102700003,"除磷阀","VT-HDQ65/320Q-N24-FD",null,"只",1,"GB/T13320","180厂部","2022-04-13"]
[9,7102700024,"液动组合式矿浆阀","YZKF-10C，DN250","阀体：耐磨钢  阀体内衬陶瓷  闸板：45#钢，表面硬化处理后镀铬；  介质：矿浆  闸板两侧各有两道密封；结构长度：310mm   铸造 带油缸、带密封组件，氟橡胶","台",2,"GB/571-1986","高炉","2022-04-13"]
[10,7100100107,"燃气减压阀","ZJD16-R","进出连接螺纹G3/4''(外螺纹) 密封形式为球面密封 两个压力输出点的螺纹为M14*1.5(内螺纹) 外形尺寸230*175*128 输出压力0-0.6MPa","只",3,"GB/T12244-2006","炼钢厂部","2022-04-13"]
[11,7502300037,"双介质气雾喷枪","621072303-03-00-2","P=0.6MP;Qmax3.7T/H;＜120°;￠3500;H~3000;枪长1600;开孔273;316L护板","把",2,"GB/T4213-1992","炼钢厂部","2022-04-13"]
[12,5702900063,"拖链订货图(不含护板)","02690005DR5004ME008-151G","成品;128Kg;拖链参数:拖链截面尺寸(宽*高):305*108mm,内腔截面尺寸(宽*高):300*80mm,弯曲半径R=250mm,节距:91mm,长度:8099mm,拖链未注尺寸及性能按型号5050.30.250.0制作","套",1,"审核图纸","180厂部","2022-04-13"]
[13,5602100007,"补偿器DN40","B227G35-14","4Kg;","件",4,"审核图纸","炼钢厂部","2022-04-13"]
[14,5602100008,"补偿器DN150","B226G45-27","12Kg;","件",4,"审核图纸","炼钢厂部","2022-04-13"]
[15,5300101032,"楔形接头","钢丝绳公称直径为36mm","楔套材料采用不低于GB/T11352-1989中规定的ZG270-500碳钢件;楔的材料采用不低于GB/T9439-1988中规定的HT200灰铸铁件","套",2,"GB/T5973-2006","炼钢厂部","2022-04-13"]
[16,5100300068,"制动器液压推动器","Ed300-60","制动器型号:YWZE630/300","台",2,"JB/T6406-2006","炼钢厂部","2022-04-13"]
[17,5300101029,"制动器摩擦片","直径630mm;厚度18mm;不带槽","适应于YWZE630/300制动器","片",20,"JB/T6406-2006","炼钢厂部","2022-04-13"]
[18,7100200112,"整流叠加板","Z4S16-2X","16通径；31.5Mpa","只",1,"DIN24 340 A型","720厂部","2022-04-13"]
[19,6600100072,"标准型定氧探头","CE1200Hi-S",null,"只",1200,"Q/IBRF1-2010","炼钢厂部","2022-04-13"]
[20,5300100663,"制动器","YWM-400/E80",null,"台",2,"JB/T7019-2013","180厂部","2022-04-13"]
[21,5100100547,"梅花联轴器","ML7；Y60*150/Y35*70",null,"套",4,"GB5272-1985","720厂部","2022-04-13"]
[22,5100100549,"尼龙柱销联轴器","HL8；J110*167/90*172","HL8；尼龙柱销","套",2,"GB/T5014-2017","720厂部","2022-04-13"]
[23,5100100548,"联轴器","GⅡCL7 Y80*172/80*172","GⅡCL7 Y80*172/80*172","套",5,"ZBJ19013","720厂部","2022-04-13"]
[24,5500300092,"炮机破粹钎杆（SYBA43)","直径75*755","42CrMo","件",2,"GB/T6481-2002","高炉","2022-04-13"]
[25,5500300091,"炮机破粹钎杆（SYB16)","直径45*580","42CrMo","件",2,"GB/T6481-2002","高炉","2022-04-13"]
[26,6100100183,"法兰式补偿器","YN3600-850","柔性连接;导电截面积≥3600mm;内部材质T2;内部通水冷却","件",3,"Q320282PEQ001-2011","炼钢厂部","2022-04-13"]
[27,5100100546,"十字轴式万向联轴器","SWC250A-780","回转直径250mm;轴线折角15°;公称转矩63KN.m","套",2,"JB/T5513-1991","炼钢厂部","2022-04-13"]
[28,5300100978,"齿轮联轴器","CLZ92.6-Q10-017","77Kg","套",2,"GB5226.2-2002","炼钢厂部","2022-04-13"]
[29,5712300052,"高温抗辐射平焰烧嘴","LBT-300PLN/G",null,"件",18,"审核图纸","340步进炉","2022-04-13"]
[30,5100100545,"LLB7(R)联轴器","Y48*112/J1 42*84","联轴器内孔孔型及直径为Y48*112与/J1 42*84，13Kg","套",4,"JB/ZQ4018","180厂部","2022-04-13"]
[31,5501000061,"双辊破碎机","2PG-φ200*125；给料粒度《10mm；出料粒度0.8-4mm；电机功率3Kw","200*125,0.8-0.4mm","台",3,"JB/T3279-2005","高炉","2022-04-13"]
[32,7502300052,"6区全水喷嘴","3/8PZ7080QZ5","材质;黄铜;最大喷射角度68°","只",200,"YB4087-1992","炼钢厂部","2022-04-13"]
[33,6600100076,"定氢探头(钢包型)","HS900",null,"支",360,"Q/IBRF6-2010","炼钢厂部","2022-04-13"]
[34,5709600170,"打孔机专用碳棒","DTB-30-520",null,"件",800,"JB/T8679-1998","340热轧","2022-04-13"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}