{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":40,"n_cols":11,"rows_kept":40,"merged":[[0,0,0,10],[1,0,1,10],[36,0,36,10],[37,0,37,10],[38,0,38,10],[39,0,39,10]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2022年2月液压缸采购项目                             项目编号：HGCGD22016"]
["序号","资材编号","资材名称","规格型号","技术参数","单位","数量","使用部门","交货时间","含税单价","生产厂家\n（品牌）"]
[1,7200100409,"液压油缸","CD250B160/100-350ACGDMA",null,"台",4,"219厂部","2022-04-30"]
[2,7200100408,"液压油缸","CD250F200/140-3000A10/02CGDMA(带北京航天位移传感器)",null,"台",4,"219厂部","2022-04-30"]
[3,7502000060,"液压缸耳环","GAS60",null,"件",2,"89油管热处理","2022-05-13"]
[4,7200100067,"液压缸","CD250B80/56-320A10/02CGDMA+GAK35","缸径Φ80,杆径Φ56,行程320 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"89油管热处理","2022-06-12"]
[5,7200400030,"液压缸","HY89G099-40B;63/36-40",null,"台",2,"89油管热处理","2022-06-12"]
[6,7200100353,"液压缸","PBIDZ000,63/45-100","缸径63mm，杆径45mm，行程100mm，压力等级25MPa，V型组合密封，符合JB/T10205-2000","台",5,"89热轧","2022-04-30"]
[7,7200100046,"液压缸","CD250E100/70-450A10/02CADMA L10=390","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",1,"219厂部","2022-06-12"]
[8,7200100089,"液压缸","CD250E125/70-250A10/02CADMA+GAS60 L10=370","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",1,"219厂部","2022-06-12"]
[9,7200500034,"液压缸","CD250B80/56-90A10/02CADMA","额定压力25MPa JB/T 5000","台",2,"180厂部","2022-06-12"]
[10,7200500024,"液压缸","0107119-36.101","额定压力25MPa JB/T 5000","台",6,"180厂部","2022-06-12"]
[11,7200100369,"液压缸","CD250F125/90-250A10/02CADMA","缸径125；杆径90；行程250；耐压等级25MPA；连接螺栓12.9级","台",2,"180厂部","2022-02-27"]
[12,7200200010,"锁紧液压缸","0290017DR5004ME002-94","125/90-120,,JB/T 5000","台",2,"180厂部","2022-06-12"]
[13,7200600064,"推坯液压缸","Z0734.02.01.01 200/140-4500改",null,"台",1,"720厂部","2022-06-12"]
[14,7200100024,"液压缸","CD250B/200/140-620A10/01CGDMA+GAK110",null,"台",1,"720厂部","2022-06-12"]
[15,7200100206,"液压缸","CD250E100/56-340A10/01CADMA;","L10=405，压力21MPa","个",2,"管加工厂部","2022-06-12"]
[16,7200100082,"液压缸","CD250E100/56-280A10/01CADMA","带耳环GAS50 L10=280 额定压力25MPa JB/T 5000","台",1,"管加工厂部","2022-06-12"]
[17,7200500037,"液压缸","HG180006 PT219.80HL1-01.04.01.07-00","额定压力25MPa JB/T 5000","台",2,"管加工厂部","2022-06-12"]
[18,7200500007,"堆取料机俯仰液压缸","TG0024.280/200-2500.09.01.15LT","带耳环，关节轴承使用国内品牌轴承，密封材质：聚氨酯+丁晴橡胶，工作压力25MPa","台",2,"原料工段","2022-08-11"]
[19,7200200004,"夹钳升降液压缸","02690017DR5004ME002-39","额定压力25MPa 实验压力32MPa JB/T 5000","台",1,"180厂部","2022-06-12"]
[20,7201300061,"2#矫直机中下辊锁紧缸","Z8037.03.04.00",null,"台",2,"340热轧","2022-06-12"]
[21,7200100341,"液压缸","PBA03C600000，CD250E200/140-250A10/02CGDMA，L10=460","缸径Φ200,杆径Φ140,行程250工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"340热轧","2022-04-28"]
[22,7200100037,"液压缸","CD250B125/70-195A10/02CGDMA","缸径Φ125,杆径Φ70,行程195 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封 油口与尾关节轴承中心线方向一致","台",2,"340热轧","2022-06-12"]
[23,7200600125,"液压缸","PBA03DK00000 100/63-150","缸径Φ100,杆径Φ63,行程150 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",2,"340热轧","2022-06-12"]
[24,7200100016,"液压缸","CD250A100/70-180A10/02CADMA+GAS50","缸径Φ100,杆径Φ70,行程180 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞采用PG型组合密封 活塞杆采用RS+USH型组合密封","台",2,"340热轧","2022-06-12"]
[25,7200100035,"液压缸","CD250F63/36-100A10/02CGDMA","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",3,"340热轧","2022-06-12"]
[26,7200400064,"液压缸","CDH1MT4/63/45-2000A11/B1CMEMAW",null,"台",1,"340热轧","2022-06-12"]
[27,7200600104,"液压缸","PAB03CG00000 100/70-290","缸径Φ100,杆径Φ70,行程290 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",2,"340热轧","2022-06-12"]
[28,7502000054,"液压缸耳环","GAK58",null,"套",5,"340热轧","2022-05-13"]
[29,7200100407,"称重油缸","CD250F40/25-175A10/02CGDMA","缸径40；活塞杆直径25；行程175；接头螺纹M14*1.5；耳环螺纹M22*1.5；法兰螺丝孔4-Φ13","台","1","219厂部","2022-04-30"]
[30,7200600236,"平衡锁紧缸","KZ1810.02.03.06.00","缸径Φ100,杆径Φ50, 工作压力14MPa,试验压力25MPa 工作环境温度-20℃~70℃，厂家：太原科达成套设备有限公司","台",1,"89油管热处理","2022-06-08"]
[31,7200100052,"液压缸","CD250B40/28-230A10/02CADMA","额定压力25MPa JB/T 5000 环境温度100℃","台",6,"180厂部","2022-07-13"]
[32,7200100377,"液压缸","CD250F125/90-380A10/02CADMA","油口G1 1/4；缸径125；杆径90；行程380；耐压等级25MPA;螺栓12.9级","台",2,"180厂部","2022-03-30"]
[33,7200500027,"液压缸","02690005DR5004ME028-5","CD250B140/90-530A10/01CGDMA 带耳环GAK65 额定压力25MPa JB/T 5000","台",1,"180厂部","2022-07-13"]
["注：1、投标报价含税，税率13% ；                                                                                                                          2、生产厂家要求全称填写准确无误 ；                                                                                                                     3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2022年2月液压缸采购项目                             项目编号：HGCGD22016"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]