{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":9,"n_cols":11,"rows_kept":9}
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","备注"]
[1,null,"铁屑撕碎机","见技术规格书",null,"台",1,null,"管加工厂铁屑撕碎机项目","2022-4-15"]
[2,7001800287,"长轴立式泵","250LD2-40;带90KW电机;额定流量480m3/h;额定扬程39.6m;泵轴材质2Cr13;叶轮、滤网材质304不锈钢;液下深度4600mm-6100mm;滚动轴承为SKF品牌",null,"台",2,null,"炼钢厂3#连铸机水系统改造项目（HG202214）","2022-5-30"]
[3,7001800406,"离心水泵","SLOW100-320-132Kw;流量283m3/h;扬程;119m;电机转速2950r/min;电机功率132Kw;效率78%;必需气蚀余量9.5m;泵重223kg;带电机",null,"台",3,null,"炼钢厂3#连铸机水系统改造项目（HG202214）","2022-5-30"]
[4,7001800407,"立式离心泵","SLS200-315（I）B；流量346m3/h;扬程24m;转速1450r/min;配用功率37Kw;带电机",null,"台",4,null,"炼钢厂3#连铸机水系统改造项目（HG202214）","2022-5-30"]
[5,6200200392,"软起动器","150-B360NBDB AB 升级为150-F361NBD；输入电压3AC 380V 功率355Kw 允许电动机最大电流625A",null,"台",3,null,"炼钢厂3#连铸机水系统改造项目（HG202214）","2022-5-30"]
[6,6600300162,"气动单座调节阀","501T-65A*40A；介质:水:口径:65A*40A:ANSI:150# A216-WCB 等百分比 气关式:阀体材质WCB:阀芯类型:P孔单座:阀芯材质316:防护等级IP65:泄露等级IV级:配KOSO阀门定位器",null,"只",9,null,"炼钢厂3#连铸机水系统改造项目（HG202214）","2022-5-30"]
[7,6600300163,"气动单座调节阀","501T-50A*32A；介质:水:口径:50A*32A:ANSI 150# A216-WCB 等百分比 气关式:阀体材质WCB:阀芯类型:P孔单座:阀芯材质316:防护等级IP65:泄露等级IV级:配KOSO阀门定位器。",null,"只",5,null,"炼钢厂3#连铸机水系统改造项目（HG202214）","2022-5-30"]
[8,6600300164,"气动单座调节阀","FlowTop 1.5inch CL150；气闭式:DN40/PN16;额定CV 18.5 等百分比 下流向 RF法兰连接:阀体材质A216-WCC;阀芯材质316SS;行程20mm 失气开;气源工作压力4MPa;定位器带阀位就地指示;带过滤减压阀",null,"只",4,null,"炼钢厂3#连铸机水系统改造项目（HG202214）","2022-5-30"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}