{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":42,"n_cols":11,"rows_kept":42,"merged":[[0,0,0,10],[1,0,1,10],[38,0,38,10],[39,0,39,10],[40,0,40,10],[41,0,41,10]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2022年3月液压备件采购项目                            项目编号：HGCGD22026"]
["序号","资材编号","资材名称","规格型号","技术参数","单位","数量","使用部门","交货时间","含税单价\n(元）","生产厂家\n（品牌）"]
[1,7502900153,"油液检测模块","FMM-O-M-0-CS1320-A-AS3-0-0-0/-000+ZBE44+ZBE08,HYDAC","包括清洁度检测、含水量检测，输出4-20MA，带显示屏，旁路安装，工作压力6-15bar,介质温度0-85℃","台",1,"340热轧","2022-05-28"]
[2,7200500058,"电液推杆","DYT-SJ15000N-360",null,"台",1,"烧结","2022-07-11"]
[3,7200500076,"电液推杆","DYTZ1750-300/60","推力17.5KN,推速60mm/s,行程300mm,电机型号Y100L-4-B5。功率2.2Kw","台",1,"烧结","2022-05-07"]
[4,7200900060,"气缸","QGSQ100*300MT4-Y","行程300，气管接头与耳轴错开90°，接头尺寸G1/2","件",4,"高炉","2022-04-27"]
[5,7200700026,"液压马达","OMH400","danfuss","台",2,"89热轧","2022-05-28"]
[6,7200700016,"液压马达","OMT400 输出轴∮40,长82,E=1/2\" DEFOSS",null,"台",4,"89热轧","2022-05-28"]
[7,7100100237,"溢流截止阀","YZF-F20L","DN20;315bar","只",4,"炼钢厂部","2022-04-27"]
[8,7000400008,"叶片泵","150T-75-F-R",null,"台",2,"720厂部","2022-04-27"]
[9,7000300011,"齿轮油泵","2CY3.3/1.45-1 流量3.3m3/h 1.45MPa",null,"台",15,"管加工厂部","2022-04-27"]
[10,7501100233,"铰接式接头","12-G3/8(SN865-WH12SR-KDS)不锈钢","SN865-WH12SR-KDS不锈钢","只",100,"180厂部","2022-04-27"]
[11,7501100233,"铰接式接头","12-G3/8(SN865-WH12SR-KDS)不锈钢","SN865-WH12SR-KDS不锈钢","只",40,"340热轧","2022-04-27"]
[12,7500600026,"蓄能器","SK350-5/2212A9-350AAF-VA-10 国产化",null,"台",2,"340热轧","2022-04-27"]
[13,7201300094,"活塞筒体BARREL","27774","PUMP SECTOPM -T SEAL 3/4\" PACKED PLUNGER GAS BOOSTER -315 RATIO ;CODE IDENT NO. 81400;DWG NO.27780;Haskel气体增压泵14AGT-125/315-29125用","件",1,"检验检测中心","2022-04-27"]
[14,7201300095,"活塞杆PLUNGER","28199","PUMP SECTOPM -T SEAL 3/4\" PACKED PLUNGER GAS BOOSTER -315 RATIO ;CODE IDENT NO. 81400;DWG NO.27780;Haskel气体增压泵14AGT-125/315-29125用","件",1,"检验检测中心","2022-04-27"]
[15,7000200059,"三螺杆泵","GR55SMT16B300LRF2(112M)","300L;含钟罩联轴器","台",1,"炼钢厂部","2022-04-27"]
[16,7200800029,"气缸","RA/8050/M/125",null,"台",4,"管加工厂部","2022-04-27"]
[17,7000700011,"S非C三相电泵","DB-100","流量100l/min H=4米 250w","台",10,"管加工厂部","2022-04-27"]
[18,5712000039,"气缸","DNG-250-80-PPV-A 151892 FESTO",null,"台",2,"340热轧","2022-04-27"]
[19,7200700014,"液压马达","MR7000M-P2E1F1N1N RIVA CALZONI OLEODINAMICA",null,"台",1,"340热轧","2022-07-11"]
[20,7200800004,"气缸","FD10W44","直径100 H40,Pmax=10bar ISO 4401","台",4,"180厂部","2022-03-13"]
[21,7200700015,"液压马达","OMS400 输出轴∮32,长67,E=1/2\" DEFOSS",null,"台",2,"89热轧","2022-04-27"]
[22,7001100001,"气动柱塞泵","No:222833","100m3/h，H=10m，配管102mm长30M,GB/T2469-2009","台",1,"89油管热处理","2022-04-27"]
[23,7000500012,"液压马达","MRE2100H-P1Q1N1N1N","DESION","台",1,"管加工厂部","2022-06-13"]
[24,7100700011,"同步马达","FMP-2I-EB",null,"台",1,"340热轧","2022-05-30"]
[25,7201200003,"水压机;增压器","APT245.105-100","耐压110MPa","台",1,"89油管热处理","2022-07-13"]
[26,5501800025,"电液推杆","UPG20XL54B2050X25X750GC1AW5","推力1500KN;行程300mm,推速60mm/s;电机功率1.5Kw","台",2,"烧结","2022-04-27"]
[27,7500400064,"不锈钢水过滤器","GL41H-40","材质:304不锈钢;通径40mm;1.6MPa;过滤精度:150um","只",2,"炼钢厂部","2022-04-27"]
[28,7500400065,"不锈钢水过滤器","GL41H-32","材质:304不锈钢;通径32mm;1.6MPa;过滤精度:150um","只",2,"炼钢厂部","2022-04-27"]
[29,7500400066,"不锈钢水过滤器","GL41H-25","材质:304不锈钢;通径25mm;1.6MPa;过滤精度:150um","只",2,"炼钢厂部","2022-04-27"]
[30,7000400031,"TRT透平机主润滑泵","BJC.60.20","公称压力0.65MPa，公称流量670L/min","台",1,"高辅工段","2022-04-27"]
[31,7100300422,"液控单向阀","405063 006;Dr.BREIT","DN70，耐压等级31.5Mpa;","只",1,"720厂部","2022-04-27"]
[32,5501800025,"电液推杆","UPG20XL54B2050X25X750GC1AW5","推力1500KN;行程300mm,推速60mm/s;电机功率1.5Kw","台",1,"原料工段","2022-04-27"]
[33,7100800040,"换向阀阀块DN10","GJ02GYL-01-03","按图纸要求，含油路块、换向阀及其它附件","台",4,"管加工厂部","2022-04-27"]
[34,7500400063,"管道过滤器","GL41H-150C","配对法兰DN150,PN1.6","只",1,"炼钢厂部","2022-04-27"]
[35,7100300421,"电磁换向阀","WV700-6-3/3-E-24-V-C*00;Bieri","DN6，耐压等级70Mpa","只",1,"720厂部","2022-04-27"]
["注：1、投标报价含税，税率13% ；                                                                                                                          2、生产厂家要求全称填写准确无误 ；                                                                                                                     3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2022年3月液压备件采购项目                       项目编号：HGCGD22026"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]