{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":44,"n_cols":13,"rows_kept":44,"merged":[[0,0,0,8],[1,0,1,12],[40,0,40,8],[41,0,41,8],[42,0,42,8],[43,0,43,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2022年4月机械配件采购项目                     项目编号：HGCGD22037"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,7502300037,"双介质气雾喷枪","621072303-03-00-2","P=0.6MP;Qmax3.7T/H;＜120°;￠3500;H~3000;枪长1600;开孔273;316L护板","把",2,"GB/T4213-1992","炼钢厂部","2022-05-29"]
[2,7502400028,"水泵","350LT-30-6","980m3/H H=30m 不带电机","台",1,"CJ/T235-2006","340热轧","2022-05-29"]
[3,5602100007,"补偿器DN40","B227G35-14","4Kg;","件",4,"审核图纸","炼钢厂部","2022-05-29"]
[4,5602100008,"补偿器DN150","B226G45-27","12Kg;","件",4,"审核图纸","炼钢厂部","2022-05-29"]
[5,5300101032,"楔形接头","钢丝绳公称直径为36mm","楔套材料采用不低于GB/T11352-1989中规定的ZG270-500碳钢件;楔的材料采用不低于GB/T9439-1988中规定的HT200灰铸铁件","套",2,"GB/T5973-2006","炼钢厂部","2022-05-29"]
[6,7001800038,"管道离心泵","S200-150-400(I)A","270m3/h H=45m","台",1,"GB/T2347-1980","管加工厂部","2022-05-29"]
[7,5500300092,"炮机破粹钎杆（SYBA43)","直径75*755","42CrMo","件",2,"GB/T6481-2002","高炉","2022-05-29"]
[8,5500300091,"炮机破粹钎杆（SYB16)","直径45*580","42CrMo","件",2,"GB/T6481-2002","高炉","2022-05-29"]
[9,6100100183,"法兰式补偿器","YN3600-850","柔性连接;导电截面积≥3600mm;内部材质T2;内部通水冷却","件",3,"Q320282PEQ001-2011","炼钢厂部","2022-05-29"]
[10,5300100978,"齿轮联轴器","CLZ92.6-Q10-017","77Kg","套",2,"GB5226.2-2002","炼钢厂部","2022-05-29"]
[11,5702300189,"下棒装置装配图","LD45(DJ)-070100","装配件；12.93Kg","套",1,"审核图纸","180厂部","2022-05-29"]
[12,5702300190,"换棒装置","LD45(DJ)-070200","装配件；11.65Kg","套",1,"审核图纸","180厂部","2022-05-29"]
[13,5702300191,"减速电机装配图","LD45(DJ)-020000","装配件；31.98Kg","套",1,"审核图纸","180厂部","2022-05-29"]
[14,7001800033,"高压浊环水泵","KQSN200-N5/334",null,"台",1,"GB5662-1985","180厂部","2022-06-13"]
[15,5707900001,"半自动卧式带锯机","G4240/50",null,"台",2,"GB/16454-2008","180厂部","2022-05-14"]
[16,7502300048,"两点喷嘴式加渣嘴160","R1.07180.20.00-1","适用于圆坯Φ220、Φ250断面","件",8,"Q/ENGD001-2008","炼钢厂部","2022-05-29"]
[17,7502300049,"两点喷嘴式加渣嘴180","R1.07180.20.00-2","适用于圆坯Φ280、Φ330断面","件",8,"Q/ENGD001-2008","炼钢厂部","2022-05-29"]
[18,5602100009,"补偿器DN125","B227G35-13","9.5Kg","件",2,"审核图纸","炼钢厂部","2022-05-29"]
[19,7501300083,"轴向内压式波纹补偿器","16CNY125X9F","配不锈钢法兰及连接密封件","只",2,"GB/T9115.1","炼钢厂部","2022-05-29"]
[20,7501300084,"轴向内压式波纹补偿器","16CNY150X9F","配不锈钢法兰及连接密封件","只",1,"GB/T9115.1","炼钢厂部","2022-05-29"]
[21,6600400248,"温湿度控制器","DWS-ZZDX-7","电源AC85/265V，50/60Hz,功率4W,工作温度0~50℃，2路加热输出负载500Ω，尺寸长112mm*宽54mm*高120mm","台",10,"JB/T 6862-1993","能源厂部","2022-05-29"]
[22,7000700024,"水压机泵组","主泵T7DS-E35-1R03-A1 2台,带主泵电机及元器件","泵组参数Q=190L/min;n=1700r/min;p=18MPa;主泵电机1SMG2-68D17CD-R1A1FA 68KW;元器件型号及数量审核图纸,图号PT219.70HL","组",1,"审核图纸","180厂部","2022-05-29"]
[23,5705000001,"罗茨鼓风机(真空泵)","RRF-250V","风量79.2m3/min","台",1,"JB/T10563-2006","180厂部","2022-06-13"]
[24,5501700061,"皮带机缓冲床","JHYHCC1012，B1000*1200","缓冲条材质为超高分子量聚乙烯，可单独拆卸；缓冲条总面积不小于1.2m2,厚度不小于70mm；缓冲支座抗冲击强度不小于100Kgf/cm2；总重约1吨","套",1,"审核图纸","原料工段","2022-05-29"]
[25,5501700071,"双向可逆皮带机JHY免维护校正器（返式）","JHYJZP1000BD-B  带宽1000，长1480×宽350×高420","露天双向可逆，；包胶花纹主辊D180×1040，主托辊辊面衬胶采用复合聚氨脂材料，具有防冻、防滑、防脱落及耐磨性能，且满足当地气候温度，托辊具有防尘、防水，动作灵敏可靠，无噪音，调偏幅度大，不损伤皮带，表面胶层硬度不得低于60～70°(邵氏A型硬度)，质保期三年，质保期内无需更换任何配件。","套",10,"ZL202020201838.8","原料工段","2022-05-29"]
[26,5501700072,"双向可逆皮带机JHY免维护校正器","JHYJZP1000AD-B   带宽1000，长1370×宽270×高267","露天双向可逆，包胶花纹主辊D159/d133×375，主托辊辊面衬胶采用复合聚氨脂材料，具有防冻、防滑、防脱落及耐磨性能，且满足当地气候温度，托辊具有防尘、防水，动作灵敏可靠，无噪音，调偏幅度大，不损伤皮带，表面胶层硬度不得低于60～70°(邵氏A型硬度)，质保期三年，质保期内无需更换任何配件。","套",4,"ZL202020201838.8","原料工段","2022-05-29"]
[27,5100300069,"电力机车液压块式制动架","YWL-250/E30","制动力矩：380， 重量：61kg","套",1,"JB/T6406-2006","高炉","2022-05-29"]
[28,7501300089,"非金属补偿器","φ1250，L=200","设计压力0.1MPa；温度不超过100℃；工作介质：空气；含密封件","套",1,"CJ/T3016.2-1994","高炉","2022-05-29"]
[29,7501300090,"非金属补偿器","长980*宽860，L=210，含密封件","设计压力0.1MPa；温度不超过100℃；工作介质：空气，","套",1,"CJ/T3016.2-1994","高炉","2022-05-29"]
[30,5500500030,"消声器","GF-20a排气型","介质：高温压空;适用压力：≤1.0MPa(A);适用流量：2900Nm3/min;使用温度：≤300℃;平均消声量：≥25dB(A);连接方式：法兰螺栓联接;材质：Q345R,冷轧镀锌孔板，耐温防潮超细玻璃棉;接口尺寸：DN1200;消声器支座按安装条件设计制作，现场焊接","台",1,"审核图纸","高辅工段","2022-05-29"]
[31,7502000201,"离心水泵叶轮","水泵型号：SBL200-400（I）B","水泵流量346m3/h，扬程38m,叶轮内径：50mm，外径350mm","件",2,"GB/7-5657-1995","能源厂部","2022-05-27"]
[32,7001200295,"五柱塞往复泵;填料环乙","5XND-315-0212-D","材质：聚四氟乙烯;原装厂家：成都西南水泵厂","件",10,"GB/T5015-2003","89油管热处理","2022-05-29"]
[33,5300800014,"全电动堆高车CDDP","CDDP    承载1.5吨，升高高度1.6米，货叉最低85mm,货叉长度1150mm","承载1.5吨，升高高度1.6米，货叉最低85mm,货叉长度1150mm","台",1,"GB/T 26949.4-2016","物流中心","2022-05-29"]
[34,5701800031,"主机升降机：SWL 5 M-1 A-II-160","主机升降机：SWL 5 M-1 A-II-160","主机升降机：SWL 5 M-1 A-II-160","套",2,"GB/T10054-2005","89包装","2022-05-29"]
[35,5701300154,"联轴器","TL5","成品  8.38Kg","套",15,"JB/ZQ4729-2006","89油管热处理","2022-05-29"]
[36,5700900276,"易格斯拖链","E4.42.12.100.0*113节（42*125*R100，节距67mm，含接头、分隔片）","成品","套",2,null,"89油管热处理","2022-05-29"]
[37,null,"铁屑撕碎机","见技术规格书",null,"台",1,null,"管加工厂铁屑撕碎机项目","2022-05-29"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2022年4月机械配件采购项目            项目编号：HGCGD22037"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":4,"n_cols":1,"rows_kept":4,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8]],"flags":["formulas_cached_only"]}
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]