{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":45,"n_cols":11,"rows_kept":45,"merged":[[0,0,0,10],[1,0,1,10],[41,0,41,10],[42,0,42,10],[43,0,43,10],[44,0,44,10]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2022年4月液压缸采购项目                             项目编号：HGCGD22040"]
["序号","资材编号","资材名称","规格型号","技术参数","单位","数量","使用部门","交货时间","含税单价","生产厂家\n（品牌）"]
[1,5722600045,"带锯机夹紧油缸","G4240/60",null,"台",1,"180厂部","2022-06-30"]
[2,7200600237,"快开油缸","KZ1810.02.01.01.00","缸径Φ280,杆径Φ140, 工作压力25MPa,试验压力25MPa 工作环境温度-20℃~70℃，厂家：太原科达重工成套设备有限公司","套",1,"89油管热处理","2022-06-30"]
[3,7200600238,"快开油缸","KZ1810.02.03.01.00","工作压力32MPa,试验压力25MPa 工作环境温度-20℃~70℃，厂家：太原科达重工成套设备有限公司","套",1,"89油管热处理","2022-06-30"]
[4,7200100410,"宽辊道挡管器油缸","液压缸;CD250F80/56-200A10/01CADMA","缸径80，杆径56，行程200，压力等级25MPA","台",1,"219厂部","2022-06-30"]
[5,7201300032,"水平夹液压缸活塞杆","HM-CG63/36-650-3",null,"件",20,"340热轧","2022-07-30"]
[6,7201300031,"水平夹液压缸6活塞杆2","HM-CG63/36-650-2",null,"件",20,"340热轧","2022-07-30"]
[7,7201300030,"水平夹液压缸活塞杆1","HM-CG63/36-650-1",null,"件",20,"340热轧","2022-07-30"]
[8,7200600061,"锁紧液压缸装置","135/60-15,SG0977",null,"台",3,"720厂部","2022-08-30"]
[9,7502000050,"液压缸耳环","GAK28",null,"件",12,"管加工厂部","2022-07-30"]
[10,7502000054,"液压缸耳环","GAK58",null,"套",6,"340热轧","2022-07-30"]
[11,7200500016,"炉顶上下密液压缸","80*56-340","带耳环，密封材质：尼龙夹布V组，工作压力25MPa","台",1,"高炉","2022-08-30"]
[12,7200200013,"液压缸","02690005DR5003ME005-33","CD250E120/90-450A10/01CGDMA","台",2,"180厂部","2022-08-30"]
[13,7200200015,"液压缸","02690005DR5003ME014-22","CD250E125/90-700A10/01CGDMA L10=620 带GAK58耳环 额定压力25MPa","台",1,"180厂部","2022-08-30"]
[14,7200400033,"液压缸","YG80/45*200-S",null,"台",8,"管加工厂部","2022-08-30"]
[15,5720300004,"液压缸","YG100/55*600-S","带耳环；压力21MPa","个",2,"管加工厂部","2022-07-30"]
[16,7200600097,"液压缸","HYZ041-45 63/40-30","缸径Φ63,杆径Φ40,行程30 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",2,"340热轧","2022-08-30"]
[17,7200600099,"液压缸","HYZ138-45 160/140-450","缸径Φ160,杆径Φ140,行程450 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"340热轧","2022-08-30"]
[18,7200600239,"导板平衡液压缸","PBID4000G;50/32-99.5","压力等级：25MPa；采用进口密封","台",2,"89热轧","2022-06-11"]
[19,7200600153,"液压缸","PBID3000G;160/40-10","45钢，40kg","台",2,"89热轧","2022-08-30"]
[20,7200400038,"液压缸","HM28J000","63/36-710","台",2,"89热轧","2022-08-30"]
[21,7200100010,"液压缸","CD160B125/56-280+GAS40",null,"台",2,"720厂部","2022-08-30"]
[22,7200100173,"液压缸","SDH2MF3/100/63/460A1XM1CHDA",null,"台",1,"720厂部","2022-08-30"]
[23,7200400086,"液压缸","CD250E100/56-600A10/01CADMA;","L10=365;带耳环GAS50","台",1,"管加工厂部","2022-06-30"]
[24,5709700290,"液压缸","268.01SB0057-23",null,"台",1,"340热轧","2022-07-30"]
[25,7200100016,"液压缸","CD250A100/70-180A10/02CADMA+GAS50","缸径Φ100,杆径Φ70,行程180 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞采用PG型组合密封 活塞杆采用RS+USH型组合密封","台",3,"340热轧","2022-08-30"]
[26,7200100120,"液压缸","CD250E80/56-725A10/02CADMA+GAS40","缸径Φ80,杆径Φ56,行程725 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"340热轧","2022-08-30"]
[27,7200100093,"液压缸","CD250E125/70-385A10/02CADMA+GAS60 L10=429.5","缸径Φ125,杆径Φ70,行程385 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"管加工厂部","2022-08-30"]
[28,7200100418,"导板摆出液压缸","CD250B125/90-600A10/01CADMA","缸径Φ125,杆径Φ90,行程600 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",2,"89热轧","2022-06-30"]
[29,7200400052,"液压缸","CD210B63/45-600Z10/13HEUM2-2A",null,"台",2,"89热轧","2022-08-30"]
[30,7200100417,"横梁平移液压缸","C250E63/45-600A10/01CGDMA","压力等级：25MPa；采用进口密封；连接螺栓12.9级；L10=250","台",2,"89热轧","2022-06-30"]
[31,7200100263,"液压缸","CD250B50/28-250A10/02CGDMA+GAK22","缸径Φ50,杆径Φ28,行程250 ,工作压力25MPa 活塞及活塞杆采用V型组合密封，带球铰耳环","台",2,"89油管热处理","2022-06-30"]
[32,7200400090,"液压缸","CD250A/63/36-450A10/02CGDMA(左侧油口M27*2）,","带球铰耳环","台",4,"管加工厂部","2022-06-30"]
[33,7200100338,"液压缸","CD250E125/90-1250A10/02-CADMA+GAS60,L10=1184.6","缸径Φ125,杆径Φ90,行程1250. 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"340热轧","2022-06-30"]
[34,7200100340,"液压缸","CD250E160/110-1000A10/02-CGDMA+GAK80,L10=792.5","缸径Φ160,杆径Φ110,行程1000 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"340热轧","2022-06-30"]
[35,7200100346,"液压缸","02680014DR5005ME035-41","按CD250B50/36-235A10/01CADMA标准制造，带防尘罩","台",1,"89热轧","2022-06-30"]
[36,7200600221,"120/45 通用液压油缸","油缸LC89501Z","缸径φ63，杆径φ45，行程500，带防尘套，上下油口","件",10,"物流中心","2022-06-30"]
[37,7200100291,"液压缸","02680014DR5005ME017-4","CD250E63/45-185A10/01CADMA;L10=255","台",2,"89热轧","2022-06-30"]
[38,7200400102,"矫直机平衡液压缸","KZ1810.02.01.02.00(包括拉杆和夹壳联轴器）","缸径Φ100,杆径Φ50,带拉杆和夹壳联轴器，工作环境温度-20℃~70℃ 工作压力15MPa,试验压力25MPa ,重量：124.748Kg,指定厂家：太原科达成套设备有限公司","套",2,"89油管热处理","2022-06-30"]
["注：1、投标报价含税，税率13% ；                                                                                                                          2、生产厂家要求全称填写准确无误 ；                                                                                                                     3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2022年4月液压缸采购项目                             项目编号：HGCGD22040"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]