{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":19,"n_cols":13,"rows_kept":19,"merged":[[0,0,0,12],[1,0,1,12],[15,0,15,8],[16,0,16,8],[17,0,17,8],[18,0,18,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2022年5月电磁备件采购项目                     项目编号：HGCGD22056"]
["标包号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,4100400044,"电缆卷筒","JTA20-25-9-Ⅱ","容量20A 电缆长度25米9通道 外置滑环","台",1,"JT/T806.4-2011","炼钢厂部","2022-05-27"]
[2,5300800011,"稀土永磁除铁器","YC12-110130-X","皮带宽度B=1000mm；驱动电机功率4KW,自重2100kg；标准架设高度300mm","台",1,"GB/T4307-2005","原料工段","2022-05-27"]
[3,6000400036,"高温高频电磁吸盘","MW929-26080L/GW-75","工作频率75% 被吸物温度200℃","台",2,"JT/T806.4-2011","管加工厂部","2022-06-13"]
[4,6000300125,"气管卷筒","QJDF-50F/20","带力矩电机及减速机","台",1,"JT/T806.4-2011","炼钢厂部","2022-05-27"]
[5,6400100042,"金属探测器","JTC5-1000","1.检测物料为铁磁性矿粉、烧结矿、焦炭等物质，安装在皮带下料斗处。               2、探测线圈尺寸为：1000*575*200.             3、金属探测控制器1台，含控制板1块，参数设置遥控器1台。供电电压为220V，故障输出点2副，动作输出点2副。      3、金属探测器灵敏度范围0~200，可根据现场物料进行调整。 4、控制箱及探测线圈防水等级IP65 。5、带机旁自锁控制箱。","台",5,"Q/SHL01-2016","原料工段","2022-05-27"]
[6,5300100523,"吸盘链条","7.5t+7.5t","1.1米/根","根",16,"GB5802-1986","炼钢厂部","2022-06-11"]
[7,5300100524,"吸盘链条","MW5-210",null,"付",2,"GB54a-1977","炼钢厂部","2022-06-11"]
[8,5300100525,"吸盘链条","MW5-250200",null,"付",2,"GB54a-1977","炼钢厂部","2022-06-11"]
[9,4100400042,"电缆卷筒","JTA100-25-2-Ⅱ","容量100A 电缆长度25米2通道 外置滑环","台",1,"JT/T806.4-2011","180厂部","2022-07-11"]
[10,5300100249,"电缆卷筒","JTA170-15-2Ⅱ",null,"台",1,"JT/T806.4-2011","物流中心","2022-06-13"]
[11,6300500263,"智能充电电路板","GDCD-2017；输入电压DC24，自动充电，抗干扰、抗静电","适合在在恶劣环境中使用，具有智能强充、浮充，更好地保护电池，延长电池寿命。","块",1,"GB/T3235-1999","管加工厂部","2022-06-26"]
[12,6300400089,"智能充电模块","\"MQZL-80Q-S；内嵌智能控制板，控制电压正负12V,主回路输入电压AC三相380V，","输出电压DC0-240V可调,与充电电路板配合，能自动检测输入电压，移相调整三相电，保持三相输入电呈正形波,适合在恶劣环境中使用。\n输出电压：+12V电源：12±0.5V ，纹波电压小于20mv 。  -12V电源：-12±0.5V ，纹波电压小于20mv\n输出电流：标称电流小于80安培产品：I+12V＞0.5A，I-12V＞0.1A\n正反向峰值耐压：≥1400V；di／dt：100A／μs；dv／dt：500V／μs\"","只",2,"IEC61508","管加工厂部","2022-06-26"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2022年5月电磁备件招标采购项目      项目编号：HGCGD22056"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}