{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":20,"n_cols":11,"rows_kept":20,"merged":[[0,0,0,10],[1,0,1,10],[16,0,16,10],[17,0,17,10],[18,0,18,10],[19,0,19,10]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2022年6月液压备件采购项目                            项目编号：HGCGD22068"]
["序号","资材编号","资材名称","规格型号","技术参数","单位","数量","使用部门","交货时间","含税单价\n(元）","生产厂家\n（品牌）"]
[1,7000200050,"叶片泵","1PV2V4-2X/50RA01MC1-16A1","品牌：WERDOHLER","台",1,"89热轧","2022-07-30"]
[2,7000500016,"手动液压装卸车","CTYB-2000",null,"台",1,"89热轧","2022-07-30"]
[3,7200700007,"液压马达","JMDG16Y-3000BD40-R",null,"台",2,"219厂部","2022-08-30"]
[4,7000300023,"人字齿轮泵","RCB160 逆时针",null,"台",1,"340热轧","2022-07-30"]
[5,7000300024,"人字齿轮泵","RCB160 顺时针",null,"台",1,"340热轧","2022-07-30"]
[6,7000200060,"螺杆泵组","HSG940*2-42TQ/YB180L-4","压力1.0MPa；流量740L/min，介质46#汽轮机油；带电机，电机型号YB180L-4","台",1,"高辅工段","2022-07-30"]
[7,7502000202,"液压拉伸器","GT110,110542","额定工作压力1500Bar;行程15mm配行程指示器;双油口可快速连接多个工具;支撑组件一体式整体设计可拆卸并可以旋转;带防滑把手","件",1,"炼钢厂部","2022-08-30"]
[8,7502000204,"拉伸器电动液压泵站","ZUTP1500E","\"泵站工作电源220V/50hz;电机功率1.25Kw;额定工作压力1500Bar;压力表量程2000Bar;双级泵设计能在低压下为快速充油提供高流量并且在高压下控制流量以达到安全、准确运行的效果;Z系列高效泵使用散热器和低电流设计;6米拖线控制器能允许远程控制;带有聚碳酸酯外壳的倾斜放置的153mm压力表安装在保护性\n金属护罩内;安全的溢流阀控制输出压力;配一条原装进口油管（含与泵站和拉伸器连接的快速接头）;铝制结构                                                \"","台",1,"炼钢厂部","2022-08-30"]
[9,7501100529,"冷却水快速接头","HY340KOO","不锈钢","套",5,"340热轧","2022-08-30"]
[10,7500400074,"高压过滤器","DF ON 1320 T L 5 D 2.X /-L24-B6","耐压为420bar;过滤精度为5μm;带目视/电气污染发讯器;最大流量为680L/min;连接螺纹SAE DN50；滤材与抗燃液相容:带滤芯（1320D005ON;HYDAC）;带旁通阀","台",12,"炼钢厂部急件","2022-06-30"]
[11,7500400075,"高压过滤器","DF ON 280 TJ5D1.X/-L24-B6","耐压为420bar;过滤精度为5μm;带目视/电气污染发讯器;最大流量为360L/min;连接螺纹SAE DN32；滤材与抗燃液相容；带滤芯（0280D005ON;HYDAC）;带旁通阀","台",6,"炼钢厂部急件","2022-06-30"]
[12,7500500231,"高压过滤器滤芯","1320D005ON","过滤精度5μm;滤芯材质BN4HC","只",36,"炼钢厂部急件","2022-06-30"]
[13,7500500232,"高压过滤器滤芯","0280D005ON","过滤精度5μm;滤芯材质BN4HC","只",24,"炼钢厂部急件","2022-06-24"]
["注：1、投标报价含税，税率13% ；                                                                                                                          2、生产厂家要求全称填写准确无误 ；                                                                                                                     3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2022年6月液压备件采购项目                       项目编号：HGCGD22068"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]