{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":77,"n_cols":11,"rows_kept":77,"merged":[[0,0,0,10],[1,0,1,10],[73,0,73,10],[74,0,74,10],[75,0,75,10],[76,0,76,10]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2022年6月液压缸采购项目                             项目编号：HGCGD22074"]
["序号","资材编号","资材名称","规格型号","技术参数","单位","数量","使用部门","交货时间","含税单价","生产厂家\n（品牌）"]
[1,7200600209,"液压缸(三)","02680014DR5005ME013-35","20Kg；其它参数见图纸上的技术要求","件",6,"89热轧","2022-07-30"]
[2,7200100296,"液压缸","02680014DR5005ME044-20","CD250B100/56-170A10/01CGDMA","台",2,"89热轧","2022-07-30"]
[3,7200400066,"液压缸","HY89G48-680E",null,"台",2,"89油管热处理","2022-10-30"]
[4,7200100182,"液压缸","WG02CG250B180/125-950A10/02.1HGDC 带传感器","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",2,"219厂部","2022-10-30"]
[5,7200100170,"液压缸","HYDRAULTC CYLINDER SF601915","额定压力25MPa JB/T 5000","台",4,"180厂部","2022-10-30"]
[6,7200200001,"摆动液压缸","02690005DR5003ME016-29","UBJZ125-180H","台",1,"180厂部","2022-10-30"]
[7,7200200020,"液压缸","02690005DR5004ME019-48","22.6Kg","台",2,"180厂部","2022-10-30"]
[8,7200500025,"液压缸","0107119-37.001","额定压力25MPa JB/T 5000","台",4,"180厂部","2022-10-30"]
[9,7200300009,"液压小仓","0109034-31.000","270/220-130，额定压力300bar","台",1,"180厂部","2022-12-30"]
[10,7200100172,"液压缸","HYZ021845","80/56-15 额定压力25MPa JB/T 5000","台",2,"180厂部","2022-10-30"]
[11,7200600027,"滑动水口(二)液压缸","100-50-170 S-100-170-R1-F1","进口密封 缸径Φ100,杆径Φ50,行程170 工作环境温度-20℃~120℃ 工作压力20MPa,试验压力30MPa 活塞及活塞杆采用V型组合耐高温密封 工作介质水乙二醇液压油","台",2,"炼钢厂部","2022-10-30"]
[12,7200600043,"流切装置液压缸","63/28-200","12Kg","台",4,"炼钢厂部","2022-10-30"]
[13,7200600011,"摆动液压缸","50/36-740","缸径Φ50,杆径Φ36,行程740 工作环境温度-20℃~140℃ 工作压力20MPa,试验压力25MPa 活塞及活塞杆采用V型组合耐高温密封 韶关液压件厂 工作介质水乙二醇液压油","台",3,"炼钢厂部","2022-10-30"]
[14,7200400025,"液压缸","CD250B50/28-325A10/02CGDMA","06.457-6","台",7,"管加工厂部","2022-10-30"]
[15,7200200036,"液压缸","02690005DR5006ME043-79","CD250E100/56-350A10/01CADMA L10=380 额定压力25MPa JB/T 5000","台",3,"管加工厂部","2022-10-30"]
[16,7200100279,"液压缸","CDH2MT4/80/56-1250A1X/B1CFDMWW,XV=320正负40调节，带耳环CGKD50","缸径Φ80,杆径Φ56,行程1250 ,中轴式，工作压力25MPa，带球铰耳环","台",2,"管加工厂部","2022-08-30"]
[17,7200200072,"液压缸","BG-D-K-F80-388度-Y",null,"台",1,"管加工厂部","2022-10-30"]
[18,7200500002,"槽下液压缸","直径100*70-350","带耳环，密封材质：聚氨酯+丁晴橡胶，工作压力25MPa","台",2,"高辅工段","2022-10-30"]
[19,7200100115,"液压缸","CD250E63/45-1500A10/01CADMA+GAS35",null,"台",3,"720厂部","2022-10-30"]
[20,7200100140,"液压缸","CDH1MP5/50/36/705.0A11B1CSDBWW 活塞杆与耳环整体制作",null,"台",5,"720厂部","2022-10-30"]
[21,7200600094,"液压缸","HG-MFL-2500.063.206-1-4# 63/36-150","缸径Φ63,杆径Φ36,行程150 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞杆采用V型组合密封 活塞密封采用格莱圈","台",1,"340热轧","2022-10-30"]
[22,7200100337,"液压缸","CD250E160/110-800A10/02-CGDMA+GAK80,L10=773","缸径Φ160,杆径Φ110,行程800 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"340热轧","2022-08-30"]
[23,7200100339,"液压缸","CD250E160/110-942A10/02-CGDMA+GAK80,L10=850.5","缸径Φ160,杆径Φ110,行程942工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"340热轧","2022-08-30"]
[24,7200200066,"液压缸","Z0745.05.02.04","额定压力25MPa JB/T 5000","台",2,"180厂部","2022-10-30"]
[25,7200100174,"液压缸","SF600179","额定压力25MPa JB/T 5000","台",5,"180厂部","2022-10-30"]
[26,7201100080,"油缸","45HL-03","额定压力25MPa;缸径140;活塞杆100;行程320","台",1,"炼钢厂部","2022-07-30"]
[27,7200100401,"液压缸","CDH1MT4/160/110/280A1X/D1CSMAW    XV=500","图号：42C10101DL10436-14;压力等级：25MPa 采用德国MERKEL密封 连接螺栓12.9级","台",1,"管加工厂部","2022-08-30"]
[28,7200100402,"液压缸","CDH1MT4/200/140/280A1X/D1CSMAW    XV=485","图号：42C10101DL10447-14；压力等级：25MPa 采用德国MERKEL密封 连接螺栓12.9级","台",1,"管加工厂部","2022-08-30"]
[29,7200100403,"液压缸","CDH1MP5/200/140/680A1X/D1CSMAW","图号：42C10101DL10447-13；压力等级：25MPa 采用德国MERKEL密封 连接螺栓12.9级","台",1,"管加工厂部","2022-08-30"]
[30,7200100404,"液压缸","CDH1MP5/160/110/680A1X/D1CSMAW","图号：42C10101DL10436-13；压力等级：25MPa 采用德国MERKEL密封 连接螺栓12.9级","台",1,"管加工厂部","2022-08-30"]
[31,7200100358,"液压缸","CD250E100/56-130A10/02CGDMT",null,"台",2,"管加工厂部","2022-08-30"]
[32,5700300538,"液压缸耳环;60","Z0726.02.01.25改01.02","45锻钢","件","3","89热轧","2022-08-11"]
[33,7200100030,"液压缸","CD250B100/70-160A10/02CGDMA+GAK45","缸径Φ100,杆径Φ70,行程160 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台","1","340热轧","2022-10-10"]
[34,7200100031,"液压缸","CD250B100/70-185A10/01.1CGDMA",null,"台","3","720厂部","2022-10-10"]
[35,7200100032,"液压缸","CD250B100/70-250A10/02CADMA","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台","2","89热轧","2022-10-10"]
[36,7200100065,"液压缸","CD250B80/56-160A10/02CADVA","缸径Φ80,杆径Φ56,行程600 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用氟橡胶密封","台","5","340热轧","2022-10-10"]
[37,7200100080,"液压缸","CD250E/200/140-380A10/01CGDMA+GAK110 L10=504",null,"台","2","720厂部","2022-10-10"]
[38,7200100104,"液压缸","CD250E140/100-900A10/02CGDMA+GAK65 L10=710","缸径Φ140,杆径Φ100,行程900 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台","1","340热轧","2022-10-10"]
[39,7200100120,"液压缸","CD250E80/56-725A10/02CADMA+GAS40","缸径Φ80,杆径Φ56,行程725 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台","2","340热轧","2022-10-10"]
[40,7200100124,"液压缸","CD250F63/36-100A10/02CADMA","缸径Φ63,杆径Φ36,行程100 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台","4","340热轧","2022-10-10"]
[41,7200100125,"液压缸","CD250F63/36-150A10/02CADMA","缸径Φ63,杆径Φ36,行程150 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台","2","340热轧","2022-10-10"]
[42,7200100213,"液压缸","CD250B100/70-280A10/02CGDMA",null,"台","2","管加工厂部","2022-10-10"]
[43,7200100214,"液压缸","CD250B125/90-120A10/011CADMAC02",null,"台","1","管加工厂部","2022-10-10"]
[44,7200100216,"液压缸","CD250A50/36-200A10/01CADMA",null,"台","3","管加工厂部","2022-10-10"]
[45,7200100282,"液压缸","CD250B80/56-345A10/02CADMA+GAS40","压力等级：25MPa 采用进口密封 连接螺栓12.9级;带球铰耳环","台","2","89油管热处理","2022-07-27"]
[46,7200100287,"液压缸","02680014DR5005ME035-22","CD250E50/36-90A10/01CADMA","台","2","89热轧","2022-07-27"]
[47,7200100327,"液压缸","CDH1MP5-100/70/200A1X/M2CGDA;","压力等级250，   带球铰耳环","台","2","管加工厂部","2022-08-26"]
[48,7200100348,"液压缸","19Q00803.4.1;","SDH2MT4/100/70/430A1XB1CFDMTC；XV=390mm；带耳环CGKD63；带防水型位移传感器RS-M0450-S1-DT05-A01；压力等级：25MPa 采用进口密封 连接螺栓12.9级","台","1","管加工厂部","2022-08-26"]
[49,7200200078,"液压缸","YG100/55-450",null,"台","3","管加工厂部","2022-10-10"]
[50,7200200086,"液压缸","PB65KSGWGG1125/90-1850双耳轴轴加粗为70","双耳轴轴加粗为70,缸体材料40Cr,原厂家韶关伟光","台","1","89热轧","2022-07-27"]
[51,7200400030,"液压缸","HY89G099-40B;63/36-40",null,"台","3","89热轧","2022-10-10"]
[52,7200400048,"液压缸","PBICJ000","63/45-140","台","2","89热轧","2022-10-10"]
[53,7200400053,"液压缸","CD250E100/56-340A10/011CADMAC02","06.46.3-3-4","台","3","管加工厂部","2022-10-10"]
[54,7200400058,"液压缸","PBA03CH00000;100/85-90",null,"台","3","340热轧","2022-10-10"]
[55,7200500039,"液压缸","HG180009,PT219.80HL-01.10.5-00","PT219.80HL-01.10.5-00 额定压力25MPa JB/T 5000","台","2","340热轧","2022-10-10"]
[56,7200500056,"大臂回转液压缸","D80/d56-1130",null,"台","1","炼钢厂部","2022-10-10"]
[57,7200600003,"EBT打开液压缸(水冷式)","90/50-135","进口密封 带水冷外壳,缸径Φ90,杆径Φ50,行程135 活塞及活塞杆采用耐高温V型组合密封 工作介质水乙二醇液压油","台","1","炼钢厂部","2022-10-10"]
[58,7200600008,"倾动锁定液压缸","HG-LG-2003 100/56-350","缸径Φ100,杆径Φ56,行程350 带缓冲 工作环境温度-20℃~100℃ 工作压力16MPa,试验压力25MPa 活塞及活塞杆采用V型组合耐高温密封 工作介质水乙二醇液压油","台","1","炼钢厂部","2022-10-10"]
[59,7200600135,"引锭杆存放液压缸","125/70-490","96Kg","台","2","炼钢厂部","2022-10-10"]
[60,7200600178,"液压缸","PBICE000;110/95-110","110/95-110；压力25MPa","台","2","89热轧","2022-10-10"]
[61,7200600196,"上辊快开机构液压缸;","SYZ8037.02.02.00;组件;2382Kg",null,"台","1","340热轧","2022-08-26"]
[62,7200600230,"G4225带锯床锯条张紧液压缸","YGZ63/30-80","缸径63， 活塞杆30， 行程80， 压力10MPa,   自带换向机构","台","1","管加工厂部","2022-08-26"]
[63,7201300027,"液压缸耳环","GAK100",null,"件","4","340热轧","2022-09-10"]
[64,7201300052,"液压缸活塞杆","直径180,行程1000",null,"件","2","720厂部","2022-08-11"]
[65,7501800015,"液压缸耳环","GAS50",null,"件","10","340热轧","2022-07-27"]
[66,7501800047,"液压缸耳环","GAK80","带80关节轴承","件","5","720厂部","2022-07-27"]
[67,7502000055,"液压缸耳环","GAK65",null,"件","8","340热轧","2022-09-10"]
[68,7502000061,"液压缸耳环","GAS70",null,"件",11,"720厂部、340热轧","2022-09-10"]
[69,7200400106,"夹紧油缸","WAW-600-JJ","外径80mm，内径60mm，行程60mm，适应WAW-600微机控制电液伺服万能试验机","件",2,"检验检测中心","2022-07-27"]
[70,7501100530,"夹紧油缸接头","WAW-600-JJT","长120mm，直径14mm，内外丝10*1mm，适应WAW-600微机控制电液伺服万能试验机","个",4,"检验检测中心","2022-07-27"]
["注：1、投标报价含税，税率13% ；                                                                                                                          2、生产厂家要求全称填写准确无误 ；                                                                                                                     3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2022年6月液压缸采购项目                             项目编号：HGCGD22074"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]