{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":34,"n_cols":10,"rows_kept":34,"merged":[[0,0,0,9],[1,0,1,9],[30,0,30,9],[31,0,31,9],[32,0,32,9],[33,0,33,9]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2022年6月-2023年5月灯具年度招标项目                                         项目编号：HGCGD22077"]
["序号","资材编号","资材名称","规格描述","技术参数","数量","单位","含税单价(元)","生产厂家\n","备注   "]
[1,"4000100006","LED泛光灯","NFK3613",null,291,"只"]
[2,"4000100008","LED路灯","LHD-L96WL04","96w 电源效率>90% 平均照度>28LUX",135,"只"]
[3,"4000100139","LED配电房专用灯","BD-A95;","30W;220-240V;斑点照明",780,"盏"]
[4,"4000100192","LED投光灯","200W/265V/3000K","黄色；防水",21,"个"]
[5,"4000100195","LED吸顶灯","CLX-BE36","功率36w；飞利浦芯片；光效≥130Lm/w、智能IC驱动；圆形；白光",25,"套"]
[6,4000100019,"厂房照明LED灯","100W","85~265VAC 色温2700K~6500K可选 寿命>50000h",204,"盏"]
[7,"4000100027","灯具","70W","LED,220V,70W,新曙光",354,"盏"]
[8,"4000100032","灯泡","NTC9210400W",",灯头螺口、E27、400W，海洋王、防振投光灯NTC9210",80,"只"]
[9,"4000100143","防爆灯","FGL-L-L150-B1-Z",null,11,"盏"]
[10,"4000100153","防爆平台灯","BPC8720 150W",null,31,"盏"]
[11,"4000100046","防尘高顶灯","NGC9810","NGC 9810 A250，220VAC，英制1/2内丝接口",180,"盏"]
[12,"4000100047","防眩泛光灯","NFC9180","150W",20,"盏"]
[13,"4000100051","防震型投光灯","NTK4021","NTK4021",112,"盏"]
[14,"4000100050","防震型投光灯","NTC9210A-N250","250W 220VAC 支架安装",80,"盏"]
[15,"4000100059","工作灯","FW6580","海洋王,LED防爆泛光灯000.1-2007,LED防爆泛光灯、海洋王",4,"盏"]
[16,"4000100061","固态免维护防爆灯","BFC8183","220V",36,"盏"]
[17,"4000100150","固态强光防爆头灯","*",null,62,"盏"]
[18,"4000100066","机床照明灯","FX-JCF20","20W AC85V-220V 防护等级IP65",6,"盏"]
[19,"4000100163","集成吊顶平板led灯","尺寸600*600；雷士","电压220VAC;功率48W;单驱动；铝合金型材拉丝边框",47,"盏"]
[20,"4000100093","平面节能灯泡","SL85-4U.C","220V 0.39A,节能灯、85W 220V 0.39A、苏州圣路 SL85-4U.C",80,"只"]
[21,"4000100197","软管射灯","220V 10W；15度~45度聚光；明装型；黑壳白光","15度~45度聚光；明装型；220V 10W；黑壳白光",28,"件"]
[22,"4000100110","手提式防爆探照灯","RJW7102","内置电池，可充电型",7,"盏"]
[23,"4000100138","探伤机;大面积悬挂式LED探伤灯","LD7545-3K;辐照度>3000μW/cm？;750*450mm",null,4,"盏"]
[24,"6400500313","探伤机;手提式荧光灯","LED鹰60",null,10,"盏"]
[25,"4000100120","微型防爆头灯","IW5130","LED头灯、海洋王",82,"盏"]
[26,"4000100176","一体式LED太阳能路灯","SL-TX-0050hy","灯光通量24001m;色温5700K;光衰1万小时<5%;光效160lm/w;IP66;灯具材质:高端铝合金、电池:3.2v、50Ah,锂电池;控制方式:光控、分时段调光智能控制",8,"套"]
[]
["注：1、投标报价含税，税率13% ；2、生产厂家要求全称填写准确无误 ；                                                                                          3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2022年6月-2023年5月灯具年度招标项目                        项目编号：HGCGD22077"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}