{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":37,"n_cols":13,"rows_kept":37,"merged":[[0,0,0,12],[1,0,1,12],[33,0,33,12],[34,0,34,9],[35,0,35,9],[36,0,36,9]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2022年7月电气备件采购项目                    项目编号：HGCGD22091"]
["序号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,6000400020,"合闸电磁铁","220VDC 205Ω",null,"GB14048.4-93","只",10,"炼钢厂部","2022-08-11"]
[2,6400400007,"增量编码器","DGS60-G4B04096 德国IEC947","电源电压DC10-30V，脉冲数1024个/圈","德国IEC947","只",1,"炼钢厂部","2022-08-11"]
[3,6400100016,"热探转换器","BTE-FMD85","24VDC/1.5W 序列号2188014F BLOCK","GB/T 18901.1-2002","个",3,"720厂部","2022-08-11"]
[4,6400600441,"凸轮开关","TKE4-0-T/201-B/RMF5","电压10-30V；电流200mA；海光机械电器厂","GB/T 1408.10-1999","台",2,"180厂部","2022-08-11"]
[5,6400300235,"接近开关","NJ1,5-8GM-N-Y18488","开关功能: 常闭 (NC), 输出类型: NAMUR, 安装: 齐平, 输出类型: 2 线, 螺纹模具: M8, 结构类型: 圆柱形，螺纹, 系列: 圆柱形; 防护等级: IP67, 材料: PUR.","GB/T14048.10-2008","只",10,"管加工厂部","2022-08-11"]
[6,4100500397,"转换开关","LW39-16A-3KC-11111/3","5档","GB/T 8946-2013","个",4,"炼钢厂部","2022-08-11"]
[7,6400300236,"限位开关","1LS19-J","3A-240VAC AC15,0.4A-30VDC DC-12","JB/T5553-2006","个",5,"炼钢厂部","2022-08-11"]
[8,4100600062,"声光报警灯","LTE-6101J","电压:AC36V   颜色:红色","GB/T14048","只",5,"180厂部","2022-08-11"]
[9,6300700061,"操作屏","smart700iev3(含程序及调试)","电压DC24V，RS422/RS485，USB","IEC61508","块",1,"高炉","2022-08-11"]
[10,6400400152,"增量型编码器","I58S/SJG001","供电5-30VDC 外壳直径58mm.安装厚度86mm,防护等级IP64，轴径10MM，脉冲数：:6000","EN61800-3","台",1,"高炉","2022-08-11"]
[11,7502500028,"轴流风机","150FZY2-S","65W","GB/T13933-2008","台",5,"219厂部","2022-08-11"]
[12,6600300166,"电动执行机构","M8430","电机功率：2KW,额定电流：3.5A，电源电压：380V/3PH 50HZ,防护等级：IP67，力矩250NM，行程/速度：36rpm","JB/T8219-1999","台",1,"能源厂部","2022-08-11"]
[13,6400600004,"温度控制器","ETS1701-100-000+TFP100+保护套",null,"ISO9001","只",2,"管加工厂部","2022-08-11"]
[14,6200300092,"中频感应加热器","ZP-300","输入三相380v,300Kw,工作频率8-10KHz,冷却水压力0.25MPA，25m3/h,工件直径60-300mm，壁厚10-80mm，加热时间1-5分钟，加热温度300-800度可调，并显示实际值，加热长度200mm.其它详情参照附件。","JB/T8669-1997","套",1,"219厂部","2022-08-11"]
[15,6400400153,"起重机无线防碰撞控制终端","WXFPZ-200A-KZZD","AC220V;功率50W;工作温度-25°-75°","GB/T3667.1-2006","台",1,"炼钢厂部","2022-08-11"]
[16,6400400154,"起重机无线防碰撞传感器","WXFPZ-200A-CGQ","AC220V;功率50W;工作温度-25°-75°","GB/T3667.1-2006","台",1,"炼钢厂部","2022-08-11"]
[17,6200100090,"变频器","CS710-4T30GB","30KW","EN61800-3","台",1,"高炉","2022-08-11"]
[18,6100900126,"操作台","720高速切管机操作台","720高切集控改造用操作台，一套包含主辅台各一个，包含柜体，柜面开关按钮，柜内模块等电气元件以及柜内接线，详细清单和接线见图纸","审核图纸","套",2,"720厂部","2022-08-11"]
[19,6200200863,"变频器","MD480T220P-L;带制动单元及电抗器、制动电阻、485通讯卡","变频器220KW、输入电压380V 额定电流426A 、尺寸：W*H*D 300*1424*500；MD系列变频器制动单元，380V制动单元-标准机；11KW制动电阻；485通讯卡MD38TX1，带隔离的modbus通讯适配卡。","EN61800-3","台",1,"180厂部","2022-08-27"]
[20,6300500240,"UPS","HTM6006-30M","容量6KVA：输入电压380VAC±25％输入频率50/60Hz±10%，输出电压：220VAC±1％输出频率50/60Hz±0.5，切换时间0ms，后备时间0.5小时。主机内置输入输出隔离变压器，采用三旁路模式（静态、维修、应急）",null,"套",1,"烧结","2022-08-07"]
[21,6400300239,"传感器","1442-PR-0830M0510N","NCPU, 8mm Probe,Reverse Mount, Metric, 30mm, 1.0m cable  AB","JB/T11279-2012","个",5,"高炉","2022-07-28"]
[22,4100700191,"高压包","DP-GC","尺寸70mm*45mm*30mm;输入电压DC24V;输出电压10KV~20KV(跟随输入电压变化);电弧距离1.5cm;电弧特性;白色;脉冲;可燃气点火;不可点燃纸","GB/T 1.1-2009","只",10,"炼钢厂部","2022-08-12"]
[23,5300100969,"天车超重限载器套件","QCX-M-5t+5t（带双传感器及8寸大屏显示器）","带2个5t传感器及8寸显示屏；","GB14048","套",2,"89油管车丝委外","2022-09-26"]
[24,5300300860,"工业高温蒸汽洁机","TN1C2-1647942432194","交流220伏","JB/T2785-2010","台",1,"物流中心","2022-07-28"]
[25,5300700016,"铁水车加盖：地面控制柜","LC8921-II/型","交流380伏","JB/T2785-2010","个",3,"物流中心","2022-07-28"]
[26,6100700019,"电压互感器","JZWXF-35","35/√3/0.1/√3/0.1/√3/0.1/3kV, ?0.2/0.5/3P ,环氧树脂浇注干式","GB20840.3-2013","台",6,"能源厂部","2022-08-27"]
[27,6300600078,"喷码机主控板","PMC-PJ1A","IC4-2216-J主控板","IEC61509","块",1,"89油管车丝委外","2022-08-27"]
[28,6400100043,"热金属检测器","HMD4-4ZC1","电源DC24V，输出24VDC高电平，负载能力>100mA，响应时间 接点＜20ms 电平与隔离＜2ms，检测温度550℃～1400℃，检测距离0.2m～8m，外壳形式 带冷却，功耗≤5W，保护  直流输入极性保护，电平输出短路及过载保护，带红光瞄准，灵敏度可调节，有电源及信号工作指示，可自检",null,"台",2,"219厂部","2022-08-27"]
[29,6400600499,"压力传感器","HDA4840A0350-424，HYDAC","量程350bar,输出型号两线制4-20mA,带6米线,防护等级IP68","GB/T15768-1995","只",5,"340热轧","2022-08-27"]
[30,6400600500,"红外光栅","ABI10-1388-8光束","探测距离10米，高度126厘米，宽度3.2厘米","GB/T27664.2-2010","对",2,"物流中心","2022-07-28"]
["注：1、投标报价含税，税率13%                      2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2022年7月电气备件采购项目        项目编号：HGCGD22091"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":4,"n_cols":1,"rows_kept":4,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8]],"flags":["formulas_cached_only"]}
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]