{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":30,"n_cols":11,"rows_kept":30,"merged":[[0,0,0,10],[1,0,1,10],[26,0,26,10],[27,0,27,10],[28,0,28,10],[29,0,29,10]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2022年7月液压备件等采购项目                            项目编号：HGCGD22099"]
["序号","资材编号","资材名称","规格型号","技术参数","单位","数量","使用部门","交货时间","含税单价\n(元）","生产厂家\n（品牌）"]
[1,7000100061,"定量泵","KD-A2F090/61R-PPB05","定量泵,斜盘結构,为工业用 排量90ml/r 61系列 顺时针旋转 带FPM轴封的丁晴橡胶密封 带键直轴DIN 6885 安装法兰ISO 4孔 工作油口连接B和S：SAE,公制固定螺钉 辅助泵， 工作介质HM-46#抗磨液压油","台",2,"管加工厂部","2022-09-26"]
[2,7100300006,"比例换向阀","4WRAE6W1-30-2X/G24K31/F1VZ31 DIN24 340 A型",null,"只",2,"高炉","2022-09-26"]
[3,7100300054,"电磁换向阀","4WE10J33/CG24N9K4","REXROTH","只",4,"340热轧","2023-01-09"]
[4,7100300041,"电磁换向阀","4WE10D33/CG24N9K4 DIN24 340 A型","ISO 4401","只",4,"340热轧","2022-09-26"]
[5,5000300101,"圆柱齿轮减速机;","QJRS-D450-63-1X-CA;i=63",null,"台",1,"炼钢厂部","2022-09-26"]
[6,7000300024,"人字齿轮泵","RCB160 顺时针",null,"台",1,"340热轧","2022-09-26"]
[7,7000300023,"人字齿轮泵","RCB160 逆时针",null,"台",1,"340热轧","2022-09-26"]
[8,7000700009,"油泵电机组","YB1叶片泵 6ml/R 6.3MPa 1450r/min 电机Y90S-4/1.1Kw",null,"台",3,"检验检测中心","2022-09-26"]
[9,7201100060,"二合一气缸","J60000","三个工作位；缸径125；","台",2,"180厂部","2022-09-26"]
[10,7200800046,"气缸","QSB80*600;","配单双悬耳","台",4,"管加工厂部","2022-10-26"]
[11,7100800046,"液压阀台订货图一","LH03407-01","按图纸要求；含阀块；液压阀；接头；闸阀；管道等。","套",1,"管加工厂部","2022-10-26"]
[12,7100800047,"液压阀台订货图二","LH03407-02","按图纸要求；含阀块；液压阀；接头；蓄能器；闸阀；管道等。","套",1,"管加工厂部","2022-10-26"]
[13,7400200025,"密封挡圈","F4-75*95*3","直径∮75*∮95*3    聚四氟乙烯","件",50,"管加工厂部","2022-09-26"]
[14,7100300432,"液压单向阀","SV10PA2-30B  压力31.5MPa,公称通径10mm",null,"个",2,"能源厂部","2022-09-26"]
[15,5700400756,"缓冲器","YF0171-4","成品；76.2kg","件",2,"89热轧","2022-09-26"]
[16,7402900067,"高压增压泵密封安装包","51398","Gas booster Haskel;14AGT-125/315-29125;Serial # 4762643-1;Air Cycling valve Seal Kit","包",1,"检验检测中心","2022-09-26"]
[17,7201300093,"摆动气缸","CDRA1BWU100-180",null,"台",2,"89热轧","2022-09-26"]
[18,4300500005,"宽皮带给料机皮带","KP-3205；3100*3205*15",null,"条",1,"烧结","2022-10-27"]
[19,7501300096,"筛下软连接","TTHBS-350-85-75","材质：帆线橡胶","套",4,"高辅工段","2022-10-27"]
[20,7501300097,"给料机-筛机软连接","TTHBS-350-85-80","材质：帆线橡胶","套",4,"高辅工段","2022-10-27"]
[21,7501300098,"闸门-给料机软连接","TTHBS-350-200","材质：进口橡胶","套",10,"高辅工段","2022-10-27"]
[22,7002000025,"液压同步拉伸泵组","TSD-4  M56","工作压力150MPa,M56，带分配阀，拉伸缸2台，螺母套，油管2米","套",2,"管加工厂部","2022-10-27"]
[23,"7000200058","螺杆泵","VKFBS440R46U8.6-W1;ALLWEILER AG","流量443-436 l/min；转速1450 l/min；额定压力15 bar；运动粘度3059-320 mm2/S；电机功率18-14.25 kW","台",1,"340热轧","2022-10-27"]
["注：1、投标报价含税，税率13% ；                                                                                                                          2、生产厂家要求全称填写准确无误 ；                                                                                                                     3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2022年7月液压备件等采购项目                       项目编号：HGCGD22099"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]