{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":47,"n_cols":13,"rows_kept":47,"merged":[[0,0,0,8],[1,0,1,12],[43,0,43,8],[44,0,44,8],[45,0,45,8],[46,0,46,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2022年7月阀门采购项目                     项目编号：HGCGD22102"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,6600300158,"智能陶瓷煤流调节阀","HMTJ-3000","工作方式：气动式，环境温度：-10℃～120℃；工况压力：0～1.6MPa，基本误差：1%；回差：1%；死区：2%，防护等级IP65","台",1,null,"高炉","2022-09-11"]
[2,7101600154,"电动金属硬密封蝶阀","D943H-2.5;","DN1600;Pg0.25MPa;温度≤300℃;高炉煤气","只",1,"JB/T8527-1997","能源厂部","2022-09-11"]
[3,7102000080,"旋启式止回阀","H44H-16C，DN50，PN1.6MPa","P=1.0MPa，DN50，使用环境：室内，品级：优级","只",2,"GB/T12233-2006","180厂部","2022-09-11"]
[4,7102000079,"低阻力倒流防止器","LHS743X，DN50,PN1.0MPa","P=1.0MPa，使用环境：室内，品级：优级","只",2,"GB/T2878-1993","180厂部","2022-09-11"]
[5,7102000078,"球型污水止回阀","HQ411.0C,DN50,PN1.0MPa","P=1.0MPa，DN50;使用环境：室内，品级：优级","只",2,"GB/T12221-2005","180厂部","2022-09-11"]
[6,6600300037,"煤气调节阀","LPB12-1D3B4DRC1-350P-16A","阀门口径 DN350 压力等级：ANSI150# 对夹式 流量特性：近似等百分比特性 行程90度 阀体WCB、阀板CF8M不锈钢、阀杆17-4PH不锈钢、阀座RPTFE：泄漏等级：ClassⅥ","只",1,"GB/T4213-2008","180厂部","2022-09-11"]
[7,7101800015,"不锈钢球阀","Q11F-25P-20","不锈钢手动球阀 内螺纹 浮动直通式 氟塑料 压力2.5mpa DN20","只",20,"GB/T 12230-2005","炼钢厂部","2022-09-11"]
[8,7101800023,"不锈钢球阀","Q11F-64P-40",null,"只",50,"GB/T 12230-2005","炼钢厂部","2022-09-11"]
[9,7101800121,"三片式不锈钢球阀","Q311F-25P-50","不锈钢手动球阀 浮动直通式 氟塑料 压力2.5mpa DN50","只",60,"GB/T12234","炼钢厂部","2022-09-11"]
[10,7101600102,"手动蝶阀","Z41H-16C","DN200","只",1,"GB/T12238-2008","340热轧","2022-09-11"]
[11,7101600050,"手动蝶阀","D343X-10","DN250","只",1,"GB/T3037-1994","高炉","2022-09-11"]
[12,5500800002,"电动金属硬密封耐磨蝶阀","DN600","铸钢 型号：防爆型 DN600 D943P-2.5 带电动装置 JB/T8527-1997 含硅胶密封条，耐温400℃ 启闭时间20S 金属垫600*670*10 电动装置型号 Z30-18B 电机功率 0.55KW 电压 380V 输出转矩 300N.m 输出转速 18r/min。","只",3,"JB/T18527-1997","高辅工段","2022-09-11"]
[13,5500800003,"电动扇型耐磨盲板阀","DN600","铸钢 型号 防爆型 F943X-2.5,工作压力0.25MPa,带电动装置,密封条材质氟橡胶246,工作温度-20℃-300℃;法兰JB/T8527-1997， 配2片金属缠绕垫600*670*10;电动装置型号 Z39-18B, 电机功率 0.5KW 电压 380V ,输出转矩 300N.m ,输出转速 18r/min,启闭时间20S；双层不锈钢金属波纹管材质为254SMo,厚度1.2mm*2;密封槽尺寸及电装联结结构尺寸需按技术规格书要求标准制造。","只",3,"JB/T18527-1997","高辅工段","2022-09-11"]
[14,5500800004,"电动卸灰耐磨球阀","DN300","铸钢 介质:高炉含尘埃气体，总长度？ 硬密封 全球阀 耐温≥250℃ 球体1Cr18Ni9Ti+硬铬,工作压力2.25MPa带电动装置 工作300℃，电动装置型号 Z32B 电机功率0.37KW 电压 380V 电流 1.38A 输出转矩 200N.m 输出转速18r/min。","只",2,"GB12221-1989","高辅工段","2022-09-11"]
[15,5501200074,"双层插板卸灰阀插板","DSXF-DN300;103","304不锈钢","件",10,null,"烧结","2022-09-11"]
[16,7102000040,"止回阀","H41H-16-80",null,"只",2,null,"89油管热处理","2022-09-11"]
[17,7100300433,"电磁球阀","AS22061a-G24","常闭，带应急按钮","个",2,"ISO4401","89热轧","2022-09-11"]
[18,7101800037,"二片式不锈钢球阀","Q211F-16P-DN20","压力1.6MPa DN20","只",30,"GB/T12237-2007","89热轧","2022-09-11"]
[19,7101600127,"双动气动球阀","V415X608DN50","PN16 密封PTFE","只",3,"GB12237-1989","219厂部","2022-09-11"]
[20,7101800207,"气动球阀","V634412","DN65;1.6MPa","台",3,"GB12224-1989","219厂部","2022-09-11"]
[21,7101800220,"双动气动球阀","D415H069","DN50;PN16;密封PTFE","只",3,"GB12237-1989","219厂部","2022-09-11"]
[22,7101800198,"双动气动球阀","D415H068","DN40 PN16 密封PTFE","只",2,"GB12237-1989","219厂部","2022-09-11"]
[23,7101800154,"高压球阀","KHM-G11/4-1112-01X",null,"件",2,"GB/T9065.2-2010","89油管热处理","2022-09-11"]
[24,7101600016,"对夹式手动蝶阀","D71X-16C","DN40","只",10,"GB/T12238","89油管热处理","2022-09-11"]
[25,7101600028,"气动蝶阀","VF-735DA-DN50","DN50","只",2,"GB/T3452.1-1992","89油管热处理","2022-09-11"]
[26,7102100009,"气动控制阀","Z014-A DN80 PN25",null,"只",8,"GB/T3452.1-1992","180厂部","2022-09-11"]
[27,7100100253,"弹簧式安全阀","A42H-16C-100","公称通径100mm；流道直径65mm；公称压力1.6Mpa;阀体材料WCB；整定压力0.95MPa；压力等级0.8－1.0MPa；回座压力0.808MPa；介质气体。","台",4,"GB/T12243-2005","180厂部","2022-09-11"]
[28,7101700015,"弹性座封闸阀","RVHX-16C-DN150 PN16 DN150","铸造 长度250mm 中心孔距220mm GB12220-1989","只",2,"GB/T 12230-2005","管加工厂部","2022-10-11"]
[29,7101900017,"不锈钢截止阀","J41H-25P-150 DN=150mm；",null,"只",1,"GB 8465.3-1987","高炉","2022-10-11"]
[30,5500800011,"气动卸灰耐磨硬密封球阀","QM647Y-1.6","DN150,双气缸 阀体WCB.球体1Cr18Ni9Ti+硬铬 1.6MPa 介质:高炉含尘埃 WCB QM647Y-1.6 双气缸 介质:高炉含尘埃,总长度390mm 硬密封 全球阀 耐温≥250℃ 球体1Cr18Ni9Ti+硬铬,工作压力1.6MPa","只",1,"GB12237-1989","高炉","2022-10-11"]
[31,5500800012,"蜗轮卸灰耐磨硬密封球阀","Q347AF-1.6","DN150 阀体WCB,球体1Cr18Ni9Ti+硬铬 1.6MPa 介质:高炉含尘埃气体 WCB Q347AF-1.61. 介质:高炉含尘埃气体，总长度390mm 硬密封 全球阀 耐温≥250℃ 球体1Cr18Ni9Ti+硬铬,工作压力1.6MPa","只",2,"GB/T12237","高炉","2022-10-11"]
[32,7102100008,"法兰式疏水阀","CS49H-25P-40",null,"只",1,null,"高辅工段","2022-10-11"]
[33,7101800130,"气动球阀","DN150 ANSI 300 ASMEB16.5","铸钢 F30，CLASS ANSI300，ASTMA216WCB，A351 CF8M，STAINLESS316，ANSI 300 ASMEB16.5","只",1,null,"高辅工段","2022-10-11"]
[34,5500800013,"星形卸灰阀","YXD-570","570*570 高度600 带电机 铸钢 GB16490-1996 工作温度450℃，介质：高炉瓦斯灰，壳体材质：Q235，叶轮材质：不锈钢，叶轮与壳体间隙30丝，轴密封采用石墨盘根，扎三圈，便于更换，带电机、减速机电动机型号 YKF2-100L1-4 电压 380V，电流 5.09 轴伸端轴承 6206-2RS 功率2.2KW 减速机型号 XLD4-2B","套",1,"GB16490-1996","高辅工段","2022-10-11"]
[35,5723400001,"不锈钢管端磁化液气动球阀","Q611F-16P DN25","DN25","件",4,"CB/T?4383-2016","管加工厂部","2022-10-26"]
[36,7100100157,"安全阀","A27H-10","DN20 1.0MPa","个",4,null,"180厂部","2022-10-11"]
[37,7100100005,"安全阀","A48Y-16C-80；压力等级1.0～1.3Mpa；整定压力1.0Mpa","铸造","只",3,"GB/T12243-2005","180厂部","2022-10-11"]
[38,7100100089,"减压阀","DR30-1-30/315YM","ISO 4401","只",2,"GB2514-1987","180厂部","2022-10-11"]
[39,7100100231,"安全阀","A48Y-16C-50","压力等级0.8-1.2Mpa；整定压力1Mpa","台",2,"GB/T12243-2005","180厂部","2022-09-11"]
[40,7102000081,"燃气止回阀","HF-G1A","内丝G1\";球头;介质:氧气","只",2,"GB13347-1992","炼钢厂部","2022-09-11"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2022年7月阀门采购项目           项目编号：HGCGD22102 "]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":4,"n_cols":1,"rows_kept":4,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8]],"flags":["formulas_cached_only"]}
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]