{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":87,"n_cols":13,"rows_kept":87,"merged":[[0,0,0,10],[1,0,1,10],[83,0,83,10],[84,0,84,10],[85,0,85,10],[86,0,86,10]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2022年8月液压缸采购项目                             项目编号：HGCGD22105"]
["序号","资材编号","资材名称","规格型号","技术参数","单位","数量","使用部门","交货时间","含税单价","生产厂家\n（品牌）"]
[1,7200100305,"挡板液压缸","CD250E63/45-300A10/02CADMA",null,"台",2,"89热轧","2022-10-27",null,null,"1115.045",2230.09]
[2,7200200086,"液压缸","PB65KSGWGG1125/90-1850双耳轴轴加粗为70","双耳轴轴加粗为70,缸体材料40Cr,原厂家韶关伟光","台",2,"89热轧","2022-10-27",null,null,"6690.27",13380.54]
[3,7201300093,"摆动气缸","CDRA1BWU100-180",null,"台",2,"89热轧","2022-10-27",null,null,"1000",2000]
[4,7200100424,"液压缸","PB6JG000;100/56-250","100/56-250","台",2,"89热轧","2022-10-27",null,null,"3400",6800]
[5,7200100041,"液压缸","CD250B125/90-340A10/02CADMA","JB/T 5000 额定压力25MPa","台",1,"219厂部","2022-11-10",null,null,"2699.12",2699.12]
[6,7200500051,"液压缸","Z0733.03.12.03.00","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",4,"219厂部","2022-11-10",null,null,"1185.84",4743.36]
[7,7200500050,"液压缸","Z0733.03.02.01.01","80/50-15 额定压力25MPa JB/T 5000","台",2,"219厂部","2022-11-10",null,null,"1486.725",2973.45]
[8,7200100181,"液压缸","WG02CD250E160/110-280A10/02A10/02.2HGD","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",1,"219厂部","2022-11-10",null,null,"5124.78",5124.78]
[9,7200100077,"液压缸","CD250D100/70-125A10/02CGDMA","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",2,"219厂部","2022-11-10",null,null,"1725.663",3451.326]
[10,7200100067,"液压缸","CD250B80/56-320A10/02CGDMA+GAK35","缸径Φ80,杆径Φ56,行程320 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"219厂部","2022-11-10",null,null,"1548.67",1548.67]
[11,7200100098,"液压缸","CD250E125/90-350A10/01.1CGDMA L10=380","缸径Φ125,杆径Φ90,行程350 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"219厂部","2022-11-10",null,null,"2546.153846",2546.153846]
[12,7200600208,"130矫直机保护液压缸","GJR13022","Φ400*20","台",1,"89油管热处理","2022-08-27",null,null,"23893.81",23893.81]
[13,7200600027,"滑动水口(二)液压缸","100-50-170 S-100-170-R1-F1","进口密封 缸径Φ100,杆径Φ50,行程170 工作环境温度-20℃~120℃ 工作压力20MPa,试验压力30MPa 活塞及活塞杆采用V型组合耐高温密封 工作介质水乙二醇液压油","台",2,"炼钢厂部","2022-10-27",null,null,"1814.16",3628.32]
[14,7200100140,"液压缸","CDH1MP5/50/36/705.0A11B1CSDBWW 活塞杆与耳环整体制作",null,"台",5,"720厂部","2022-10-27",null,null,"564.1026",2820.5130000000004]
[15,7200600148,"中间包倾翻顶出油缸","80/56-500","头部法兰式油缸 缸径Φ80,杆径Φ56,行程500 工作环境温度-20℃~140℃ 工作压力20MPa,试验压力25MPa 活塞及活塞杆采用V型组合耐高温密封 工作介质聚酯抗燃液压油","台",2,"炼钢厂部","2022-10-27",null,null,"1230.7692",2461.5384]
[16,7200600213,"水冷式液压缸","125/90-380","中间铰接式;带水冷外壳;带缓冲;工作环境温度-20℃~150℃;工作压力15MPa;试验压力25MPa;活塞及活塞杆采用V型组合密封;工作介质聚酯抗燃液压油;附图","台",3,"炼钢厂部","2022-10-27",null,null,"3362.832",10088.496]
[17,7200600055,"热修位液压缸","90/45-203","配进口密封 缸径Φ90,杆径Φ45,行程203 工作环境温度-20℃~140℃ 工作压力20MPa,试验压力25MPa 活塞及活塞杆采用V型组合耐高温密封 工作介质水乙二醇液压油","台",2,"炼钢厂部","2022-11-10",null,null,"1943.365",3886.73]
[18,5700700386,"液压缸耳环","PB172700","45锻钢;15.2Kg","件",4,"89热轧","2022-10-27",null,null,"486.726",1946.904]
[19,5700300538,"液压缸耳环;60","Z0726.02.01.25改01.02","45锻钢","件",3,"89热轧","2022-10-27",null,null,"362.832",1088.496]
[20,7200100211,"液压缸","CD250B160/110-115A10/02CGDMA+GAK80",null,"台",1,"340热轧","2022-11-10",null,null,"5274.34",5274.34]
[21,7200100420,"液压缸","CD250E100/56-280A10/01CADMA;L10=385;配耳环GAS50(带锁紧螺钉)","带GAS50球铰耳环.  L10=385；","台",1,"340热轧","2022-10-27",null,null,"1959.29",1959.29]
[22,7200100421,"液压缸","CD250E125/70-580A10/01CADM;L10=527;配耳环GAS60(带锁紧螺钉)","缸径Φ125,杆径Φ70,行程580 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"340热轧","2022-10-27",null,null,"3250.35",3250.35]
[23,7200100422,"液压缸","CD250E160/110-1080A10/01CADMA;L10=832.5;配耳环GAS80(带锁紧螺钉)","缸径Φ160,杆径Φ110,行程1080 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"340热轧","2022-10-27",null,null,"8271.68",8271.68]
[24,7200100423,"液压缸","CD250E160/110-1045A10/01CADMA;L10=815;配耳环GAS80(带锁紧螺钉)","缸径Φ160,杆径Φ110,行程1045 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"340热轧","2022-10-27",null,null,"8121.68",8121.68]
[25,7200100197,"液压缸","CDH2MT4/80/50-1200A1X/B1",null,"台",1,"管加工厂部","2022-11-10",null,null,"2228.32",2228.32]
[26,5722100010,"增压缸","HGZYG40.30L-2.56-00;2440kg","2440kg","台",1,"管加工厂部","2022-10-26",null,null,"70353.98",70353.98]
[27,7200100256,"液压缸","CG250E100/56-195A10/01CADMA","CG250E100/56-195A10/01CADMA","台",3,"管加工厂部","2022-11-10",null,null,"1724.14",5172.42]
[28,5720300005,"液压缸","YG80/55*770-F","带耳环；压力21MPa","个",4,"管加工厂部","2022-10-27",null,null,"1576.99",6307.96]
[29,7201100052,"液压缸","YG63/36-160-S","缸筒直径63，活塞杆直径36，行程160，工作压力25Mpa，寿命65万次","台",4,"管加工厂部","2022-10-27",null,null,"1017.7",4070.8]
[30,7200400077,"液压缸","BG-D-K-F80-478度-Y",null,"台",2,"管加工厂部","2022-11-10",null,null,"5500",11000]
[31,7200100367,"液压缸","CDH2MS2/63/45/800A1X/M1CHDMWW","63/45/800A","台",1,"管加工厂部","2022-10-27",null,null,"1592.92",1592.92]
[32,7200100162,"液压缸","CDH3MP5/63/45/140A1X/B1HADMWW 活塞杆与耳环整体",null,"台",3,"720厂部","2022-11-10",null,null,"1283.186",3849.558]
[33,7200500043,"液压缸","WG01CD250C100/70-1200 缸径100mm杆径70mm行程1200mm","带耳环，密封材质：尼龙夹布V组，工作压力25MPa","台",2,"720厂部","2022-11-10",null,null,"3185.84",6371.68]
[34,7200100178,"液压缸","WG01CD250B/100/56-210 A10/02.2CADDMAW","额定压力25MPa JB/T 5000","台",2,"180厂部","2022-11-10",null,null,"1508.85",3017.7]
[35,7200500034,"液压缸","CD250B80/56-90A10/02CADMA","额定压力25MPa JB/T 5000","台",2,"180厂部","2022-11-10",null,null,"1132.745",2265.49]
[36,7200500040,"液压缸","HG180011","TJ219HL-03.07-00 额定压力25MPa JB/T 5000","台",1,"管加工厂部","2022-12-10",null,null,"1056.9",1056.9]
[37,5722900049,"液压缸","CD250B60/43-290A10-01CADMA, 配GAS35型球铰耳环","行程290mm；配GAS35型球铰耳环","台",5,"管加工厂部","2022-10-26",null,null,"600",3000]
[38,5718700023,"液压缸","CD250B50/36-240A1001CADMA；","缸径Φ50,杆径Φ36,行程240 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封；","套",2,"管加工厂部","2022-10-26",null,null,"800",1600]
[39,5718700024,"液压缸","CG250E80/45-200A10-01CGDMA L10=270；","缸径Φ80,杆径Φ45,行程200 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封；","套",1,"管加工厂部","2022-10-26",null,null,"900",900]
[40,7200500037,"液压缸","HG180006 PT219.80HL1-01.04.01.07-00","额定压力25MPa JB/T 5000","台",2,"180厂部","2022-12-10",null,null,"1283.185",2566.37]
[41,7200500039,"液压缸","HG180009,PT219.80HL-01.10.5-00","PT219.80HL-01.10.5-00 额定压力25MPa JB/T 5000","台",1,"180厂部","2022-12-10",null,null,"1592.92",1592.92]
[42,7200500077,"液压缸","CDM1MT4/63/45/190X/B1CGDMEW,XV=153","缸径63；杆径45；行程190；压力25PMA","台",2,"180厂部","2022-10-27",null,null,"1061.945",2123.89]
[43,7200100044,"液压缸","CD250B140/100-260A10/02CADMA+GAS70",null,"台",2,"720厂部","2022-12-10",null,null,"3591.895",7183.79]
[44,7200100052,"液压缸","CD250B40/28-230A10/02CADMA","额定压力25MPa JB/T 5000 环境温度100℃","台",4,"180厂部","2022-12-10",null,null,"755.752",3023.008]
[45,7200100078,"液压缸","CD250D80/56-100A10/02CGDMA","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",2,"219厂部","2022-12-10",null,null,"1200.172",2400.344]
[46,7200100166,"液压缸","CGH1MF3/200/140/450A1X/B1CSDBWB",null,"台",1,"720厂部","2022-12-10",null,null,"9734.51",9734.51]
[47,7200100189,"液压缸","CD250E125/90-250A10/02CADMA",null,"台",1,"管加工厂部","2022-12-10",null,null,"2336.28",2336.28]
[48,7200100218,"液压缸","CDH2MT4/80/50-400A1X/B1CFDMWV,XV=480","缸径Φ80,杆径Φ50,行程400 ,工作压力25MPa","台",2,"管加工厂部","2022-12-10",null,null,"1433.63",2867.26]
[49,7200100322,"液压缸","CD250E100/56-460A10/01CADMA；","L10=440；带耳环；JB2162-1991","台",1,"管加工厂部","2022-10-26",null,null,"2212.39",2212.39]
[50,7200100324,"液压缸","CD250C80/56-50A10/02CADAM","缸径80mm，杆径56mm，行程50mm，符合CD250系列标准，V型组合密封","台",2,"89热轧","2022-10-26",null,null,"1548.67",3097.34]
[51,7200100428,"液压缸","CD250F80/56-300A10/02CADMA","80/56-300","台",2,"89热轧","2022-09-30",null,null,"1600",3200]
[52,7200200036,"液压缸","02690005DR5006ME043-79","CD250E100/56-350A10/01CADMA L10=380 额定压力25MPa JB/T 5000","台",2,"管加工厂部","2022-12-10",null,null,"1725.663",3451.326]
[53,7200200038,"液压缸","02690005DR5006ME051-103","CD250E100/70-340A10/01CADMA L10=390 额定压力25MPa JB/T 5000","台",2,"管加工厂部","2022-12-10",null,null,"1811.2",3622.4]
[54,7200200064,"液压缸","Z0745.04.02.02.01G","CD250E80/56-115A10/02CGDMA L10=200 额定压力25MPa JB/T 5000","台",1,"180厂部","2022-12-10",null,null,"5088.497",5088.497]
[55,7200400019,"液压缸","YG63/45-510",null,"套",2,"89油管热处理","2022-12-10",null,null,"1168.14",2336.28]
[56,7200400042,"液压缸","YG63/45*600-F",null,"台",4,"管加工厂部","2022-12-10",null,null,"1362.833",5451.332]
[57,7200400049,"液压缸","SLL-366",null,"台",1,"管加工厂部","2022-12-10",null,null,"1150.44",1150.44]
[58,7200400055,"液压缸","CD250B100/70-345A10/011CADMAC02",null,"台",1,"89油管热处理","2022-12-10",null,null,"1959.29",1959.29]
[59,7200400081,"卡紧油缸","APT127.80-01.09.10","缸径40，杆径25，行程90","台",2,"89油管热处理","2022-11-10",null,null,"1150.44",2300.88]
[60,7200400103,"液压缸","HSGL01-125/70E-1510-300","缸径125，杆径70，行程300，压力等级：25Mpa","台",1,"219厂部","2022-09-26",null,null,"2243.36",2243.36]
[61,7200500035,"液压缸","DYG40X110A-00","额定压力25MPa JB/T 5000","台",2,"180厂部","2022-12-10",null,null,"1221.24",2442.48]
[62,7200500046,"液压缸","Z0224.04.04.01 100/70-135","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",2,"219厂部","2022-12-10",null,null,"7743.365",15486.73]
[63,7200500047,"液压缸","Z0224.12.03.01 80/56-205 进口密封","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",4,"219厂部","2022-12-10",null,null,"1460.176",5840.704]
[64,7200600002,"EBT打开液压缸(水冷式)","80/45-150","缸径Φ80,杆径Φ45,行程150 带水冷外壳 工作环境温度-20℃~140℃ 工作压力20MPa,试验压力25MPa 活塞及活塞杆采用V型组合耐高温密封","台",1,"炼钢厂部","2022-12-10",null,null,"2476.105",2476.105]
[65,7200600023,"钢包升降液压缸","直径450-340","柱塞缸,缸径Φ450,行程340 伸缩防护套耐温150度 工作环境温度-20℃~80℃ 工作压力25MPa,试验压力37.5MPa 工作介质水乙二醇液压油 带缓冲,行程30mm 采用V型组合耐高温密封 重量约3.7t 工作介质水乙二醇液压油 韶关液压件厂","台",1,"炼钢厂部","2022-12-10",null,null,"104427.3505",104427.3505]
[66,7200600134,"液压缸","Z0734.03.01 350/260-70",null,"台",1,"720厂部","2022-12-10",null,null,"31538.46149",31538.46149]
[67,7200600151,"液压缸","268.23SB0081-17;CD250B125/90-200A10/01CADMA+GAS60改;","耐30兆帕高压，密封为进口件，位移传感器灵敏度不得有误，带耳环GAS60","台",1,"管加工厂部","2022-11-10",null,null,"3226.55",3226.55]
[68,7200600206,"液压缸","YF0176-23P","CD250E50/36-220A10/01CADMA;L10=200,带与位移传感器953AC40230MXXSX相配的磁环；不带传感器","台",4,"89热轧","2022-10-11",null,null,"1194.69",4778.76]
[69,7201300033,"液压缸耳环","GAK22",null,"件",10,"89热轧","2022-11-10",null,null,"38.938",389.38]
[70,7501800015,"液压缸耳环","GAS50",null,"件",2,"管加工厂部","2022-09-26",null,null,"121.416",242.832]
[71,7502000053,"液压缸耳环","GAK45",null,"件",2,"管加工厂部","2022-11-10",null,null,"115.045",230.09]
[72,7502000054,"液压缸耳环","GAK58",null,"套",2,"管加工厂部","2022-11-10",null,null,"181.417",362.834]
[73,5723000021,"液压缸","CD250B100/56-200A10/01CADMA, 配GAS50球铰耳环","行程200mm；配GAS50球铰耳环","台",2,"管加工厂部","2022-10-26",null,null,"800",1600]
[74,5723000022,"液压缸","CD250A100/56-165A10/14CADMA","行程165mm","台",2,"管加工厂部","2022-10-26",null,null,"800",1600]
[75,5723000023,"液压缸","CD250A125/70-296A10/02CADMA","行程296mm","只",2,"管加工厂部","2022-10-26",null,null,"900",1800]
[76,7200400084,"液压缸","CDH2-MT4-80-56-250-1X-MCHMWW","缸径80；杆径56；行程250；带CGKD50耳环","台",1,"180厂部","2022-09-26",null,null,"1394",1394]
[77,7200400107,"磁粉探伤拨料缸","HSGL01-125/70E-3510-300","缸径125，杆径70，行程300，压力等级：25Mpa","台",1,"219厂部","2022-10-26",null,null,"2500",2500]
[78,7200600231,"锯床举升油缸","油缸型号：80*430","缸径：80；行程：430；锯床G4240/50上用","台",2,"管加工厂部","2022-10-26",null,null,"800",1600]
[79,7200600232,"锯床张紧油缸","油缸型号：90*30","缸径：90；行程：30；锯床G4240/50上用","台",2,"管加工厂部","2022-10-26",null,null,"500",1000]
[80,7200600233,"锯床夹钳油缸","油缸型号：90*380","缸径：90；行程：380；锯床G4240/50上用","台",2,"管加工厂部","2022-10-26",null,null,"800",1600]
["注：1、投标报价含税，税率13% ；                                                                                                                          2、生产厂家要求全称填写准确无误 ；                                                                                                                     3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2022年8月液压缸采购项目                             项目编号：HGCGD22105"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]