{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":37,"n_cols":13,"rows_kept":37,"merged":[[0,0,0,8],[1,0,1,12],[33,0,33,8],[34,0,34,8],[35,0,35,8],[36,0,36,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2022年8月机械配件采购项目Ⅱ                     项目编号：HGCGD22106"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,5000400112,"蜗轮蜗杆斜齿轮减速机","SA92-1/100-YEJ4kW-6P-M1","传动比47.2;额定功率4Kw;配反力矩环板GST97-01QT K","台",2,"Q/ZTB04-2000","炼钢厂部","2022-10-11"]
[2,5501700061,"皮带机缓冲床","JHYHCC1012，B1000*1200","缓冲条材质为超高分子量聚乙烯，可单独拆卸；缓冲条总面积不小于1.2m2,厚度不小于70mm；缓冲支座抗冲击强度不小于100Kgf/cm2；总重约1吨","套",2,"审核图纸","高辅工段","2022-10-11"]
[3,6700200044,"冲击试验机 硫化氢减压阀 R11LG-EGG-00-00","R11LG-EGG-00-00",null,"只",1,"JB/T10365-2002","检验检测中心","2022-10-11"]
[4,7001200343,"高压泵连杆","3D-250-0102",null,"根",4,null,"219厂部","2022-10-11"]
[5,7100300433,"电磁球阀","AS22061a-G24","常闭，带应急按钮","个",2,"ISO4401","89热轧","2022-10-11"]
[6,7101800177,"不锈钢水嘴","15",null,"只",10,"CJ/T406-2012","219厂部","2022-10-11"]
[7,5400100044,"离心式空压机 中间冷却器","FS-ELLIOTT 260","铆焊 材质：管道为紫铜，翅片为铝 耐压大于1.6Mpa 耐温大于250℃ 冷却气量大于300m3/min 冷却出口温度<52℃","台",1,"JB/T10598","能源厂部","2022-10-11"]
[8,7102100009,"气动控制阀","Z014-A DN80 PN25",null,"只",8,"GB/T3452.1-1992","180厂部","2022-10-11"]
[9,5501700003,"堆取料机;斗轮机构轴承座","D223A-11.0","ZG35 孔径50，轴向孔距145，径向孔距530，座低平面与孔中心线夹角5°侧端盖带注油孔M10","件",2,null,"原料工段","2022-10-11"]
[10,6600300037,"煤气调节阀","LPB12-1D3B4DRC1-350P-16A","阀门口径 DN350 压力等级：ANSI150# 对夹式 流量特性：近似等百分比特性 行程90度 阀体WCB、阀板CF8M不锈钢、阀杆17-4PH不锈钢、阀座RPTFE：泄漏等级：ClassⅥ","只",1,"GB/T4213-2008","180厂部","2022-10-11"]
[11,5601700022,"拖链","TL180III-R450*510*8640","支撑板宽度510mm:节数48;附订货图","件",2,"JB/T6608-1993","炼钢厂部","2022-10-11"]
[12,5501700071,"双向可逆皮带机JHY免维护校正器（返式）","JHYJZP1000BD-B  带宽1000，长1480×宽350×高420","露天双向可逆，；包胶花纹主辊D180×1040，主托辊辊面衬胶采用复合聚氨脂材料，具有防冻、防滑、防脱落及耐磨性能，且满足当地气候温度，托辊具有防尘、防水，动作灵敏可靠，无噪音，调偏幅度大，不损伤皮带，表面胶层硬度不得低于60～70°(邵氏A型硬度)，质保期三年，质保期内无需更换任何配件。","套",2,"ZL202020201838.8","原料工段","2022-10-11"]
[13,5501700072,"双向可逆皮带机JHY免维护校正器","JHYJZP1000AD-B   带宽1000，长1370×宽270×高267","露天双向可逆，包胶花纹主辊D159/d133×375，主托辊辊面衬胶采用复合聚氨脂材料，具有防冻、防滑、防脱落及耐磨性能，且满足当地气候温度，托辊具有防尘、防水，动作灵敏可靠，无噪音，调偏幅度大，不损伤皮带，表面胶层硬度不得低于60～70°(邵氏A型硬度)，质保期三年，质保期内无需更换任何配件。","套",2,"ZL202020201838.8","原料工段","2022-10-11"]
[14,5501200074,"双层插板卸灰阀插板","DSXF-DN300;103","304不锈钢","件",10,null,"烧结","2022-10-11"]
[15,7101800130,"气动球阀","DN150 ANSI 300 ASMEB16.5","铸钢 F30，CLASS ANSI300，ASTMA216WCB，A351 CF8M，STAINLESS316，ANSI 300 ASMEB16.5","只",1,null,"高辅工段","2022-10-11"]
[16,5500800013,"星形卸灰阀","YXD-570","570*570 高度600 带电机 铸钢 GB16490-1996 工作温度450℃，介质：高炉瓦斯灰，壳体材质：Q235，叶轮材质：不锈钢，叶轮与壳体间隙30丝，轴密封采用石墨盘根，扎三圈，便于更换，带电机、减速机电动机型号 YKF2-100L1-4 电压 380V，电流 5.09 轴伸端轴承 6206-2RS 功率2.2KW 减速机型号 XLD4-2B","套",1,"GB16490-1996","高辅工段","2022-10-11"]
[17,7100100089,"减压阀","DR30-1-30/315YM","ISO 4401","只",2,"GB2514-1987","180厂部","2022-10-11"]
[18,5720400017,"管加3号线淬火炉插管式空气换热器","插件安装尺寸2526*1420*4290mm;","燃烧介质为混合煤气;换热器前烟气温度650~780℃，排烟量15000~18000Nm3/h ;空气量8000~12000Nm3/h，风压7~12kPa; 预期空气预热温度 ~350℃;材质:换热器材质1Cr18Ni9钢管;附：安装示意图（插件部份成套设备） 。","套",1,"审核图纸","管加工厂部","2022-10-11"]
[19,7100100232,"安全阀","A48Y-16C-40","压力等级0.8-1.1Mpa；整定压力0.85Mpa","台",1,"GB/T12243-2005","高辅工段","2022-10-11"]
[20,7100100254,"安全阀","A48Y-25-100","压力等级1.3-1.6Mpa；整定压力1.45Mpa，DN100","只",1,"GB/T12243-2005","能源厂部","2022-09-26"]
[21,7100100255,"安全阀","A48Y-25-80","压力等级1.3-1.6Mpa；整定压力1.45Mpa，DN80","只",1,"GB/T12243-2005","能源厂部","2022-09-26"]
[22,7100100256,"安全阀","A48Y-25-65","压力等级1.3-1.6Mpa；整定压力1.32Mpa，DN65","只",1,"GB/T12243-2006","能源厂部","2022-09-26"]
[23,5100100540,"高压泵尼龙柱销","直径34.5*65","材料:尼龙","只",60,"GB/T1972-2005","高辅工段","2022-10-11"]
[24,5100100541,"高压泵尼龙柱销","直径29.5*55","材料：尼龙","只",60,"GB/T1972-2005","高辅工段","2022-10-11"]
[25,5100100567,"弹性套柱销","LT12","直径38，长度165，配挡圈，弹簧垫，4连体弹性圈，紧固螺母M30，材质：45，","只",50,"GB4323-84","管加工厂部","2022-10-26"]
[26,5400200039,"声波清灰清堵器过滤器","LTFGLQ—01","接口尺寸DN25，1.0MP，具有压缩空气过滤及调压功能，材质铸铝，滤芯材质为黄铜","个",4,"GB/T6165","能源厂部","2022-09-26"]
[27,5400200040,"声波清灰清堵器电磁阀","LTFDCF—02","接口尺寸DN25，1.0Mpa,电源：220V，功率25KW，材质：黄铜，高强度滤芯","只",2,"JISB8373-1993","能源厂部","2022-10-11"]
[28,5716700092,"2号线脉冲烧嘴1","天燃气烧嘴SIO 140HB-150/135;430KW;","烧嘴含观火玻璃孔、点火电检、检测电极;内丝通径DN40;","套",2,"执行标准GB/T 35073-2018","管加工厂部","2022-10-26"]
[29,5716700093,"2号线脉冲烧嘴2","天燃气烧嘴SIO 100HB-150/135;230KW;","烧嘴含观火玻璃孔、点火电检、检测电极;内丝通径DN25;","套",2,"执行标准GB/T 35073-2018","管加工厂部","2022-10-26"]
[30,5716700094,"2号线脉冲烧嘴3","天燃气烧嘴SIO 800HB-150/135;150KW;","烧嘴含观火玻璃孔、点火电检、检测电极;内丝通径DN20;","套",5,"执行标准GB/T 35073-2018","管加工厂部","2022-10-26"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误          "]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2022年8月机械配件采购项目Ⅱ             项目编号：HGCGD22106"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":4,"n_cols":1,"rows_kept":4,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8]],"flags":["formulas_cached_only"]}
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]