{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":77,"n_cols":13,"rows_kept":77,"merged":[[0,0,0,10],[1,0,1,10],[73,0,73,10],[74,0,74,10],[75,0,75,10],[76,0,76,10]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2022年9月液压缸采购项目                             项目编号：HGZB"]
["序号","资材编号","资材名称","规格型号","技术参数","单位","数量","使用部门","交货时间","含税单价","生产厂家\n（品牌）"]
[1,7200600241,"快开增压缸","02690045DR5005ME009-16","快开缸260/200-70；工作压力50MPa；增压缸260/140-245；工作压力14MPa","台",1,"720热轧","2022-11-28",null,null,"1115.045",1115.045]
[2,5700300538,"液压缸耳环;60","Z0726.02.01.25改01.02","45锻钢","件",3,"89热轧","2022-11-28",null,null,"6690.27",20070.81]
[3,7200200086,"液压缸","PB65KSGWGG1125/90-1850双耳轴轴加粗为70","双耳轴轴加粗为70,缸体材料40Cr,原厂家韶关伟光","台",2,"89热轧","2022-11-28",null,null,"1000",2000]
[4,7200600208,"130矫直机保护液压缸","GJR13022","Φ400*20","台",1,"89油管热处理","2022-11-28",null,null,"3400",3400]
[5,7200500047,"液压缸","Z0224.12.03.01 80/56-205 进口密封","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",4,"219厂部","2022-12-10",null,null,"2699.12",10796.48]
[6,7200600206,"液压缸","YF0176-23P","CD250E50/36-220A10/01CADMA;L10=200,带与位移传感器953AC40230MXXSX相配的磁环；不带传感器","台",4,"89热轧","2022-11-28",null,null,"1185.84",4743.36]
[7,7200500069,"液压缸","0107119-41.011",null,"台",2,"180厂部","2022-11-28",null,null,"1486.725",2973.45]
[8,7200600027,"滑动水口(二)液压缸","100-50-170 S-100-170-R1-F1","进口密封 缸径Φ100,杆径Φ50,行程170 工作环境温度-20℃~120℃ 工作压力20MPa,试验压力30MPa 活塞及活塞杆采用V型组合耐高温密封 工作介质水乙二醇液压油","台",2,"炼钢厂部","2022-11-28",null,null,"5124.78",10249.56]
[9,7200100140,"液压缸","CDH1MP5/50/36/705.0A11B1CSDBWW 活塞杆与耳环整体制作",null,"台",5,"720厂部","2022-11-28",null,null,"1725.663",8628.315]
[10,7200600148,"中间包倾翻顶出油缸","80/56-500","头部法兰式油缸 缸径Φ80,杆径Φ56,行程500 工作环境温度-20℃~140℃ 工作压力20MPa,试验压力25MPa 活塞及活塞杆采用V型组合耐高温密封 工作介质聚酯抗燃液压油","台",2,"炼钢厂部","2022-11-28",null,null,"1548.67",3097.34]
[11,5722100010,"增压缸","HGZYG40.30L-2.56-00;2440kg","2440kg","台",1,"管加工厂部","2022-11-28",null,null,"2546.153846",2546.153846]
[12,7200100256,"液压缸","CG250E100/56-195A10/01CADMA","CG250E100/56-195A10/01CADMA","台",3,"管加工厂部","2022-11-28",null,null,"23893.81",71681.43000000001]
[13,7200400077,"液压缸","BG-D-K-F80-478度-Y",null,"台",2,"管加工厂部","2022-11-28",null,null,"1814.16",3628.32]
[14,7200500040,"液压缸","HG180011","TJ219HL-03.07-00 额定压力25MPa JB/T 5000","台",1,"管加工厂部","2022-12-10",null,null,"564.1026",564.1026]
[15,5722900049,"液压缸","CD250B60/43-290A10-01CADMA, 配GAS35型球铰耳环","行程290mm；配GAS35型球铰耳环","台",5,"管加工厂部","2022-11-28",null,null,"1230.7692",6153.846]
[16,5718700024,"液压缸","CG250E80/45-200A10-01CGDMA L10=270；","缸径Φ80,杆径Φ45,行程200 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封；","套",1,"管加工厂部","2022-11-28",null,null,"3362.832",3362.832]
[17,7200500037,"液压缸","HG180006 PT219.80HL1-01.04.01.07-00","额定压力25MPa JB/T 5000","台",2,"180厂部","2022-12-10",null,null,"1943.365",3886.73]
[18,7200600023,"钢包升降液压缸","直径450-340","柱塞缸,缸径Φ450,行程340 伸缩防护套耐温150度 工作环境温度-20℃~80℃ 工作压力25MPa,试验压力37.5MPa 工作介质水乙二醇液压油 带缓冲,行程30mm 采用V型组合耐高温密封 重量约3.7t 工作介质水乙二醇液压油 韶关液压件厂","台",1,"炼钢厂部","2022-12-10",null,null,"486.726",486.726]
[19,5723000021,"液压缸","CD250B100/56-200A10/01CADMA, 配GAS50球铰耳环","行程200mm；配GAS50球铰耳环","台",2,"管加工厂部","2022-11-28",null,null,"362.832",725.664]
[20,5723000022,"液压缸","CD250A100/56-165A10/14CADMA","行程165mm","台",2,"管加工厂部","2022-11-28",null,null,"5274.34",10548.68]
[21,5723000023,"液压缸","CD250A125/70-296A10/02CADMA","行程296mm","只",2,"管加工厂部","2022-11-28",null,null,"1959.29",3918.58]
[22,7200600231,"锯床举升油缸","油缸型号：80*430","缸径：80；行程：430；锯床G4240/50上用","台",2,"管加工厂部","2022-10-26",null,null,"3250.35",6500.7]
[23,7200600232,"锯床张紧油缸","油缸型号：90*30","缸径：90；行程：30；锯床G4240/50上用","台",2,"管加工厂部","2022-11-28",null,null,"8271.68",16543.36]
[24,7200600233,"锯床夹钳油缸","油缸型号：90*380","缸径：90；行程：380；锯床G4240/50上用","台",2,"管加工厂部","2022-11-28",null,null,"8121.68",16243.36]
[25,7200200036,"液压缸","02690005DR5006ME043-79","CD250E100/56-350A10/01CADMA L10=380 额定压力25MPa JB/T 5000","台",2,"管加工厂部","2022-12-10",null,null,"2228.32",4456.64]
[26,7200400042,"液压缸","YG63/45*600-F",null,"台",4,"管加工厂部","2022-12-10",null,null,"70353.98",281415.92]
[27,7200400049,"液压缸","SLL-366",null,"台",1,"管加工厂部","2022-12-10",null,null,"1724.14",1724.14]
[28,7200600134,"液压缸","Z0734.03.01 350/260-70",null,"台",1,"720厂部","2022-12-10",null,null,"1576.99",1576.99]
[29,7200200064,"液压缸","Z0745.04.02.02.01G","CD250E80/56-115A10/02CGDMA L10=200 额定压力25MPa JB/T 5000","台",1,"180厂部","2022-12-10",null,null,"1017.7",1017.7]
[30,7200500035,"液压缸","DYG40X110A-00","额定压力25MPa JB/T 5000","台",2,"180厂部","2022-12-10",null,null,"5500",11000]
[31,7200100241,"液压缸","CD250E100/56-435A10/01CADMA",null,"台",1,"管加工厂部","2023-01-10",null,null,"1592.92",1592.92]
[32,5721700042,"预密封缸","FPWV220*390-00；570kg；","系统压力25MPa，增压容积15升，水腔试验压力为16MPa","套",1,"管加工厂部","2022-11-26",null,null,"1283.186",1283.186]
[33,7200200079,"液压缸","YG125/70*420-S",null,"台",2,"管加工厂部","2023-01-10",null,null,"3185.84",6371.68]
[34,7200400033,"液压缸","YG80/45*200-S",null,"台",4,"管加工厂部","2023-01-10",null,null,"1508.85",6035.4]
[35,7200400078,"液压缸","YG100/55*220-S",null,"台",1,"管加工厂部","2023-01-10",null,null,"1132.745",1132.745]
[36,7200100260,"液压缸","CD250E100/56-220A10/01CADMA311","必须带球铰耳环GAS50 额定压力25MPa L10=311   GB/T15622-2005","台",4,"管加工厂部","2022-10-27",null,null,"1056.9",4227.6]
[37,7200100022,"液压缸","CD250A80/56-170A10/02CGDMA","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",2,"管加工厂部","2023-01-10",null,null,"600",1200]
[38,7200100064,"液压缸","CD250B80/45-80A10-02CADMA","缸径Φ80,杆径Φ45,行程80 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"219厂部","2023-01-10",null,null,"800",800]
[39,7200100108,"液压缸","CD250E180/110-265A10/02CADMA+GAS90 L10=570 内置传感器及保护罩",null,"台",1,"720厂部","2023-01-10",null,null,"900",900]
[40,7200100171,"液压缸","HYDRAULTC CYLINDER SF601916","额定压力25MPa JB/T 5000","台",2,"180厂部","2023-01-10",null,null,"1283.185",2566.37]
[41,7200400058,"液压缸","PBA03CH00000;100/85-90",null,"台",4,"340热轧","2023-01-10",null,null,"1592.92",6371.68]
[42,7200600130,"液压缸","WG11252 125/90-150","缸径Φ125,杆径Φ90,行程150 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞采用PG型组合密封 活塞杆采用RS+USH型组合密封","台",4,"340热轧","2023-01-10",null,null,"1061.945",4247.78]
[43,7200400046,"液压缸","HY89G34-360B",null,"台",2,"89热轧","2023-01-10",null,null,"3591.895",7183.79]
[44,7200200013,"液压缸","02690005DR5003ME005-33","CD250E120/90-450A10/01CGDMA","台",1,"180厂部","2023-01-10",null,null,"755.752",755.752]
[45,7201200001,"稳压缸","HGWYG80.15L-4.94-15","400*180-600,试验水腔压力96MPa","台",1,"管加工厂部","2023-01-10",null,null,"1200.172",1200.172]
[46,7200500038,"液压缸","HG180007,JAJ89-273-31-00","JAJ89-273-31-00 额定压力25MPa JB/T 5000","台",3,"管加工厂部","2023-01-10",null,null,"9734.51",29203.53]
[47,7200500041,"液压缸","HG180012","TJ219HL-07.01.27 额定压力25MPa JB/T 5000","台",2,"管加工厂部","2023-01-10",null,null,"2336.28",4672.56]
[48,7200400069,"液压缸","100/56-250","17MPa;带连接耳环;带MTS传感器","台",1,"管加工厂部","2023-01-10",null,null,"1433.63",1433.63]
[49,7501800032,"液压缸活塞杆","EC03J0000",null,"件",8,"340热轧","2022-11-11",null,null,"2212.39",17699.12]
[50,7502000058,"液压缸耳环","GAS35",null,"件",3,"180厂部","2022-12-11",null,null,"1548.67",4646.01]
[51,7501800015,"液压缸耳环","GAS50",null,"件",9,"219厂部","2022-10-27",null,null,"1725.663",15530.967]
[52,7502000057,"液压缸耳环","GAS30",null,"件",10,"180厂部","2022-12-11",null,null,"1811.2",18112]
[53,7502000060,"液压缸耳环","GAS60",null,"件",13,"管加工厂部","2022-12-11",null,null,"1168.14",15185.820000000002]
[54,7502000059,"液压缸耳环","GAS40",null,"件",3,"180厂部","2022-12-11",null,null,"1362.833",4088.4990000000003]
[55,7502000061,"液压缸耳环","GAS70",null,"件",3,"180厂部","2022-12-11",null,null,"1150.44",3451.32]
[56,7200100257,"液压缸","CD250B125/90-405A10/01CADMAJB/T10205-2000","250B125/90-405A10/01CADMAJB/T10205-2000","台",2,"管加工厂部","2023-01-10",null,null,"1959.29",3918.58]
[57,7200100286,"液压缸","02680014DR5005ME003-12","CD250B63/45-115A10/01CGDMA","台",5,"89热轧","2022-10-27",null,null,"1150.44",5752.200000000001]
[58,7200100300,"液压缸","02680014DR5005ME048-3","CD250B63/45-355A10/01CGDMA","台",2,"89热轧","2022-10-27",null,null,"2243.36",4486.72]
[59,7200100344,"液压缸","02680014DR5005ME024-66","按CD250F140/100-5350A10/01CGDMA标准，进口密封件","台",1,"89热轧","2022-12-11",null,null,"1221.24",1221.24]
[60,7200600202,"液压缸","CDH1/MP3/50/28/250A1X+GAS30 带耳环;","带耳环;缸径Φ50,杆径Φ28,行程250 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",5,"管加工厂部","2022-11-26",null,null,"7743.365",38716.825]
[61,5723600003,"注水阀油缸","08 201934-01.02.05.10","缸径80，杆径45，行程310，额定压力20MP，接头G3/4","台",2,"管加工厂部","2022-11-26",null,null,"1194.69",2389.38]
[62,5723600004,"排气阀油缸","12 201934-01.09.04.05","缸径80，杆径45，行程210，额定压力20MP，接头G3/4","台",2,"管加工厂部","2022-11-26"]
[63,5723600005,"注水端油缸","06 201909-01.02.12","缸径100，杆径70，行程550，额定压力25MP，接头G3/4，带耳环","台",2,"管加工厂部","2022-11-26"]
[64,5723600006,"卡环油缸","07 201934-01.02.20","缸径50，杆径280，行程140，额定压力25MP，接头G1/2","台",2,"管加工厂部","2022-11-26"]
[65,7200100405,"油缸","CD250E125/70-130A10/01CADMA","配GAS60耳环；缸径125，杆径70，行程130","台",2,"管加工厂部","2022-11-26",null,null,"38.938",77.876]
[66,7200100430,"液压缸","CD250E160/100-600A10/02+耳环+磁环","全套进口密封件；L10=650","台",1,"219厂部","2022-10-12",null,null,"121.416",121.416]
[67,7200100431,"液压缸","CD250E140/90-670A10/02+耳环","全套进口密封；L10=525","台",1,"219厂部","2022-10-12",null,null,"115.045",115.045]
[68,7200100432,"液压缸","CD250B125/70-170A10/01+耳环","全套进口密封","台",1,"219厂部","2022-10-12",null,null,"181.417",181.417]
[69,7200100433,"液压缸","CD250E80/56-2000A10/02CADMA+GAS50 L10=1265","缸径Φ80,杆径Φ56,行程2000 工作环境温度20℃~80℃ 工作压力15MPa,试验压力25MPa 活塞及活塞杆采用格莱圈密封 工作介质46#抗磨液压油","台",2,"340热轧","2022-10-27"]
[70,7200600002,"EBT打开液压缸(水冷式)","80/45-150","缸径Φ80,杆径Φ45,行程150 带水冷外壳 工作环境温度-20℃~140℃ 工作压力20MPa,试验压力25MPa 活塞及活塞杆采用V型组合耐高温密封","台",1,"炼钢厂部","2022-12-27",null,null,"800",800]
["注：1、投标报价含税，税率13% ；                                                                                                                          2、生产厂家要求全称填写准确无误 ；                                                                                                                     3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2022年9月液压缸采购项目                             项目编号：HGZB"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]