{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":69,"n_cols":12,"rows_kept":69,"merged":[[0,0,0,11],[1,0,1,11],[65,0,65,8],[66,0,66,8],[67,0,67,8],[68,0,68,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2022年9月电气备件采购项目Ⅱ                    项目编号：HGCGD22122"]
["序号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家"]
[1,6100400164,"电位器","WX03-4.7K",null,"GB/T 11210-1989","只",20,"管加工厂部","2022-12-10"]
[2,6400400052,"主轴编码器","IRS660-1024-826","IEC 61131-3","IEC 61131-3","只",2,"管加工厂部","2022-12-10"]
[3,4100800030,"声光报警器","FMD-116/A","3A，35W，220V GB 10963.1","GB 10963.1","台",10,"炼铁厂部","2022-12-10"]
[4,6300500046,"安全继电器","PNOZ XV3 30SEC","24VDC",null,"块",1,"340热轧","2023-01-10"]
[5,6100500380,"时间继电器","H3YN-2 TIMER","AC200-230V ;50/60HZ;8针","GB14048.5","只",20,"180厂部","2022-12-10"]
[6,7101600168,"气动控制阀门","D376XE73;OMAL","DN125;OMAL;带执行器","ISO5211","台",1,"89油管车丝委外","2022-12-10"]
[7,6100600194,"熔断器座","RT18-32X","500/380V 32A",null,"个",20,"检验检测中心","2022-12-10"]
[8,4100600018,"声光报警蜂鸣器","AD16-22SM","AC220V 红色 开孔直径22mm","SJ/T 10660-1995","只",50,"89油管车丝委外","2022-12-10"]
[9,4100400023,"PVC电缆号码套管","*","φ4.0 100m/卷 塑料 阻燃性VW-1 耐温200℃ 内径4mm2","GB/T 28605-201","卷",2,"物流中心","2022-12-10"]
[10,4100400024,"PVC电缆号码套管","*","φ2.5 100m/卷 塑料 阻燃性VW-1 耐温 200℃内径2.5mm2","YD/T841.2-2008","卷",2,"物流中心","2022-12-10"]
[11,6300500256,"位移监测模块","EK-C6682","EK-C6682双通道位置监测模块，可接收两个标准的电涡流传感器输入信号，监测轴端止推轴承的轴向位置，电源：220VAC",null,"个",1,"高炉","2022-12-10"]
[12,6600300160,"阀门回讯器","SBU-AD-M208-K211-M01","U;250V;I;5A;IP65/IP67/IP68","GB/T12237","个",5,"炼钢厂部","2022-12-10"]
[13,6300200175,"PLC模块","1769-OB32","供电电压;24VDC;   点数;继电器输出32点;   AB","IEC61508","块",2,"高炉","2022-12-10"]
[14,6300300146,"控制模块","1756-CN2R","AB；","IEC61508","块",1,"高炉","2022-12-10"]
[15,6300100116,"CPU模块","1756-L72","AB；","IEC61508","块",1,"高炉","2022-12-10"]
[16,6300700061,"操作屏","smart700iev3(含程序及调试)","电压DC24V，RS422/RS485，USB","IEC61508","块",1,"高炉","2022-12-10"]
[17,6000400020,"合闸电磁铁","220VDC 205Ω",null,"GB14048.4-93","只",10,"炼钢厂部","2022-12-10"]
[18,6100900049,"不锈钢电阻器","RS54-280M-8/5H","75KW","IEC61508","套",1,"炼钢厂部","2022-12-10"]
[19,6200200205,"变频器","20G11NC072JA0NNNNN 37Kw PowerFIex755","进线电压：3相 380V-480VAC 额定功率37KW 重载功率30KW 额定电流72A",null,"台",2,"管加工厂部","2022-12-10"]
[20,6200200055,"变频器","20BC011A3AYNANCO 5.5Kw/4Kw AB E0.967X","E0.969X","E0.967X","台",1,"高炉","2022-12-10"]
[21,6400400036,"绝对编码器","CEV65M-01460 ELECTRONIC GMBH","输出方式: （绝对式}：工作电压: 11-27vDC：防护等级(IP66)：Nr 1358438","DIN 32878-1993","只",2,"180厂部","2022-12-10"]
[22,7502500038,"电机冷却通风机","G180-A",null,"GB14711-2006","台",5,"炼钢厂部","2022-12-10"]
[23,6000300199,"不锈钢电阻器","RVS34-315M-10","与调压调速装置配套YZR315M-10/75KW电机匹配;电阻段R4=0.084Ω;R3=0.140Ω;R2=0.220Ω;R1=0.440Ω;U\\V\\W三相各段阻值相等.","JB/T 11410-2013","台",1,"炼钢厂部","2022-12-10"]
[24,6600300020,"阀门定位器","YT-1000RDM132SOO","输入信号4-20mA 供气压力 1.4-7.0kgf/c㎡cm 工作温度 -20-70℃ 双作用","GB/T9248-1999","只",4,"管加工厂部","2022-12-10"]
[25,6200200619,"调速器底板","QT-006DI-H",null,"JB/T8680-2008","块",1,"管加工厂部","2022-12-10"]
[26,6100300155,"断路器:","DZ158-100A/3P","380V 3P 100A","JB/T8735.2011","只",10,"180厂部","2022-12-10"]
[27,6200200453,"调压调速散热风机","KA9225HA2","AC220v","GB/T22712-2008","只",10,"180厂部","2022-12-10"]
[28,6100300268,"分闸线圈","ZN5","DC220V,线径0.31mm，匝数3660，","GB/T14048","个",5,"能源厂部","2022-12-10"]
[29,6400200054,"光电开关安装支架","BEF-WG-W24 德国IEC947","订货号:4 026 324","德国IEC947","件",20,"180厂部","2022-12-10"]
[30,6100500408,"微型继电器","G2R-1","24VDC(5脚)","EN 60947-5-2","只",10,"炼钢厂部","2022-12-10"]
[31,6400200066,"热金属检测器","LOS-R2-4ZC1","反光板型 直流24V 输出形式pnp和继电器一常开一常闭 快速接头10芯引出线 带反光板SP-17/N 环境温度-25℃-+120℃","Q/3204BCK010-2013","台",19,"管加工/219厂部","2022-12-10"]
[32,6400600505,"位移传感器","KYCM-HL0500FS/ZDA,防水型；","工作电源24Ⅴ，测量量程500mm，输出信号4-20ma","Q/XKYC9-2009","只",1,"管加工厂部","2022-12-10"]
[33,6200100094,"停电保护控制系统 蓄电池","6QW-200AH；外形尺寸：507*221*195*218；","额定电压：12V；容量：200AH；放电倍率在6倍率以上；耐高温，荷电常温贮存一年。","XK06-006-00420","只",18,"管加工厂部","2022-12-10"]
[34,6400600507,"负荷传感器","BK-1B;15t","12VDC; 输出4-20mA; 精度等级：0.1",null,"台",2,"180厂部","2022-12-10"]
[35,6200200868,"变频器","NZ200-22G/30P-4","INPUT:3PH 380V 50Hz/60Hz  OUTPUT:3PH 380V G22/P30KW 45/60A","GB/T12668.2-2002","台",2,"炼钢厂部","2022-12-10"]
[36,6200200859,"变频器","GD200A-004G/5R5P-4","4Kw～5.5Kw;3AC380V（-15%）-440V（+10%）","IEC/EN 61800-3","台",1,"炼钢厂部","2022-12-10"]
[37,6400400122,"编码器","GHU9-30//5G39//1024G//3R","增量型编码器;UB:+9～30V,脉冲数1024 HTL;IP67;法国艾迪克","EN 60947-5-2","只",1,"炼钢厂部","2022-12-10"]
[38,7502500101,"机柜排风扇","FKL6626.230-D","额定工作电230V/50Hz;空气流量1200m3/h;额定电流0.291A;额定功率210瓦;工作温度范围-10℃至+55℃;出口过滤器型号FK6626.300","GB/T23174-2008","台",4,"炼钢厂部","2022-12-10"]
[39,6400500841,"碳刷","板簧和碳H742003","H742039  BH DS","JB/T4003-2001","个",30,"管加工厂部","2022-12-10"]
[40,6300600074,"喷标机主板","303001A","DRA3000-16N自喷标机主板;型号303001A",null,"块",1,"720厂部","2022-12-10"]
[41,6100600260,"熔断器","NGT1;1000V,100A","1000V,100A","IEC269;GB13539","个",6,"720厂部","2022-12-10"]
[42,6400600504,"超声波传感器","UM30-13111","工作电压12-30VDC ;模拟输出4-20mA；感应距离30-1300mm; 防护等级(IP67) 5针M12插头","DIN EN 62365-2010","只",3,"180厂部","2022-12-10"]
[43,6600100242,"专用电池","数显游标卡尺专用电池",null,"GB/T 4844.1-1995","瓶",20,"180厂部","2022-12-10"]
[44,6000300235,"瓦格拉锯电机风轮","YF-1","直径：250mm,高：64mm, 孔：19mm,键槽：6mm","GB/T 1236-2000","个",5,"89油管车丝委外","2022-12-10"]
[45,6000300236,"瓦格拉锯电机风轮","YF-2","直径：180mm,高：80mm, 孔：19mm,键槽：6mm","GB/T 1236-2000","个",5,"89油管车丝委外","2022-12-10"]
[46,6300600078,"喷码机主控板","PMC-PJ1A","IC4-2216-J主控板","IEC61509","块",1,"89油管车丝委外","2022-12-10"]
[47,6400200013,"对射式光电开关","OM30-EVP6 ELCO JT 2-30s/1499","外形:圆柱型 外壳材质:金属 检测模式/感应类型:对射式（接收器） 供电范围:10-30VDC 感应范围:0-25m 输出形式:PNP 输出特性:常开1点，常闭1点 接线方式:导线输出连接 防护等级:IP67","JT 2-30s/1499","只",10,"检验检测中心","2022-12-10"]
[48,6600200123,"阀门定位器","EPA814","输入 4-20mA/DC，气源:8Kgf/cm2 8Bar 最大120Psi 800KPa","JB/T8219-2000","只",4,"219厂部","2022-12-10"]
[49,6200100035,"直流调速装置","DCM-CON70-V 0","四相限控制 带profibus-dp通讯板 小装置控制大功率晶闸管整流装置 带励磁控制单元220V,39A 晶闸管主回路直流输出电压DC850V 额定输出直流电流3162A，直流电机带编码器速度反馈，可弱磁升速。",null,"套",1,"219厂部","2022-12-10"]
[50,6100300284,"时控开关","SX102L","工作电压：3*380VAC±15%;50-60HZ;控制负载≤4KW三相（阻性）;控制电流：3*16A","GB/T14536.1","个",5,"检验检测中心","2022-12-10"]
[51,6400100014,"热金属检测器光纤","OFH-A1","光纤长度L=5000mm 金属外壳","GB/T 29231-2012","根",7,"219厂部","2022-12-10"]
[52,6400100004,"热金属检测器 光钎检测头","OF-A1","一体型 金属外壳 检测高温物体 接插光纤传导输出 IP67","CNS 12081-1987","只",6,"219厂部","2022-12-10"]
[53,6100900121,"智能控制柜","TDF-30H-3-S","内含主钩跟配电保护两个工作单元，采用一体化无触点装置，装置电源380V；无触点通断；正反转延时保护；缺相保护；偏流保护；智能散热，电流显示，HMI编程面板，柜体防护等级：IP65","JB/T8680-2008","台",1,"物流中心","2022-12-10"]
[54,6100900122,"智能控制柜","TDF-31H-3-S","内含四个大车的控制单元，采用一体化无触点装置，装置电源380V；无触点通断；正反转延时保护；缺相保护；偏流保护；智能散热，电流显示;HMI编程面板；柜体防护等级：IP65","JB/T8680-2008","台",1,"物流中心","2022-12-10"]
[55,6100900123,"智能控制柜","TDF-32H-3-S","内含小车与旋转小车的的控制单元，采用一体化无触点装置，装置电源380V；无触点通断；正反转延时保护；缺相保护；偏流保护；智能散热，电流显示;HMI编程面板；柜体防护等级：IP65","JB/T8680-2008","台",1,"物流中心","2022-12-10"]
[56,6100100218,"周向隔离变压器","SF-BA-24000AT-A/15.2KVA","380V/380V/40A/15.2KW；单相；F级绝缘",null,"台",1,"219厂部","2022-12-10"]
[57,6400500873,"可控硅控制板","SF-DPJ-85","CDW-24000AT磁粉探伤",null,"块",1,"219厂部","2022-12-10"]
[58,6400500874,"可控硅模块","MTT11OA/16E","It(av)=110A ； Vdrm/Vrrm=1600V",null,"只",3,"219厂部","2022-12-10"]
[59,6400500875,"可控硅模块","MTT20OA/16E","It(av)=2000A ； Vdrm/Vrrm=1600V",null,"只",3,"219厂部","2022-12-10"]
[60,6400200026,"反光镜","SW50 1000131","高温反射器，玻璃，可旋紧：直径 50 mm：运行环境温度≤ +300 ℃","DIN EN 61757-1-2013","块",18,"340/180/89热轧","2022-12-10"]
[61,6600300021,"阀门定位器","YT-1000RDn13201","输入信号4-20mA 供气压力 1.4-7.0kgf/c㎡cm 工作温度 -20-70℃ 双作用 内置PTM","JB/T8219-1999","台",2,"180厂部","2022-12-10"]
[62,6600300031,"阀门定位器","YT-1000RD 13","输入:4-20mA/DC","JB-T8219-1999","只",2,"720厂部","2022-12-10"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2022年9月电气备件采购项目Ⅱ        项目编号：HGCGD22122"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":4,"n_cols":1,"rows_kept":4,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8]],"flags":["formulas_cached_only"]}
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]