{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":50,"n_cols":13,"rows_kept":50,"merged":[[0,0,0,8],[1,0,1,12],[46,0,46,8],[47,0,47,8],[48,0,48,8],[49,0,49,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2022年9月机械配件采购项目                     项目编号：HGCGD22123"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,6700200044,"冲击试验机 硫化氢减压阀 R11LG-EGG-00-00","R11LG-EGG-00-00",null,"只",1,"JB/T10365-2002","检验检测中心","2022-11-26"]
[2,7001200343,"高压泵连杆","3D-250-0102",null,"根",4,null,"219厂部","2022-11-26"]
[3,5701600186,"双柱式强力带锯床","G4230/50B","锯条规格3920*34*1.1","台",1,"JB/T4318.3-1996","89油管热处理","2022-11-26"]
[4,5702000063,"充水阀","18Q00601.01.05","装配件;185kg;配安装螺栓。","件",1,"审核图纸","89油管热处理","2022-11-26"]
[5,5702000062,"排气阀","18Q00601.02.02","装配件;164.9kg;配安装螺栓。","件",1,"审核图纸","89油管热处理","2022-11-26"]
[6,5702000061,"控制阀组件","18Q00602.02.05.01","装配件;10.7kg","件",2,"审核图纸","89油管热处理","2022-11-26"]
[7,4201700122,"手推式自动行走洗地机","飞默普    IMX BT","洗地宽度 :510 毫米;吸水扒宽度:680 毫米;清水箱:40 升;污水箱:40 升;理论工作效率:2040 平米/小时  ;前进速度:0-4 千米/小时;最大爬坡度:10%;真空吸力:61  mbar;锂电池:24伏 / 100 安时;充满电连续工作时间:5 小时;机器重量(不含电池):76 千克;尺寸（长×宽×高）:1180×590×1030 毫米;标配附件:智能充电器1个、24伏/100安时锂电池1组、洗地盘刷1个;质保期限:整机质保12个月，锂电池质保3年","台",1,"EN60335-2-72","检验检测中心","2022-11-26"]
[8,5000400112,"蜗轮蜗杆斜齿轮减速机","SA92-1/100-YEJ4kW-6P-M1","传动比47.2;额定功率4Kw;配反力矩环板GST97-01QT K","台",2,"Q/ZTB04-2000","炼钢厂部","2022-11-26"]
[9,7102100009,"气动控制阀","Z014-A DN80 PN25",null,"只",8,"GB/T3452.1-1992","180厂部","2022-11-26"]
[10,6600300075,"气动调节阀","8-40200CSPS6GP2323","Bray","只",1,"GB/T4213-2008","180厂部","2022-11-26"]
[11,5501700003,"堆取料机;斗轮机构轴承座","D223A-11.0","ZG35 孔径50，轴向孔距145，径向孔距530，座低平面与孔中心线夹角5°侧端盖带注油孔M10","件",2,null,"原料工段","2022-11-26"]
[12,5400100103,"Ingersoll Rand螺杆空压机;空气过滤器","MXU250W-2S；No.39903265;","圆筒式折叠V型密褶式过滤器;玻璃纤维;过滤精度10um;使用寿命大于2000h；GB/T 6165-2008；","件",2,"GB/T 6165-2008","能源厂部","2022-11-26"]
[13,5400100102,"Ingersoll Rand;螺杆机;油过滤器","MXU250W-2S；No.92888262;","玻璃纤维;过滤精度;5μm-12μm;初始压差;≤0.03MPa;最大工作压力;1.4MPa-2.5MPa;使用寿命大于2000h；ANSI/ASTM F1567-1997","件",4,"ANSI/ASTM F1567-1997","能源厂部","2022-11-26"]
[14,7101800130,"气动球阀","DN150 ANSI 300 ASMEB16.5","铸钢 F30，CLASS ANSI300，ASTMA216WCB，A351 CF8M，STAINLESS316，ANSI 300 ASMEB16.5","只",1,null,"高辅工段","2022-11-26"]
[15,7100100089,"减压阀","DR30-1-30/315YM","ISO 4401","只",2,"GB2514-1987","180厂部","2022-11-26"]
[16,7100300398,"气动换向阀","MN1H-5/3G-D-3-C","3-10bar:FESTO","只",4,"FESTO","180厂部","2022-11-26"]
[17,7100100256,"安全阀","A48Y-25-65","压力等级1.3-1.6Mpa；整定压力1.32Mpa，DN65","只",1,"GB/T12243-2006","能源厂部","2022-11-26"]
[18,7100100254,"安全阀","A48Y-25-100","压力等级1.3-1.6Mpa；整定压力1.45Mpa，DN100","只",1,"GB/T12243-2005","能源厂部","2022-11-26"]
[19,7100100255,"安全阀","A48Y-25-80","压力等级1.3-1.6Mpa；整定压力1.45Mpa，DN80","只",1,"GB/T12243-2005","能源厂部","2022-11-26"]
[20,5716700094,"2号线脉冲烧嘴3","天燃气烧嘴SIO 800HB-150/135;150KW;","烧嘴含观火玻璃孔、点火电检、检测电极;内丝通径DN20;","套",5,"执行标准GB/T 35073-2018","管加工厂部","2022-11-26"]
[21,7502400138,"机床切削液专用混配器","Master Mix M-10","配比浓度0%~20%，流量38升/分，进水口1/2英寸，出水口3/4英寸，水压：2bar~4bar","套",2,"Q/MT 005-2016","管加工厂部","2022-11-26"]
[22,7101500060,"煤气调节阀","6-40200CSPS6GP2323",null,"只",1,"GB/T4213-2008","720厂部","2022-11-26"]
[23,5712300129,"气动活塞双偏心球面硬密封调节蝶阀","HB2414-J1222K","DN350","台",2,"GB/T4213-1992","180厂部","2022-11-26"]
[24,5500800015,"旋风除尘输灰机","DS100T-AZ","16Mn DS100T-AZ 含机壳.轴.轴承座、带防爆电机、减速机、螺旋叶片(耐磨合金 厚度12mm).，电机型号YB3-200L-4,30KW,转速1470r/min,电机轴直径110 搅拌叶片采用高铬抗磨铸铁，硬度HRC≥50壳体采用16Mn优质板材焊接而成 板厚12mm，焊缝采用坡口焊接 搅拌轴采用40Cr轴头和厚壁缝钢管焊接制作，喷水管材质采用1Cr18Ni9Ti 金属构件等应进行除锈，内表面采用防锈底漆两道，外表面采用防锈底漆两道，面漆两道。","套",1,null,"高炉","2022-11-26"]
[25,5502000036,"除尘耐磨输灰管","φ600*φ580","材质：NM400;介质：除尘灰;工作温度：50-200℃","吨",3,"DL/K680-2015","烧结","2022-11-26"]
[26,5502000034,"除尘耐磨输灰管","φ440*φ420","材质：NM400;介质：除尘灰;工作温度：50-200℃","吨",3,"DL/K680-2015","烧结","2022-11-26"]
[27,5502000035,"除尘耐磨输灰管","φ250*φ230","材质：NM400;介质：除尘灰;工作温度：50-200℃","吨",3,"DL/K680-2015","烧结","2022-11-26"]
[28,5602600067,"事故割炬","SG-II","图号QGJ-22;L=2400mm","把",4,"GB5108-1985","炼钢厂部","2022-11-26"]
[29,7101600168,"气动控制阀门","D376XE73;OMAL","DN125;OMAL;带执行器","台",2,"ISO5211","管加工厂部","2022-11-26"]
[30,4000300241,"轴承座","HX110(GB/T2563-2007);轴承座材质ZG270-500；","带铜瓦；润滑油口M10*1；","套",10,"审核图纸","管加工厂部","2022-11-26"]
[31,5400100140,"螺杆空压机 进气阀总成","ZL2508214","材质：铸铁，带气缸及连接管道","套",1,"GB/T24738-2009","能源厂部","2022-11-26"]
[32,7001900049,"喷码机滑轮","D2312","原装厂家：厦门德瑞雅喷码科技有限公司","只",1,null,"720厂部","2022-11-26"]
[33,5501100052,"智能振打装置","ZGD1500","电压380~220V,电流2.2A,频率50HZ,振动力15KN,重量153kg，安装尺寸长600*宽350*高550","套",6,"JB/T1038.3-2016","烧结","2022-11-26"]
[34,6400500876,"蓝色油墨","LLY-1","适应1.0mm喷枪；适应标准GB/T1723-1993","桶",20,"GB/T1723-1993","180厂部","2022-11-26"]
[35,5714900003,"螺旋升降机","268.27SB040324-45 SWL25M-1AⅣ-100FZ","组件 76Kg","台",2,null,"720厂部","2022-11-26"]
[36,5712400006,"42100带锯机 右导向爪装配","G42100B-04300-04302",null,"套",2,null,"720厂部","2022-11-26"]
[37,5712400010,"42100带锯机 左导向爪装配","G42100B-04300-04301",null,"套",2,null,"720厂部","2022-11-26"]
[38,5501400007,"烧结;成品仓振动给料机","QZS-80-130F 不带电机；面宽800mm，长1300mm","铆焊","台",4,"JB/T8096-2013","烧结","2022-11-26"]
[39,5000600019,"螺旋升降机","SWL25L-1AⅢ-1000(F)Z","带电机","台",2,"JB/T8809-1998","管加工厂部","2022-11-26"]
[40,5300200063,"圆柱齿轮减速机","ZSC650-IV-2i=51.7",null,"台",1,"JB/T8853-2001","物流中心","2022-11-26"]
[41,5300200061,"圆柱齿轮减速机","ZSC50-Ⅲ-1i=33.1",null,"台",1,"JB/T8853-2001","物流中心","2022-11-26"]
[42,5712300125,"气动活塞双偏心密封调节(切断)蝶阀","HB2412","DN150 WCB 气开 流量系数1300","只",1,"GB/T4213-1992","340热轧","2022-12-11"]
[43,5712300132,"气动活塞双偏心硬密封调节切断蝶阀","HB2414","DN300 304 流量系数5100","只",1,null,"340热轧","2022-12-11"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2022年9月机械配件采购项目                     项目编号：HGCGD22123"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":4,"n_cols":1,"rows_kept":4,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8]],"flags":["formulas_cached_only"]}
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]