{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":48,"n_cols":13,"rows_kept":48,"merged":[[0,0,0,8],[1,0,1,12],[44,0,44,8],[45,0,45,8],[46,0,46,8],[47,0,47,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2022年10月机械备件采购项目                     项目编号：HGCGD22131"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,5712300126,"气动活塞双偏心球面硬密封调节蝶阀","HB2414-E12222K","PN0.6MPa","只",1,"GB/T4213-1993","720厂部","2022-12-27"]
[2,6600300017,"气动活塞调节(切断)蝶阀","HB2416-16 912158 DN100 WCB 带全套附件","DN100 PN0.6MPa","套",1,"GB/T4213-1992","720厂部","2022-12-27"]
[3,7502500099,"离心通风机","9-28;5.6A","30Kw;右旋0°","台",2,"GB/T13274-1991","炼钢厂部","2022-12-27"]
[4,5707700036,"切管机 进刀油缸总成","QGB1130","铸件","台",1,"审核图纸","219厂部","2022-12-27"]
[5,5501700003,"堆取料机;斗轮机构轴承座","D223A-11.0","ZG35 孔径50，轴向孔距145，径向孔距530，座低平面与孔中心线夹角5°侧端盖带注油孔M10","件",2,null,"原料工段","2022-12-27"]
[6,5712400006,"42100带锯机 右导向爪装配","G42100B-04300-04302",null,"套",2,null,"720厂部","2022-12-27"]
[7,5712400010,"42100带锯机 左导向爪装配","G42100B-04300-04301",null,"套",2,null,"720厂部","2022-12-27"]
[8,5501400007,"烧结;成品仓振动给料机","QZS-80-130F 不带电机；面宽800mm，长1300mm","铆焊","台",4,"JB/T8096-2013","烧结","2022-12-27"]
[9,7100300398,"气动换向阀","MN1H-5/3G-D-3-C","3-10bar:FESTO","只",4,"FESTO","180厂部","2022-12-27"]
[10,7502400138,"机床切削液专用混配器","Master Mix M-10","配比浓度0%~20%，流量38升/分，进水口1/2英寸，出水口3/4英寸，水压：2bar~4bar","套",2,"Q/MT 005-2016","管加工厂部","2022-12-27"]
[11,6700200044,"冲击试验机 硫化氢减压阀 R11LG-EGG-00-00","R11LG-EGG-00-00",null,"只",1,"JB/T10365-2002","检验检测中心","2022-12-27"]
[12,7001200343,"高压泵连杆","3D-250-0102",null,"根",4,null,"219厂部","2022-12-27"]
[13,7101600032,"气动控制阀门","D376XE74",null,"只",2,"JB/T6375-1992","180厂部","2022-12-27"]
[14,7101600191,"气动控制阀门","D376XE75","DN200","台",2,"ISO5211","180厂部","2022-12-27"]
[15,6600300106,"气动控制阀","FV-302B;600S;100A*100A","Pn0.6MPa;CV=278;行程90度;KOSO","台",2,"GB/T4213-2008","720厂部","2022-12-27"]
[16,5722600094,"带锯床导向臂","G4250/70;","材料ZG310-570；  重量28kg;","对",4,"JB/T8853-1999","管加工厂部","2022-12-27"]
[17,5400300008,"煤气冷凝水排水器","SDLT-4000-100","Q235 GB6222","台",2,"GB6222","高辅工段","2022-12-27"]
[18,5712300125,"气动活塞双偏心密封调节(切断)蝶阀","HB2412","DN150 WCB 气开 流量系数1300","只",1,"GB/T4213-1992","340热轧","2022-12-27"]
[19,7200400080,"带锯机;夹紧油缸;G4250/85","G4250/85","压力等级：25MPa；采用进口密封；连接螺栓12.9级","台",3,"JB/T11588-2013","管加工厂部","2022-12-27"]
[20,5300300383,"GKIC0262机车 喷油泵","6240ZJ","S=20mm","只",8,null,"物流中心","2022-12-27"]
[21,5701600053,"预热式烧嘴换热器","SINMAX2M/C545","60kW","只",3,null,"89厂部","2022-12-27"]
[22,5701600056,"预热式烧嘴陶瓷燃烧室","SINMAX2M/C545",null,"只",4,"GB/T21944.4-2009","89厂部","2022-12-27"]
[23,5701600036,"燃气式高温陶瓷管二","*","L=200mm","根",4,null,"89厂部","2022-12-27"]
[24,5701600038,"燃气式高温陶瓷管三","*","L=300mm","根",24,null,"89厂部","2022-12-27"]
[25,5705300024,"G4240X50卧式带锯床；可移动夹紧虎钳","滚珠丝杆横移距离200mm，夹钳夹持长度420mm。中心高230mm。","滚珠丝杆横移距离200mm，夹钳夹持长度420mm。中心高230mm。G4240X50带锯机使用，与其原尺寸及结构保持一致。","套",1,null,"检验检测中心","2022-12-27"]
[26,5602600067,"事故割炬","SG-II","图号QGJ-22;L=2400mm","把",4,"GB5108-1985","炼钢厂部","2022-12-27"]
[27,4000300241,"轴承座","HX110(GB/T2563-2007);轴承座材质ZG270-500；","带铜瓦；润滑油口M10*1；","套",10,"审核图纸","管加工厂部","2022-12-27"]
[28,5501400034,"烧结;A2筛筛板(二)","HBS2050(TTHBS-450-1)-b","上层棒条直径16mm，长度270mm，间距25mm；下层棒条直径16mm，长度320mm，间距16mm；棒条材质HBZL-5CrSiV；棒条布置角度16°","件",1,null,"烧结","2022-12-27"]
[29,5501400035,"烧结;A3筛筛板(三)","HBS2050(TTHBS-450-1)-c","上层棒条直径9mm，长度260mm，间距6mm；下层棒条直径7mm，长度210mm，间距4mm；棒条材质HBZL-5CrSiV；棒条布置角度15°","件",1,null,"烧结","2022-12-27"]
[30,5501400036,"烧结;A1筛筛板(一)","HBS2050(TTHBS-450-1)-a","上层棒条直径16mm，长度270mm，间距16mm；下层棒条直径13mm，长度320mm，间距12mm；棒条材质HBZL-5CrSiV；棒条布置角度18°","件",1,null,"烧结","2022-12-27"]
[31,5712000134,"直线导轨滑块","JSA-LG45KL","滚动轴承座材质：: 轴承钢;装配后组合尺寸：H:62mm、W:37.5mm;滑块尺寸:120*51*15*25*10","块",10,"GB/T4250","340热轧","2022-12-27"]
[32,5000300123,"SEW减速器","M3PSF70，i=50，输入输出轴双轴伸，输入功率：N=132KW，输入转速：n=1480r/min，带散热风扇","运行功率132KW，使用系数2.29，传动比1:48.7384，重量1676KG，转速1480/30.4r/min","台",2,"JB/T8853-1999","高辅工段","2022-12-27"]
[33,7101600218,"气动开关蝶阀","Z011-A-PN16-DN300","阀体材质:球墨铸铁GGG-40;阀板材质;不锈钢1.4408;阀杠材质;2Cr13;阀座密件;EPDM;连接方式;对夹;阀板工作压力;16bar","只",3,"GB/T8100-2006","炼钢厂部","2022-12-27"]
[34,5712300132,"气动活塞双偏心硬密封调节切断蝶阀","HB2414","DN300 304 流量系数5100","只",1,null,"340热轧","2022-12-27"]
[35,5600300010,"90t电炉;EBT出钢机构","*",null,"套",1,"受控图纸","炼钢厂部","2023-02-10"]
[36,5500300110,"全封闭型钢制拖链架","TLE125Ⅲ-250x300x5200","250x300x5200 材质：铝合金组件","套",1,"JB/T12471-2015","高炉","2022-12-27"]
[37,7502400141,"加药搅拌轴及叶轮","750-32","搅拌轴：304不锈钢材质，直径32mm,长度：1200mm，实心；三叶叶轮：不锈钢材质，内孔Φ32mm，外直径Φ750mm，厚度6mm","套",2,null,"340热轧","2022-12-27"]
[38,5719700002,"PP袋式污水过滤袋","180*810-150微米--2号；","过滤精度：150μm；过滤面积：0.5㎡；最大流量：40m3/h ；袋口固定环：镀锌钢圈","只",50,"GB12625-1990","管加工厂部","2023-01-26"]
[39,7102600084,"电动调节阀","RXDF-1v","公称压力：1.6MPa，通径50mm，阀体材质：ZG230-450,滤芯材质OCr 18Ni 9,带配套电动执行机构","台",1,"TS-2743018-2022","能源厂部","2022-12-27"]
[40,5501200134,"柔性翻板式新型双层卸灰装置","JYXF300×1800","\"驱动方式：下阀板分别由单个独立液压缸驱动；液压站（含滤油器+缓冲装置）：电机功率：2.2KW   厂家：节能高效电机\n油泵：康百世齿轮泵   ；密封件材质：橡胶软密封（耐温200℃）；工作压力：16Kpa～20Kpa；物料堆重比：2.2t/m3；漏风率：≤0.05%\"","套",2,"审核图纸","烧结","2022-12-27"]
[41,5603200033,"布袋","D120*4402","纤维;玄武岩/PI;克重>750g/m2;厚度1.2mm;透气量6m3/m2/min@12.5mmH20;后处理;PTFE乳液浸渍处理","条",166,"GB12625-1990","炼钢厂部","2022-12-27"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2022年10月机械备件采购项目            项目编号：HGCGD22131"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":4,"n_cols":1,"rows_kept":4,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8]],"flags":["formulas_cached_only"]}
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]