{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":57,"n_cols":12,"rows_kept":57,"merged":[[0,0,0,11],[1,0,1,11],[53,0,53,8],[54,0,54,8],[55,0,55,8],[56,0,56,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2022年10月电气备件采购项目                    项目编号：HGCGD22133"]
["序号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家"]
[1,6200200205,"变频器","20G11NC072JA0NNNNN 37Kw PowerFIex755","进线电压：3相 380V-480VAC 额定功率37KW 重载功率30KW 额定电流72A",null,"台",2,"管加工厂部","2023-01-10"]
[2,6200200055,"变频器","20BC011A3AYNANCO 5.5Kw/4Kw AB E0.967X","E0.969X","E0.967X","台",1,"高炉","2023-01-10"]
[3,6400400036,"绝对编码器","CEV65M-01460 ELECTRONIC GMBH","输出方式: （绝对式}：工作电压: 11-27vDC：防护等级(IP66)：Nr 1358438","DIN 32878-1993","只",2,"180厂部","2023-01-10"]
[4,6600300020,"阀门定位器","YT-1000RDM132SOO","输入信号4-20mA 供气压力 1.4-7.0kgf/c㎡cm 工作温度 -20-70℃ 双作用","GB/T9248-1999","只",4,"管加工厂部","2023-01-10"]
[5,6400200026,"反光镜","SW50 1000131","高温反射器，玻璃，可旋紧：直径 50 mm：运行环境温度≤ +300 ℃","DIN EN 61757-1-2013","块",8,"340热轧","2023-01-10"]
[6,6100300268,"分闸线圈","ZN5","DC220V,线径0.31mm，匝数3660，","GB/T14048","个",5,"能源厂部","2023-01-10"]
[7,6100400164,"电位器","WX03-4.7K",null,"GB/T 11210-1989","只",20,"管加工厂部","2023-01-10"]
[8,6400400052,"主轴编码器","IRS660-1024-826","IEC 61131-3","IEC 61131-3","只",2,"管加工厂部","2023-01-10"]
[9,6300500046,"安全继电器","PNOZ XV3 30SEC","24VDC",null,"块",1,"340热轧","2023-01-10"]
[10,6100500380,"时间继电器","H3YN-2 TIMER","AC200-230V ;50/60HZ;8针","GB14048.5","只",20,"180厂部","2023-01-10"]
[11,6400400122,"编码器","GHU9-30//5G39//1024G//3R","增量型编码器;UB:+9～30V,脉冲数1024 HTL;IP67;法国艾迪克","EN 60947-5-2","只",1,"炼钢厂部","2023-01-10"]
[12,6100600260,"熔断器","NGT1;1000V,100A","1000V,100A","IEC269;GB13539","个",6,"720厂部","2023-01-10"]
[13,6600200123,"阀门定位器","EPA814","输入 4-20mA/DC，气源:8Kgf/cm2 8Bar 最大120Psi 800KPa","JB/T8219-2000","只",4,"219厂部","2023-01-10"]
[14,6400600504,"超声波传感器","UM30-13111","工作电压12-30VDC ;模拟输出4-20mA；感应距离30-1300mm; 防护等级(IP67) 5针M12插头","DIN EN 62365-2010","只",3,"180厂部","2023-01-10"]
[15,5300300359,"GK1C机车 空气压缩机直流电机","ZTP-82","110V 238A","JB/T2785-2010","台",1,"物流中心","2023-01-10"]
[16,6100900050,"控制柜","2000*800*800;标准",null,null,"台",2,"340热轧","2023-01-10"]
[17,6400200087,"光电开关","V2R-1200DP","电源：DC10-30V 10%；检测距离：0.01-12M；电流：35mA以下；环境温度：-25-55℃；品牌：日本奥普士","JB/T 6475-1992","个",30,"340热轧","2023-01-10"]
[18,6600300046,"全电子式电动执行器","LSDZ-2000","电源220VAC输出4-20mA 反馈4-20mA 动作时间50S 转角90度 输出力矩2000N.m","JB/T8219-1999","台",1,"炼铁厂部","2023-01-10"]
[19,6300400027,"电源模块","1756-PA72/C AB","输入电压额定值120/220VAC 100W 输出5.1VDC/10.0A,24VDC/2.8A,3.3VDC/4.0A,1.2VDC/1.5A 标准IEC61508","IEC61508","块",5,"219厂部","2023-01-10"]
[20,6300100046,"处理器","1756-L61 AB","标准IEC61508","IEC61508","块",1,"89油管车丝委外","2023-01-10"]
[21,6200200391,"软起动器","150-B240NBDB AB 升级为150-F251NBD","输入电压3AC 380V 功率250Kw 允许电动机最大电流435A","IEC947","台",1,"89热轧","2023-01-10"]
[22,6600100242,"专用电池","数显游标卡尺专用电池",null,"GB/T 4844.1-1995","瓶",20,"180厂部","2023-01-10"]
[23,6400600419,"激光测距仪","OSM160-RPL40PN6L","电源16-30VDC/max200mA:测量范围0.2-40m:精度±2mm:重复精度0.3mm;测量输出时间2ms:分辨率可调整:profibus预设1mm,SSI预设0.1mm","IEC 60947-5-1","台",1,"炼钢厂部","2023-01-10"]
[24,4100400212,"耐热套管","FDA-1","25mm","FDA标准","米",100,"炼钢厂部","2023-01-10"]
[25,6400400132,"绝对值编码器","CEV65M-27010  ;TR","steps：4096；Revolution:4096；Pinout：2293A;Interface：SSI;Supply Voltage：11-27V;带金属防护外壳","符合标准DIN EN 61000-6-4，DIN EN 61000-6-2","台",1,"219厂部","2023-01-10"]
[26,6400400019,"绝对编码器","CEV115M TR D-78647","绝对值型 金属外壳 外形尺寸115mm 侧向12针插头连接 SSI输出 Nr.CEV115-10021 Sn:0012 11-27vdc Pruif Nr.1300743 08063 符合标准DIN EN 61000-6-4，DIN EN 61000-6-2","D-78647","只",1,"219厂部","2023-01-10"]
[27,6200300015,"平波电抗器","500Kw 700A 575V 5mH 1000HZ","500Kw 700A 575V 5mH 1000HZ","GB/T1094.6-2011","台",1,"89油管车丝委外","2023-01-10"]
[28,5300300719,"机车用车载台话筒","ZTD-8型",null,null,"只",6,"物流中心","2023-01-10"]
[29,6300600080,"直流电源","BPS2501R2","INPUT:SHORT AC100/120V 50/60HZ 6.0A OPEN AC 200/240V 50/60HZ 3.0A OUTPUT:DC 250V 1.2A","IEC61509","台",1,"89油管车丝委外","2023-01-10"]
[30,6300600078,"喷码机主控板","PMC-PJ1A","IC4-2216-J主控板","IEC61509","块",1,"89油管车丝委外","2023-01-10"]
[31,6200100035,"直流调速装置","DCM-CON70-V 0","四相限控制 带profibus-dp通讯板 小装置控制大功率晶闸管整流装置 带励磁控制单元220V,39A 晶闸管主回路直流输出电压DC850V 额定输出直流电流3162A，直流电机带编码器速度反馈，可弱磁升速。",null,"套",1,"219厂部","2023-01-10"]
[32,4100500083,"空气开关","CM1-225H/3300；","250A","GB/T 6170-2000","只",5,"管加工厂部","2023-01-10"]
[33,5300100969,"天车超重限载器套件","QCX-M-5t+5t（带双传感器及8寸大屏显示器）","带2个5t传感器及8寸显示屏；","GB14048","套",2,"89油管车丝委外","2023-01-10"]
[34,6100700022,"电流互感器","HDC-800F","800A,4V","GB1208-2006","只",2,"炼钢厂部","2023-01-10"]
[35,6200100095,"变频器","MD480T18.5GB","功率18.5Kw;输入3PH AC 380-480V 49.5A 50Hz;输出3PH AC 0-480V 37.0A 0-500Hz","EN61800-3","台",1,"炼钢厂部","2023-01-10"]
[36,6400600511,"磁致伸缩线性位移传感器","KYDM-LGS-GC0355J-TS","电源:24VDC, 输出:4-20mA,防护等级:IP65，量程：355mm;精度：0.05%F.S","GB/T14048","套",3,"炼铁厂部","2023-01-10"]
[37,6400600510,"磁致伸缩线性位移传感器","HT-SGLBDM241260KOS","电源:24VDC, 输出:4-20mA,防护等级:IP65，量程：260mm;精度：0.05%F.S","GB/T28857-2012","套",2,"炼铁厂部","2023-01-10"]
[38,6100900132,"10KV成套高压开关柜","KYN28A-12","1、采用南自线路保护装置（ PSL641UX）；2、真空断路器采用库柏耐吉（VN3-12/2500-31.5），额定电流：2500A，短路断电流：31.5kA；3、屏柜操控装置：DN6700/HS2/X/DC220/Z；4、操作电源：直流220V；5、电流互感器：LZZBJ15-10，变比2500/5A，0.2/0.5/10p10/10p20，户内；6、三相电子式多功能电能表，DSSD331长沙威胜；7、氧化锌避雷器：HY5WS-17/50；8、母线套管3只（100*10的双铜排）；9、提供并现场制作搭接母线主铜排（100*10*2）；10、提供与VN3-12/2500断路器转运小车1台","GB 3906-2006","台",1,"能源厂部","2023-01-10"]
[39,6400600509,"位移传感器","RHM0260MD701S2G1100","MTS R系列SSI；带定位磁环、附件及10m电缆","GB/T 28857-2012","只",1,"720厂部","2023-01-10"]
[40,6600200846,"无功补偿控制器","JKW1A-12","无功功率补偿柜用，12路输出，线包供电电压AC220/380v，带LED显示,具备手自动切换功能，A\\B相测压，C相测电流，原厂家温州清华电子工程有限公司，生产编号081205287102","DL-T597-1996","台",6,"720厂部","2023-01-10"]
[41,6100500413,"热过载继电器","TGR36-32","AC-15;lth:5A;Ue:380V;le:0.47A;脱扣级别：10A;厂家：浙江天正电气股份有限公司","GB/T 14048.4","个",3,"340热轧","2023-01-10"]
[42,6100900133,"无线遥控开关器控制箱","380V 4KW","工作电压：380V;有效距离：3000米;额定功率：4KW;频率:35HZ;开关箱带无线遥控发送、接收器一套，控制器一个，断路器一个，接触器一个，保护器一个；带手动+遥控两种模式,缺相保护、过载保护、短路保护功能","JB/T8219-1999","个",5,"340热轧","2023-01-10"]
[43,6200200159,"变频器","20BC105A0AYNANC0 E0.967X","55Kw 105A 400VAC AB","E0.967X","台",1,"炼铁厂部","2023-03-12"]
[44,6200200215,"变频器","20BC037A3AYNANCO 18.5Kw/15Kw AB",null,"GB/Z22720.2-2013","台",1,"炼铁厂部","2023-03-12"]
[45,6200200875,"伺服驱动器","A06B-6140-H006","输入：200-240V ~26A 50Hz/60Hz ；输出：283-339V~6.8KW","EN50178 UL508C","块",1,"检验检测中心","2023-01-10"]
[46,6200200876,"伺服驱动器","A06B-6117-H304","输入：283-339V ~9.5KW；输出：240V；输出电流：L axis 6.5A，M axis 6.5A ，N axis 13A","EN50178 UL508C","块",1,"检验检测中心","2023-01-10"]
[47,6100300292,"马达保护器","GV3P40","30-40A","IEC60947-2","个",1,"检验检测中心","2023-01-10"]
[48,6300300050,"同步模块","1757-SRM B F/W REV2.22 AB",null,"JB/T4333-2013","块",2,"炼铁厂部","2023-01-10"]
[49,6400600498,"位移传感器","RH5MA0620M01R031A100","MTS公司产品，R系列模拟量，带定位磁环、附件及3mPVC电缆，电压24VDC，输出电流4－20MA",null,"只",1,"219厂部","2023-01-10"]
[50,6400500033,"探伤机 荧光磁粉","1KG/瓶","HLY-20 附合格证","GB/T15822.2-2005","瓶",200,"管加工厂部","2023-01-11"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2022年10月电气备件采购项目        项目编号：HGCGD22133"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":4,"n_cols":1,"rows_kept":4,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8]],"flags":["formulas_cached_only"]}
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]