{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":84,"n_cols":12,"rows_kept":84,"merged":[[0,0,0,11],[1,0,1,11],[80,0,80,8],[81,0,81,8],[82,0,82,8],[83,0,83,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2022年12月电气备件采购项目                    项目编号：HGCGD22146"]
["序号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家"]
[1,6200100035,"直流调速装置","DCM-CON70-V 0","四相限控制 带profibus-dp通讯板 小装置控制大功率晶闸管整流装置 带励磁控制单元220V,39A 晶闸管主回路直流输出电压DC850V 额定输出直流电流3162A，直流电机带编码器速度反馈，可弱磁升速。",null,"套",1,"219厂部","2023-01-27"]
[2,6400400132,"绝对值编码器","CEV65M-27010  ;TR","steps：4096；Revolution:4096；Pinout：2293A;Interface：SSI;Supply Voltage：11-27V;带金属防护外壳","符合标准DIN EN 61000-6-4，DIN EN 61000-6-2","台",1,"219厂部","2023-01-27"]
[3,5300100969,"天车超重限载器套件","QCX-M-5t+5t（带双传感器及8寸大屏显示器）","带2个5t传感器及8寸显示屏；","GB14048","套",2,"89油管车丝委外","2023-01-27"]
[4,7500500115,"喷标机 油漆过滤器","62.5L-LPH-SL-100-N2",null,"JB/T8679-1998","件",10,"89油管热处理","2023-01-27"]
[5,6100500382,"中间继电器","JZX-22F/4Z","AC220V，3A，4开4闭，14脚，无底座","GB/T14048.1-2006","只",20,"物流中心","2023-01-27"]
[6,6300600079,"喷码机驱动板","BP11-43","IC4-2216-J 驱动板","IEC61509","块",1,"89油管车丝委外","2023-01-27"]
[7,6300300148,"PLC模块","1756-IF8;AB",null,null,"块",2,"219厂部","2023-01-27"]
[8,6400300053,"接近开关","LJ18A3-8-J/EZ AC90-250V",null,"GB/T14048.10-2008","只",3,"检验检测中心","2023-01-27"]
[9,6700200056,"系列摆锤式冲击试验机 电磁铁","ZBC2000-C",null,null,"只",2,"检验检测中心","2023-01-27"]
[10,6700200063,"万能试验机 拉线位移传感器","RLX50A-1500mm-0.04","JJF1305-2011","JJF1305-2011","只",2,"检验检测中心","2023-01-27"]
[11,6100500044,"时间继电器","H3Y－2PYF08A DC24V 0.5？1S",null,"GB/T 14598.1-2002","只",5,"检验检测中心","2023-01-27"]
[12,6100500075,"中间继电器","RJ25-CL-D24 DC24V RU2S","IEC61810-1","IEC61810-1","只",5,"检验检测中心","2023-01-27"]
[13,6200200875,"伺服驱动器","A06B-6140-H006","输入：200-240V ~26A 50Hz/60Hz ；输出：283-339V~6.8KW","EN50178 UL508C","块",1,"检验检测中心","2023-01-27"]
[14,6200200876,"伺服驱动器","A06B-6117-H304","输入：283-339V ~9.5KW；输出：240V；输出电流：L axis 6.5A，M axis 6.5A ，N axis 13A","EN50178 UL508C","块",1,"检验检测中心","2023-01-27"]
[15,6400300202,"接近开关","FBM-30D20P1-D3","工作电压10-30VDC;感应距离20mm;PNP型;电感式传感器;齐平安装;全金属圆柱形带螺纹外壳;外形尺寸30mm;常开模式;3线式",null,"个",10,"89油管车丝委外","2023-01-27"]
[16,6400600326,"行车遥控发射接收器","F24-60",null,null,"套",1,"219厂部","2023-01-27"]
[17,5300100231,"触发板","KTC3-2",null,"Q/IRKJ1-2010","块",1,"219厂部","2023-01-27"]
[18,6400600512,"位移传感器","CI43-6-1BR01T13000SA4201A","电源DC24V,输出4-20MA，电缆直接","Q/JT01-2011","支",1,"219厂部","2023-01-27"]
[19,6100100219,"干式整流变压器","ZSG-11KVA","输入电压380V/3，输出电压170/190V，接线方式Y/DY","JB4315-1986","只",1,"219厂部","2023-01-27"]
[20,5400100141,"DF-12机车:空压机调速器","704-I型","压力范围200-1200kpa, 压差范围80-300kpa","TB/T2630-1995","个",3,"物流中心","2023-01-27"]
[21,6100300293,"万能式断路器","DW15-2500","额定电压1140v，50hz，额定电流2500A，额定极限短路分断能力25KA,额定运行短路分断能力20KA,长延时0.7-1In，0.4s瞬时3-6In，欠压脱口器分励脱口器储能电动机电压均为交流220v；断路器尺寸需与现有使用的一致。原厂家：浙江正泰电器股份有限公司","GB14048.2","台",1,"219厂部","2023-01-27"]
[22,6300500241,"UPS电源","SP20KL-31P","输入电压：交流380V；输出电压：交流220V；输出功率：20KVA/18KW；持续供电60分钟；尺寸：576×250 ×592；带故障, 负载容量, 电池容量, 旁路, 市电模式, 电池模式, 电池故障, 过载显示功能；配套电池：12V65AH（松下）20只；电池柜：A20,尺寸：959× 470 ×1210。",null,"套",2,"219厂部","2023-01-27"]
[23,6400600343,"压力传感器","KY-B2003G12M1P2C1","150Mpa,精度0.5%;10-30VDC,4-20mA,防护等级IP65","GB/T15768-1995","个",5,"89油管车丝委外","2023-01-27"]
[24,6700400264,"点火电极","C5500I-02-05，品号212009025","每套2件，由长电极和中心电极组成；5E-KCIII量热仪专用","JJG672-2018","套",1,"检验检测中心","2023-01-27"]
[25,6300300150,"模拟量模块","TIF-08AD-1","Number of Channels:8,single ended(1 common);Input Ranges:0-20mA,4-20MA,-20 to20mA;Resolution:14bit(13 bit plus sign bit);Input Resistance:250 Ω","IEC 1000–5–1&2 /IEC 1131–4.","个",1,"检验检测中心","2023-01-27"]
[26,6200200879,"变频器","DP200-4T075B","输入：AC3PH 390V 50/60Hz，输出：0-400V 75A","IEC/EN 61800-5-1 IEC/EN 61800-3","台",1,"检验检测中心","2023-01-27"]
[27,6300700069,"数控车床总线系统面板","K100T-Ci","工作电源AC220V，7英寸液晶屏，面板尺寸400*245，横式安装","GB/T 23567.2-2018    GB/T 23567.3-2018","台",1,"检验检测中心","2023-01-27"]
[28,6200200882,"数控车床主轴伺服控制器","ZD011-43P7-E2","输入380V，输出0-400V，7kVA 9A","GB2828-2003","台",1,"检验检测中心","2023-01-27"]
[29,6200200881,"数控车床伺服控制器","KND SD200-20","输入单相或三相220V，输出110V","GB2828-2003","台",1,"检验检测中心","2023-01-27"]
[30,6200200883,"数控车床伺服控制器","GR2000系列GR2045T","输入三相220V，额定输出电流14A","GB2828-2003","台",1,"检验检测中心","2023-01-27"]
[31,6200200880,"变频器","EM500-4R0G/5R5P-3B","输入三相380V，额定功率4KW/5.5KW，额定电流9.4A/12A","IEC/EN 61800-5-1 IEC/EN 61800-3","台",1,"检验检测中心","2023-01-27"]
[32,6400400163,"旋转编码器","HMD1-1505AC10-30E900B0.25M-S5-C1","电源10-30VDC，输出电路E，最大转速6000r/m，最大径向负载40N，最大轴向负载20N","Q/DXJ 325-2019","个",1,"检验检测中心","2023-01-27"]
[33,6400400164,"旋转编码器","OVW2-36-2MHC","外型尺寸：Ф38×30；轴径：Ф6/D型切口；脉冲数：60P/R-3600P/R，电压：5-12V或12-24V；输出信号：A相.B相.Z相，输出形式：开放集电极输出、电压输出、推拉输出、PNP型开放集电极输出长线驱动推拉输出；8、最高响应频率：200KHZ，最高转速：6000r/min，保护等级：IP50，使用温度：-10℃+70℃","Q/DXJ 325-2019","个",1,"检验检测中心","2023-01-27"]
[34,6400600516,"行车超载限制器","QCX-HL（5T）","工作电压AC380V，工作方式：常闭","TSG Q7014-2008","个",1,"检验检测中心","2023-01-27"]
[35,6200300094,"箱式电阻炉","炉膛尺寸(深×宽×高)：400×200×160mm","1、最高温度：1400℃，，长期工作温度：≤1350℃；2、电源及功率：AC380V/10KW；3、炉膛尺寸(深×宽×高)：400×200×160mm；4、测温：铂铑（S分度号）热电偶+精密数显程序控温仪；5、控温：可控硅移相调压+智能PID调节+程序升降温，控温精度：±1℃；6、发热元件：硅碳棒。","JJF1376-2012","台",1,"检验检测中心","2023-01-27"]
[36,6300400011,"PLC 电源模块","1756-PA72","AB","GBT15969","块",2,"管加工厂部","2023-01-27"]
[37,6100900050,"控制柜","2000*800*800;标准",null,null,"台",2,"340热轧","2023-01-27"]
[38,6100400164,"电位器","WX03-4.7K",null,"GB/T 11210-1989","只",20,"管加工厂部","2023-01-27"]
[39,6100500380,"时间继电器","H3YN-2 TIMER","AC200-230V ;50/60HZ;8针","GB14048.5","只",20,"180厂部","2023-01-27"]
[40,6100500412,"热继电器","JR36-20(1-1.6A)","电流范围1-1.6A","GB/T14048.4","只",5,"炼钢厂部","2023-01-27"]
[41,5300101069,"行车应答器","FK-GD","工作电压:AC220V 50HZ；输出接点:常开常闭各1组；报警声音:语音、蜂鸣或音乐；工作状态显示:高亮LED；材质:主机钢板喷塑，控制开关铸铝",null,"台",12,"炼钢厂部","2023-01-27"]
[42,6100600260,"熔断器","NGT1;1000V,100A","1000V,100A","IEC269;GB13539","个",6,"720厂部","2023-01-27"]
[43,6600100242,"专用电池","数显游标卡尺专用电池",null,"GB/T 4844.1-1995","瓶",20,"180厂部","2023-01-27"]
[44,6200200419,"调压调速晶闸管模块","MTC-100/1600","dv/dt=1000V","Q/IRKJ1-2010","块",10,"720厂部","2023-01-27"]
[45,6100500403,"中间继电器","DZY-210","DC220V；嵌入式","GB/T22387-2008","只",5,"能源厂部","2023-01-27"]
[46,4100800046,"主令控制器","XKD-F12420420",null,"GB/T 23637--2009","台",2,"管加工厂部","2023-01-27"]
[47,4100800047,"主令控制器","XKD-F12520210",null,"GB/T 23637--2009","台",2,"管加工厂部","2023-01-27"]
[48,6400200060,"光敏开关","AS20-220V；RMSCSH","现场照明灯采用光控开关 输入/输出电压220V 路灯光控开关 塑料白色外壳 圆锥型","IEC 60947-5-2","只",5,"340热轧","2023-01-27"]
[49,6100600048,"快速熔断器","NGT00C-380V/100A；",null,null,"只",8,"340热轧","2023-01-27"]
[50,6100500353,"时间继电器","SK4-220d；0.1～3S","通电延时型空气延时头；延时动作时间0.1～3S；触头额定电流：0.95A主触头触点形式：双断电；工作条件：周围空气温度-50℃—+40℃，24小时的平均值不超过+35℃；空气的相对湿度为不超过50%；安装地点海拔不超过2000M；","GB14048.4-2010","只",20,"340热轧","2023-01-27"]
[51,4100500040,"行程开关","YBLX-K3/20S/T",null,"JB/T5553-2006","只",10,"炼钢厂部","2023-01-27"]
[52,6100600174,"熔断器","RN2-10KVA","0.5A",null,"只",12,"炼钢厂部","2023-01-27"]
[53,4100700018,"多转精密电位器","3590S-2-103L","10K欧 +-5%","GB/T11210-1989","只",10,"炼钢厂部","2023-01-27"]
[54,6400600124,"磁伸宿传感器","KYDM-LPIA4210-GB0800M1C10-WO",null,"GB/T14048","只",1,"管加工厂部","2023-01-27"]
[55,6400200092,"光电开关","GS10-P4311","外形:矩形 外壳材质:金属 检测模式/感应类型:漫反射式 供电范围:10-30VDC 感应范围:典型最大10-1200MM 输出形式:PNP/NPN 输出特性:常开1点，常闭1点 , 防护等级:IP67","JB/T 6475-1992","只",5,"管加工厂部","2023-01-27"]
[56,6400200093,"光电开关","GS10-D4311","外形:矩形 外壳材质:金属 检测模式/感应类型:漫反射式 供电范围:10-30VDC 感应范围:典型最大10-1200MM 输出形式:PNP/NPN 输出特性:常开1点，常闭1点 , 防护等级:IP67","JB/T 6475-1992","只",5,"管加工厂部","2023-01-27"]
[57,6100500367,"中间继电器","C10-A10FX","24VDC;带座;10A 250V AC1;10A 30V DC1;RELECO","JBT 56288-1999","只",30,"炼铁厂部","2023-01-27"]
[58,6400400049,"增量编码器","DKS40-E5J01000 带弹性联轴器9402 8*8 SICK","增量型 金属外壳 脉冲数1024 侧向电缆直接 10 V ... 30 V 供电，符合标准DIN EN 61000-6-4，DIN EN 61000-6-2","EN61000-6-2","只",2,"720厂部","2023-01-27"]
[59,6400600509,"位移传感器","RHM0260MD701S2G1100","MTS R系列SSI；带定位磁环、附件及10m电缆","GB/T 28857-2012","只",1,"720厂部","2023-01-27"]
[60,6100300074,"断路器","DZ47-60,2P 20A","Ue:690V.50/60Hz","GB14048.2-2001","只",20,"340热轧","2023-01-27"]
[61,6400300052,"接近开关","GH1-JK320M 380V",null,"JB14048","只",10,"340热轧","2023-01-27"]
[62,6100600035,"熔断器","RT28-32 2A",null,null,"只",4,"能源厂部","2023-01-27"]
[63,6700300011,"漏电断路器","C20 DZ47LEII-50/3N",null,"GB10963.1-2005","只",10,"能源厂部","2023-01-27"]
[64,6100200055,"Elx万能转换开关","LW21-16XZDH04-3N","4档3节，面板文字带分、合，通用互开型钥匙，面板带分、合指示灯。","GB 2682-81","个",5,"能源厂部","2023-01-27"]
[65,6100700024,"电压抽取装置","TYD220/√3-0.005","型式：单相/户外/叠装级次组合： 0.5/3P\n  额定输出（VA）： 75/100VA\n  额定电容量（pF）：5000pF 额定变比：220/√3 |0.1/√3|0.1KV","GB4703","个",1,"能源厂部","2023-01-27"]
[66,4100300018,"进口高温PROFIBUS网线","DDZF-1F-2P-065HY 德国IEC947","DDZF-1F-2P-065HY","德国IEC947","米",800,"720厂部","2023-02-10"]
[67,6300100121,"6点AI模块","1756-IR6I AB","6点AI模块热电阻 4-20MA 电阻值输入","IEC61508","只",1,"炼铁厂部","2023-01-27"]
[68,6300100122,"CPU模块","1769-30ER","电压24V DC，防护等级IP54,","GB/T 39360-2020","块",2,"炼铁厂部","2023-01-27"]
[69,6100700023,"高压电流互感器","LZZBJ1-10W1  150/5A","户内，12KV，150/5A，15VA/0.5/20VA/5P20","GB1208-2006","台",3,"炼铁厂部","2023-01-27"]
[70,6100100142,"电容","CD60-300V-2000UF","CD60-300V-2000UF 上海天和","JB/T 7110-1993","只",2,"管加工厂部","2023-01-27"]
[71,6400600513,"位移传感器","CG5/0155KS201-S5+CPR02","量程155mm 电源24VDC 输出4-20mA，测量起始端以外保持4mA输出，超出测量末端保持20mA输出，5米屏蔽电缆直接，带磁环。","GB/T 28857-2012","只",3,"340热轧","2023-01-27"]
[72,6400600514,"位移传感器","CG5/0225KS201-S5+CPR02","量程225mm 电源24VDC 输出4-20mA，测量起始端以外保持4mA输出，超出测量末端保持20mA输出，5米屏蔽电缆直接，带磁环。","GB/T 28857-2012","只",3,"340热轧","2023-01-27"]
[73,6400400158,"编码器防护箱","TBB-9Z-RB","传动轴方向：右出轴;带接线端子；IP56；温州海光电器","GB3836.3-2010","件",2,"180厂部","2023-01-27"]
[74,6400400159,"编码器防护箱","TBB-9Z-LB","传动轴方向：左出轴;带接线端子；IP56；温州海光电器","GB3836.3-2010","件",2,"180厂部","2023-01-27"]
[75,4100400285,"10KV冷缩中间接头","JLS-15/1.3","150-240mm2","GB/T 11017.3","套",6,"炼钢厂部","2023-01-27"]
[76,6100300294,"熔断器手车套管","KYN61-40.5","用于户内35kv高压熔断器手车，套管内置熔断器：XRNT-40.5; 40.5kv  10A  31.5KA","GB/T21706-2008","个",1,"能源厂部","2023-01-27"]
[77,6200200878,"变频器","T9400-3R7G/5R5P","输入380VAC； 功率5.5kw","GB/T12668.2-2002","台",1,"能源厂部","2023-01-27"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2022年12月电气备件采购项目        项目编号：HGCGD22146"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}