{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":37,"n_cols":13,"rows_kept":37,"merged":[[0,0,0,8],[1,0,1,12],[33,0,33,8],[34,0,34,8],[35,0,35,8],[36,0,36,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2022年12月阀门采购项目                     项目编号：HGCGD22147"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,7101800154,"高压球阀","KHM-G11/4-1112-01X",null,"件",2,"GB/T9065.2-2010","89油管热处理","2023-02-11"]
[2,7101300010,"高压球阀","KHM-50-F6-11141-02X",null,"只",3,null,"219厂部","2023-02-11"]
[3,7101800055,"高压球阀","BKH-20S-1123",null,"只",5,"GB/T9065.2-2010","219厂部","2023-02-11"]
[4,7102000081,"燃气止回阀","HF-G1A","内丝G1\";球头;介质:氧气","只",2,"GB13347-1992","炼钢厂部","2023-02-11"]
[5,7101800057,"高压球阀","BKH-30S-1125",null,"只",8,"ISO228","炼钢厂部","2023-02-11"]
[6,7101800058,"高压球阀","BKH-38S-1125",null,"只",4,"GB/T9065.2-2010","炼钢厂部","2023-02-11"]
[7,7101800053,"高压球阀","BKH-16S-1123",null,"只",25,"GB/T12230-2005","管加工厂部","2023-02-11"]
[8,7101800055,"高压球阀","BKH-20S-1123",null,"只",25,"GB/T9065.2-2010","管加工厂部","2023-02-11"]
[9,7101800057,"高压球阀","BKH-30S-1125",null,"只",25,"ISO228","管加工厂部","2023-02-11"]
[10,7101600114,"气动蝶阀","V637713","1.6MPa;DN250","个",2,null,"管加工厂部","2023-02-11"]
[11,7100100257,"安全阀","A47H-25L-80","压力等级1.6-2.0Mpa；整定压力1.4Mpa","只",1,"GB/T12243-2005","高辅工段","2023-02-11"]
[12,7100100258,"安全阀","A27W-10T-25","压力等级0.8-1.2Mpa；整定压力0.8Mpa","只",2,"GB/T12243-2005","高辅工段","2023-02-11"]
[13,7101600232,"电动金属硬密封蝶阀","D943P-2.5C-350","DN350 带输入/输出远程接口 含法兰.垫片；介质：除尘烟气","套",11,"GB/T12237","烧结","2023-02-11"]
[14,7101800054,"高压球阀","BKH-16S-1443",null,"只",10,"GB/T12230-2005","340热轧","2023-02-11"]
[15,7101800055,"高压球阀","BKH-20S-1123",null,"只",10,"GB/T9065.2-2010","340热轧","2023-02-11"]
[16,7101800058,"高压球阀","BKH-38S-1125",null,"只",25,"GB/T9065.2-2010","管加工厂部","2023-02-11"]
[17,7101300010,"高压球阀","KHM-50-F6-11141-02X",null,"只",6,null,"管加工厂部","2023-02-11"]
[18,5716000022,"高压泵安全阀","A41Y-320P  DIN24342",null,"只",1,"DIN24342","管加工厂部","2023-02-10"]
[19,7101900062,"截止阀","J41H-16C;","DN125;     1.6MPa;","只",2,"GB/T12237-1989","管加工厂部","2023-01-26"]
[20,5500800004,"电动卸灰耐磨球阀","DN300","铸钢 介质:高炉含尘埃气体，总长度？ 硬密封 全球阀 耐温≥250℃ 球体1Cr18Ni9Ti+硬铬,工作压力2.25MPa带电动装置 工作300℃，电动装置型号 Z32B 电机功率0.37KW 电压 380V 电流 1.38A 输出转矩 200N.m 输出转速18r/min。","只",3,"GB12221-1989","高辅工段","2023-02-11"]
[21,7101800053,"高压球阀","BKH-16S-1123",null,"只",20,"GB/T12230-2005","720厂部","2023-02-11"]
[22,7101900022,"不锈钢截止阀","J41W-16P-50","法兰连接直通式不锈钢截止阀 压力1.6MPa DN50","只",2,"GB 8465.3-1987","高炉","2023-02-11"]
[23,7101700077,"闸阀","Z41H-40-50","DN50;压力:4.0MPa;材质:铸钢;连接形式:法兰","只",4,"GB/T12232-2005","高炉","2023-01-27"]
[24,7101800229,"不锈钢球阀","Q41F-16p-100","DN100；压力1.6MPa； 浮动直通式，氟塑料；手动，法兰连接","只",2,"GB/T12224-1989","高炉","2023-01-27"]
[25,7101800010,"不锈钢法兰式球阀","Q41F-25P-25 DN25,PN2.5","GB/T12221-2005,公称直径：DN25，压力等级：P≤2.5Mp，阀体长度：165mm，阀体不锈钢","只",2,"GB/T12237","高炉","2023-02-11"]
[26,7102100003,"法兰式疏水阀","CS49H-16-25","铸造","只",2,null,"高炉","2023-02-11"]
[27,5500800003,"电动扇型耐磨盲板阀","DN600","铸钢 型号 防爆型 F943X-2.5,工作压力0.25MPa,带电动装置,密封条材质氟橡胶246,工作温度-20℃-300℃;法兰JB/T8527-1997， 配2片金属缠绕垫600*670*10;电动装置型号 Z39-18B, 电机功率 0.5KW 电压 380V ,输出转矩 300N.m ,输出转速 18r/min,启闭时间20S；双层不锈钢金属波纹管材质为254SMo,厚度1.2mm*2;密封槽尺寸及电装联结结构尺寸需按技术规格书要求标准制造。","只",3,"JB/T18527-1997","高辅工段","2023-02-11"]
[28,5500800004,"电动卸灰耐磨球阀","DN300","铸钢 介质:高炉含尘埃气体，总长度？ 硬密封 全球阀 耐温≥250℃ 球体1Cr18Ni9Ti+硬铬,工作压力2.25MPa带电动装置 工作300℃，电动装置型号 Z32B 电机功率0.37KW 电压 380V 电流 1.38A 输出转矩 200N.m 输出转速18r/min。","只",2,"GB12221-1989","高辅工段","2023-02-11"]
[29,7101800120,"三片式不锈钢球阀","Q311F-25P-40","不锈钢手动球阀 浮动直通式 氟塑料 压力2.5mpa DN40","只",100,"GB/T12237","炼钢厂部","2023-02-11"]
[30,7100200099,"法兰式不锈钢手动煤气快速球阀","Q41F-16C；DN125","PN1.6;阀芯材质：304","只",10,"HG20592-2009","340热轧","2023-02-26"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2022年12月阀门采购项目           项目编号：HGCGD22147"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":4,"n_cols":1,"rows_kept":4,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8]],"flags":["formulas_cached_only"]}
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]