{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":46,"n_cols":11,"rows_kept":46,"merged":[[0,0,0,10],[1,0,1,10],[43,0,43,6],[44,0,44,6],[45,0,45,6]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2022年12月液压缸公开招标采购项目                                         项目编号：HGCGD22148"]
["序号","资材编号","资材名称","规格型号","技术参数","单位","数量","交货时间","使用部门","含税单价(元)","生产厂家\n"]
[1,7200100439,"液压缸","CD250E63/45-200 A10/01CADMA 带GAS35Q球铰耳环","缸径Φ63,杆径Φ45,行程200","个",1,"2023-03-30","管加工厂部"]
[2,7200100130,"液压缸","CD350E63/45-600B10/02CADMA+GAS40 L10=250","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",2,"2023-05-30","219厂部"]
[3,7200100053,"液压缸","CD250B125/70-125A10/02CADMA","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",1,"2023-05-30","219厂部"]
[4,7200100015,"液压缸","CD250A100/70-110A10/02CADMA","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",1,"2023-05-30","219厂部"]
[5,7200100038,"液压缸","CD250B125/90-235A10/02CGDMA","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",1,"2023-05-30","219厂部"]
[6,7200100075,"液压缸","CD250C80/56-100C/DMT","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",2,"2023-05-30","219厂部"]
[7,7200100074,"液压缸","CD250C63/45-60A10/02CADMA","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",3,"2023-05-30","219厂部"]
[8,7200100020,"液压缸","CD250A160/110-320A10/01.4CADMA","缸径Φ160,杆径Φ110,行程320 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"2023-05-30","219厂部"]
[9,7200100089,"液压缸","CD250E125/70-250A10/02CADMA+GAS60 L10=370","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",2,"2023-05-30","219厂部"]
[10,7200100267,"液压缸","CD250E63/36-380A10/02CADMA+GAS35 L10=350","缸径Φ63,杆径Φ36,行程380 ,工作压力25MPa 活塞及活塞杆采用V型组合密封，带球铰耳环","台",1,"2023-03-30","89油管热处理"]
[11,7200100272,"液压缸","CD250B125/90-115A10/02CADMA+GAS60","缸径Φ125,杆径Φ90,行程115 ,工作压力25MPa 活塞及活塞杆采用V型组合密封，带球铰耳环","台",1,"2023-03-30","89油管热处理"]
[12,7200400063,"液压缸","CD250B125/90-255A10/01CADMA",null,"台",2,"2023-05-30","89油管热处理"]
[13,7200400092,"液压缸","YG63/36-120","工作压力25MPa，缸径63mm，杆径36mm，行程120mm","台",2,"2023-04-30","89油管热处理"]
[14,7200100313,"油缸","CDH2MP3/50/36/900A1X/B1CFEMWW","油口G1/2  压力等级：25MPa","台",1,"2023-03-30","89油管热处理"]
[15,7201300033,"液压缸耳环","GAK22",null,"件",8,"2023-04-30","管加工厂部"]
[16,7200100187,"液压缸","CD250E100/56-220A10/01CADMA","L10=220","台",2,"2023-05-30","管加工厂部"]
[17,7200400033,"液压缸","YG80/45*200-S",null,"台",4,"2023-05-30","管加工厂部"]
[18,7200200015,"液压缸","02690005DR5003ME014-22","CD250E125/90-700A10/01CGDMA L10=620 带GAK58耳环 额定压力25MPa","台",1,"2023-05-30","180厂部"]
[19,7200200019,"液压缸","02690005DR5004ME005-21","CD250E125/90-410A10/01CGDMA 额定压力25MPa JB/T 5000","台",1,"2023-05-30","180厂部"]
[20,7200200061,"液压缸","Z0733.03.02.04.00","额定压力25MPa","台",2,"2023-05-30","180厂部"]
[21,7200100041,"液压缸","CD250B125/90-340A10/02CADMA","JB/T 5000 额定压力25MPa","台",1,"2023-05-30","180厂部"]
[22,7200400094,"液压缸","02690005DR5004ME043-67M","不带位移传感器；带磁环； 额定压力25MPa 100/70-200","台",2,"2023-03-30","180厂部"]
[23,7200500024,"液压缸","0107119-36.101","额定压力25MPa JB/T 5000","台",6,"2023-05-30","180厂部"]
[24,7200600044,"炉盖提升缸","140/80-470","缸径Φ140,杆径Φ80,行程470 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力25MPa 活塞及活塞杆采用V型组合耐高温密封 工作介质水乙二醇液压油","台",1,"2023-04-30","炼钢厂部"]
[25,7200600226,"钢包加盖横移液压缸（三)","90/60-800","缸径Φ90,杆径Φ60,行程800;工作环境温度≤200℃;工作压力25MPa;试验压力31.5MPa;活塞及活塞杆采用V型组合密封;工作介质水乙二醇液压油;配GAS50耳环;图号:GBJG-HGL-02-4","台",1,"2023-03-30","炼钢厂部"]
[26,7200600021,"顶渣液压缸","80/55-300","缸径Φ80,杆径Φ55,行程300 工作环境温度-20℃~100℃ 工作压力17MPa,试验压力25MPa 活塞及活塞杆采用V型组合耐高温密封 工作介质水乙二醇液压油","台",2,"2023-05-30","炼钢厂部"]
[27,7200600032,"浇注液压缸","90/45-115","配进口密封 缸径Φ100,杆径Φ50,行程170 工作环境温度-20℃~120℃ 工作压力20MPa,试验压力30MPa 活塞及活塞杆采用V型组合耐高温密封 工作介质水乙二醇液压油","台",3,"2023-05-30","炼钢厂部"]
[28,7201300017,"液压缸 三位活塞杆","WG10525-03","42CrMn","件",6,"2023-04-30","340热轧"]
[29,7200100067,"液压缸","CD250B80/56-320A10/02CGDMA+GAK35","缸径Φ80,杆径Φ56,行程320 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"2023-05-30","340热轧"]
[30,7200600111,"液压缸","PBA03CL00000 63/45-125","缸径Φ63,杆径Φ45,行程125 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",4,"2023-05-30","340热轧"]
[31,7200100276,"液压缸;","PBA03CN00000;80/56-225","缸径Φ80,杆径Φ56,行程225 工作环境温度-20℃~70℃ 工作压力16MPa,试验压力20MPa 活塞密封为格莱圈，活塞杆采用V型组合密封","台",3,"2023-05-30","340热轧"]
[32,7200100056,"液压缸","CD250B63/36-25A10/02CGDMA","缸径Φ63,杆径Φ36,行程25 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"2023-05-12","340热轧"]
[33,7200100152,"液压缸","CDH1MT4/80/56-300A1X/B1CSDMWW+GAS40 XV=342","缸径Φ80,杆径Φ56,行程300 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"2023-05-12","340热轧"]
[34,7200100172,"液压缸","HYZ021845","80/56-15 额定压力25MPa JB/T 5000","台",2,"2023-05-12","340热轧"]
[35,7200100226,"液压缸","CD250B100/56-60A10/011CADMAC02",null,"台",1,"2023-05-12","管加工厂部"]
[36,7200600084,"液压缸","CDH1MP5/125/70-100A1X/D1CSEMWW 带耳环","缸径Φ125,杆径Φ70,行程100 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",5,"2023-05-12","340热轧"]
[37,7200600120,"液压缸","PBA03DC00000 100/63-150","缸径Φ100,杆径Φ63,行程150 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞采用PG型组合密封 活塞杆采用RS+USH型组合密封","台",2,"2023-05-12","340热轧"]
[38,7200400001,"C型转子翻车机摘钩液压缸","HSGL01-40/20-1101-80/305","带耳环，密封材质：聚氨酯+丁晴橡胶，工作压力25MPa","台",2,"2023-05-12","原料工段"]
[39,5722700005,"液压缸","CD250B125/90-300A10/01CADMA：  图号：02680018DR5008ME038-46","带GAS60球铰耳环","台",2,"2023-03-28","管加工厂部"]
[40,5723700013,"低压注水油缸","DZSF200-08A","缸径80，杆径45，行程230，额定压力20MPa","台",3,"2023-03-28","管加工厂部"]
["投标人：                         （盖单位公章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日  期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2022年12月液压缸公开招标采购项目                项目编号：HGCGD22148"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位公章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日  期：      年      月      日                "]