{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":30,"n_cols":13,"rows_kept":30,"merged":[[0,0,0,8],[1,0,1,12],[26,0,26,8],[27,0,27,8],[28,0,28,8],[29,0,29,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2022年12月机械备件采购项目                     项目编号：HGCGD22150"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,7101000065,"偏心旋转控制阀","MaxFlo4;DN150;PN40;Positioner Model:Logix 500 series","气关式","台",1,"EN 1092-1","炼钢厂部","2023-02-26"]
[2,5300400268,"双向可逆皮带机校正器（槽式）","JHYJZP800AD-B   带宽800","露天双向可逆，包胶花纹主辊D159/d133×315，主托辊辊面衬胶采用复合聚氨脂材料，具有防冻、防滑、防脱落及耐磨性能，且满足当地气候温度，托辊具有防尘、防水，动作灵敏可靠，无噪音，调偏幅度大，带宽800，长1185×宽350×高400；不损伤皮带，表面胶层硬度不得低于60～70°(邵氏A型硬度)，质保期三年，质保期内无需更换任何配件。","套",2,"ZL202020201838.8","原料工段","2023-02-26"]
[3,5300400269,"双向可逆皮带机校正器（返式）","JHYJZP800BD-B  带宽800","露天双向可逆，包胶花纹主辊D180×840，主托辊辊面衬胶采用复合聚氨脂材料，具有防冻、防滑、防脱落及耐磨性能，且满足当地气候温度，托辊具有防尘、防水，动作灵敏可靠，无噪音，调偏幅度大，带宽800，长1170×宽270×高270；不损伤皮带，表面胶层硬度不得低于60～70°(邵氏A型硬度)，质保期三年，质保期内无需更换任何配件。","套",2,"ZL202020201838.8","原料工段","2023-02-26"]
[4,4100300044,"易格斯拖链","HG3400.175.150.0","材质：塑料；节距：67mm/节；内高：45mm;内宽：175mm；弯曲半径：150mm","米",18,"ISO9001-2015","管加工厂部","2023-03-28"]
[5,5714100033,"气体弹簧","90.10.00500.160 PED","进口件 进口件，90.10.00500.160","只",20,"PED","720厂部","2023-03-13"]
[6,7001200343,"高压泵连杆","3D-250-0102",null,"根",4,null,"219厂部","2023-02-26"]
[7,5501700003,"堆取料机;斗轮机构轴承座","D223A-11.0","ZG35 孔径50，轴向孔距145，径向孔距530，座低平面与孔中心线夹角5°侧端盖带注油孔M10","件",2,null,"原料工段","2023-02-26"]
[8,5400300008,"煤气冷凝水排水器","SDLT-4000-100","Q235 GB6222","台",2,"GB6222","高辅工段","2023-02-26"]
[9,5501400007,"烧结;成品仓振动给料机","QZS-80-130F 不带电机；面宽800mm，长1300mm","铆焊","台",4,"JB/T8096-2013","烧结","2023-02-26"]
[10,7502400138,"机床切削液专用混配器","Master Mix M-10","配比浓度0%~20%，流量38升/分，进水口1/2英寸，出水口3/4英寸，水压：2bar~4bar","套",2,"Q/MT 005-2016","管加工厂部","2023-02-26"]
[11,7001200251,"高压泵 夹管举管组合体","PT245.105-001.04",null,"套",1,"JB/T9872-2000","管加工厂部","2023-02-26"]
[12,5500300029,"上下调整拉杆","KD300","锻钢调质 炉前泥炮KD300 上下调整拉杆，45# 锻造，调质处理，带销轴，带干油嘴","件",1,null,"高炉","2023-02-26"]
[13,5601700022,"拖链","TL180III-R450*510*8640","支撑板宽度510mm:节数48;附订货图","件",2,"JB/T6608-1993","炼钢厂部","2023-02-26"]
[14,5602600067,"事故割炬","SG-II","图号QGJ-22;L=2400mm","把",4,"GB5108-1985","炼钢厂部","2023-02-26"]
[15,4000300241,"轴承座","HX110(GB/T2563-2007);轴承座材质ZG270-500；","带铜瓦；润滑油口M10*1；","套",10,"审核图纸","管加工厂部","2023-02-26"]
[16,7502400141,"加药搅拌轴及叶轮","750-32","搅拌轴：304不锈钢材质，直径32mm,长度：1200mm，实心；三叶叶轮：不锈钢材质，内孔Φ32mm，外直径Φ750mm，厚度6mm","套",2,null,"340热轧","2023-02-26"]
[17,6600300111,"空气过滤减压阀","YT-200B","出口气压2-8公斤可调","只",5,null,"340热轧","2023-02-26"]
[18,5719700002,"PP袋式污水过滤袋","180*810-150微米--2号；","过滤精度：150μm；过滤面积：0.5㎡；最大流量：40m3/h ；袋口固定环：镀锌钢圈","只",50,"GB12625-1990","管加工厂部","2023-02-26"]
[19,5500500040,"倒流休风阀","QR743R","公称通径：600mm；工作温度：≦1350度；工作压力：0.40MPa；工作介质：热空气，密封面堆焊硬质合金 阀盖铸钢件 阀板及密封面 铸钢件，密封面堆焊硬质合金 阀杆材质316L不锈钢，带金属垫及螺栓整套，带油缸","台",1,"GB/T12238-2008","高炉","2023-02-26"]
[20,7502500104,"抽风机;机壳","适用于YXQ-1200D型号离心通风机","左.右旋;180°;不锈钢材质;厚度8mm;侧下方带清渣口","件",2,"GB/T19232-2003","炼钢厂部","2023-02-26"]
[21,6600300170,"电动调节阀","M8610S","功率0.5kw，直行程，行程距离0-50，输入信号4-20ma ，反馈信号4-20ma，电压220VAC， 扭矩20-50Nm连接F10，；齿轮箱L8210,连接方式S105-12X4-80 M12X1.25；阀体HT-S10000,1.6MPA,口径DN65,80℃；","台",1,"JB/T8219-1999","能源厂部","2023-02-26"]
[22,7502500105,"罗茨鼓风机","JTS 125","鼓风机参数：进气压力：101.3Kpa、流量：16.1m3、转速：1450r/min、进气温度：＜40C°、升压：58.8Kpa 含电机，电机参数：型号Y200L-4 额定功率30KW 额定转速1470r/min 额定电流56.8A 三角型接法 电压380V 防护等级IP44 绝缘等级B级","台",1,"JB/T10563-2006","能源厂部","2023-02-26"]
[23,7502500103,"离心高温风机转子组","Y6-30-11NO19.4F；1700.02转子组","含叶轮、轴、轴承、轴承座，总重1820Kg；叶轮工作温度120-260℃；正常使用寿命五年","套",1,"JB/T8689-1998","高辅工段","2023-02-26"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2022年12月机械备件采购项目               项目编号：HGCGD22150"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":4,"n_cols":1,"rows_kept":4,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8]],"flags":["formulas_cached_only"]}
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]