{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":31,"n_cols":13,"rows_kept":31,"merged":[[0,0,0,8],[1,0,1,12],[27,0,27,8],[28,0,28,8],[29,0,29,8],[30,0,30,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2023年2月机械备件采购项目                     项目编号：HGJY-G2023012"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,5715900029,"切管机QG1163伺服进刀装置","QG6302004A","伺服装置一级丝杆输出速度要求6~18s/mm，自由调节,动作运行平稳，模块化设计","台",2,"审核图纸","720厂部","2023-04-26"]
[2,5601700022,"拖链","TL180III-R450*510*8640","支撑板宽度510mm:节数48;附订货图","件",2,"JB/T6608-1993","炼钢厂部","2023-04-26"]
[3,5400300008,"煤气冷凝水排水器","SDLT-4000-100","Q235 GB6222","台",2,"GB6222","高辅工段","2023-04-26"]
[4,5501400007,"烧结;成品仓振动给料机","QZS-80-130F 不带电机；面宽800mm，长1300mm","铆焊","台",4,"JB/T8096-2013","烧结","2023-04-26"]
[5,7502400138,"机床切削液专用混配器","Master Mix M-10","配比浓度0%~20%，流量38升/分，进水口1/2英寸，出水口3/4英寸，水压：2bar~4bar","套",2,"Q/MT 005-2016","管加工厂部","2023-04-26"]
[6,7502400141,"加药搅拌轴及叶轮","750-32","搅拌轴：304不锈钢材质，直径32mm,长度：1200mm，实心；三叶叶轮：不锈钢材质，内孔Φ32mm，外直径Φ750mm，厚度6mm","套",2,null,"340热轧","2023-04-26"]
[7,5719700002,"PP袋式污水过滤袋","180*810-150微米--2号；","过滤精度：150μm；过滤面积：0.5㎡；最大流量：40m3/h ；袋口固定环：镀锌钢圈","只",50,"GB12625-1990","管加工厂部","2023-04-26"]
[8,5714100033,"气体弹簧","90.10.00500.160 PED","进口件 进口件，90.10.00500.160","只",20,"PED","720厂部","2023-04-26"]
[9,7502500104,"抽风机;机壳","适用于YXQ-1200D型号离心通风机","左.右旋;180°;不锈钢材质;厚度8mm;侧下方带清渣口","件",2,"GB/T19232-2003","炼钢厂部","2023-04-26"]
[10,6600300170,"电动调节阀","M8610S","功率0.5kw，直行程，行程距离0-50，输入信号4-20ma ，反馈信号4-20ma，电压220VAC， 扭矩20-50Nm连接F10，；齿轮箱L8210,连接方式S105-12X4-80 M12X1.25；阀体HT-S10000,1.6MPA,口径DN65,80℃；","台",1,"JB/T8219-1999","能源厂部","2023-04-26"]
[11,5300400268,"双向可逆皮带机校正器（槽式）","JHYJZP800AD-B   带宽800","露天双向可逆，包胶花纹主辊D159/d133×315，主托辊辊面衬胶采用复合聚氨脂材料，具有防冻、防滑、防脱落及耐磨性能，且满足当地气候温度，托辊具有防尘、防水，动作灵敏可靠，无噪音，调偏幅度大，带宽800，长1185×宽350×高400；不损伤皮带，表面胶层硬度不得低于60～70°(邵氏A型硬度)，质保期三年，质保期内无需更换任何配件。","套",2,"ZL202020201838.8","原料工段","2023-04-26"]
[12,5300400269,"双向可逆皮带机校正器（返式）","JHYJZP800BD-B  带宽800","露天双向可逆，包胶花纹主辊D180×840，主托辊辊面衬胶采用复合聚氨脂材料，具有防冻、防滑、防脱落及耐磨性能，且满足当地气候温度，托辊具有防尘、防水，动作灵敏可靠，无噪音，调偏幅度大，带宽800，长1170×宽270×高270；不损伤皮带，表面胶层硬度不得低于60～70°(邵氏A型硬度)，质保期三年，质保期内无需更换任何配件。","套",2,"ZL202020201838.8","原料工段","2023-04-26"]
[13,4100300044,"易格斯拖链","HG3400.175.150.0","材质：塑料；节距：67mm/节；内高：45mm;内宽：175mm；弯曲半径：150mm","米",18,"ISO9001-2015","管加工厂部","2023-04-26"]
[14,4201700133,"超轻型硫化机","BW=800;YHG3448","尺寸：800*830mm，智能数字仪表控温系统，可“水压、气压、油压”通用切换打压，电压380伏","套",1,"GB/T19001-2016","原料工段","2023-04-26"]
[15,4201700134,"超轻型硫化机","BW=650;YHG3448","尺寸：650*700mm，智能数字仪表控温系统，可“水压、气压、油压”通用切换打压，电压380伏","套",1,"GB/T19001-2016","原料工段","2023-04-26"]
[16,7001200343,"高压泵连杆","3D-250-0102",null,"根",4,null,"219厂部","2023-04-26"]
[17,5900100004,"带锯机夹钳","行程大于800mm，挡板高大于600mm","行程大于800mm，挡板高大于600mm，包含横梁，同步齿轮、齿条；适用于GB4280C双立柱卧式带锯床","套",1,"JB/T4318","检验检测中心","2023-04-26"]
[18,5900100007,"夹钳梯形丝杆","直径25mm，总长550mm","直径25mm，总长550mm，包括梯形丝杆和梯形螺母；用于G4240/50卧式带锯床","根",2,"JB/T4318.3","检验检测中心","2023-04-26"]
[19,5709300144,"离心通风机","9-19N09D","全压:4000-4500Pa;介质密度:1.2kg/m3;流量:8000-10000m3/h;介质温度:2.0℃;转速:1450r/min;电机功率:22Kw","台",1,"GB14711-2006","219厂部","2023-04-26"]
[20,5716000029,"带锯床；夹紧齿轮齿条","G4280，每套3件，两根齿条，一个齿轮。",null,"套",2,"GB/T861-1897","炼钢厂部","2023-04-26"]
[21,7501600006,"30T闭式冷却塔","FBN-30T","冷却能力：150000kcal/h冷却器：304不锈钢管，直径19mm，每支1.7米长，壁厚0.7mm主泵流量/扬程25m3/h，28米工作水压0.15～0.3Mpa外形尺寸3000×1250×2300 mm进出水口径DN65","套",1,"JB/T2977-1992","219厂部","2023-04-26"]
[22,7502100045,"SAE法兰焊接组件","DSFS6002/1.4571","接管材质：不锈钢","只",15,"ISO7169-1998","89热轧","2023-04-26"]
[23,7502100046,"SAE法兰焊接组件","DSFS3003/1.4571","接管材质：不锈钢","只",10,"ISO7169-1999","89热轧","2023-04-26"]
[24,7502300014,"喷嘴","TP6505-TC","SPRAYINGSYSTEMS CO. DIN28025-2003","只",20,"DIN28025-2003","340热轧","2023-04-26"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2023年2月机械备件采购项目            项目编号：HGJY-G2023012"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":4,"n_cols":1,"rows_kept":4,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8]],"flags":["formulas_cached_only"]}
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]