{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":74,"n_cols":12,"rows_kept":74,"merged":[[0,0,0,11],[1,0,1,11],[70,0,70,8],[71,0,71,8],[72,0,72,8],[73,0,73,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2023年2月电气备件采购项目                    项目编号：HGJY-G2023015"]
["序号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家"]
[1,6300400011,"PLC 电源模块","1756-PA72","AB","GBT15969","块",2,"管加工厂部","2023-04-27"]
[2,6100400164,"电位器","WX03-4.7K",null,"GB/T 11210-1989","只",20,"管加工厂部","2023-04-27"]
[3,6100500380,"时间继电器","H3YN-2 TIMER","AC200-230V ;50/60HZ;8针","GB14048.5","只",20,"180厂部","2023-04-27"]
[4,6100600260,"熔断器","NGT1;1000V,100A","1000V,100A","IEC269;GB13539","个",6,"720厂部","2023-04-27"]
[5,6400200060,"光敏开关","AS20-220V；RMSCSH","现场照明灯采用光控开关 输入/输出电压220V 路灯光控开关 塑料白色外壳 圆锥型","IEC 60947-5-2","只",5,"340热轧","2023-04-27"]
[6,6100600048,"快速熔断器","NGT00C-380V/100A；",null,null,"只",8,"340热轧","2023-04-27"]
[7,4100500040,"行程开关","YBLX-K3/20S/T",null,"JB/T5553-2006","只",10,"炼钢厂部","2023-04-27"]
[8,6100600174,"熔断器","RN2-10KVA","0.5A",null,"只",12,"炼钢厂部","2023-04-27"]
[9,4100700018,"多转精密电位器","3590S-2-103L","10K欧 +-5%","GB/T11210-1989","只",10,"炼钢厂部","2023-04-27"]
[10,6100500367,"中间继电器","C10-A10FX","24VDC;带座;10A 250V AC1;10A 30V DC1;RELECO","JBT 56288-1999","只",30,"炼铁厂部","2023-04-27"]
[11,6400400049,"增量编码器","DKS40-E5J01000 带弹性联轴器9402 8*8 SICK","增量型 金属外壳 脉冲数1024 侧向电缆直接 10 V ... 30 V 供电，符合标准DIN EN 61000-6-4，DIN EN 61000-6-2","EN61000-6-2","只",2,"720厂部","2023-04-27"]
[12,6100300074,"断路器","DZ47-60,2P 20A","Ue:690V.50/60Hz","GB14048.2-2001","只",20,"340热轧","2023-04-27"]
[13,6400300052,"接近开关","GH1-JK320M 380V",null,"JB14048","只",10,"340热轧","2023-04-27"]
[14,6100600035,"熔断器","RT28-32 2A",null,null,"只",4,"能源厂部","2023-04-27"]
[15,6300500270,"UPS电源","R-3KB;额定功率3KVA;后备时间7Min;","输入电压电压：220V;输出电压： 220~240V 50~60Hz","IEC62040-1-2013","台",3,"管加工厂部","2023-04-27"]
[16,4000200359,"35KV穿墙套管","CWC-35/2000A","35KV/2000A;尺寸：L:950\\L1：790\\L2：422\\L3：12\\d1:16\\d2:45\\a:200","JB/DQ2553-1989","只",9,"能源厂部","2023-04-27"]
[17,6100300295,"断路器","CM3-400M/33202；400A","额定工作电压 AC690V/400V；额定绝缘电压800V;额定频率50HZ/60HZ;额定电流400A;瞬时脱扣整定电流12In","IEC60947-2 GB14048.2","只",1,"180厂部","2023-04-27"]
[18,6100900137,"不锈钢成套开关箱","\"1、材质:不锈钢;\n2、规格:宽*高*深700mm*800mm*200mm；          3、包含开关、电表、互感器、零母排、地母排等)\"","内含：①三相塑壳式断路器CKCM1-400L 400A一个，②3个电流互感器200/5，③长沙威胜三相四线智能电表1块（3*1.5（6）A），④3P100A空开1个，⑤3P63A空开1个，⑥2P63A空开1个，⑦漏电开关2P40A1个;","JB/T9265-1999","个",1,"能源厂部","2023-04-27"]
[19,6100900138,"不锈钢成套开关箱","\"1.材质:不锈钢;\n2.规格: 宽*高*深400mm*800mm*200mm；          3、包含开关、零母排、地母排等)\"","内含：三相塑壳式断路器CKCM1-400L 215A 1个；3P100A空开1个；3P63A空开2个；2P63A空开2个；2P40A漏电开关1个；","JB/T9265-1999","个",1,"能源厂部","2023-04-27"]
[20,6100900139,"不锈钢成套开关箱","\"1.材质:不锈钢;\n2.规格: 宽*高*深700mm*800mm*200mm；          3、包含开关、接触器、零母排、地母排等)\"","内含：三相塑壳式断路器CKCM1-400L 250A 1个，3个三相80A的接触器分别由按钮控制，3P63A空开3个，2P32A2空开2个，2P40A漏电开关1个；","JB/T9265-1999","个",1,"能源厂部","2023-04-27"]
[21,4000200360,"穿墙套管","CWB-10/1000A","额定电压：10kv，电流：1000A；导电铜排：60mm*10mm；套管固定螺丝4*Φ14，孔距150mm；套管总长度350mm（不含连接铜排）","JB/DQ2553-1989","只",4,"能源厂部","2023-03-29"]
[22,4000200361,"电容器组型氧化锌避雷器","HY5WR-51/134","系统运行电压35KV","GB11032","个",12,"能源厂部","2023-03-14"]
[23,4100700192,"防护电容器","FWF35/√3-0.1","35/√3KV；0.105μF；50HZ；绝缘水平80/85KV;单相","GB/T 30841-2014","只",6,"能源厂部","2023-03-29"]
[24,7101500073,"阀门电动装置","型号00M3.T.J  080388D","输出扭矩600Nm，输出转速18r/min,防护等级IP67",null,"套",1,"高炉","2023-03-29"]
[25,5501300058,"环冷机;隔振型永磁耦合器","YCL2-0015/6","最大转速/rpm;990;传递功率/kW;7.5;额定转矩/N.m;72.3;外形尺寸/mm;Φ330×93;设备重量/kg;50","Q/320192MGNT001-2018","套",2,"烧结","2023-03-14"]
[26,6000300248,"变频器风扇","MMF-08D24ES","CA1639H01;24VDC,0.16A;品牌：三菱","GB/T22712-2008","台",2,"340热轧","2023-04-27"]
[27,6000300249,"变频器风扇","9LB1424H507","SanAce140L,24VDC,0.6A,14CM,品牌：三洋","GB/T22712-2008","台",2,"340热轧","2023-04-27"]
[28,6000300250,"变频器风扇","W2S130-AA03-87","230V，50/60Hz,45/39W,ebmpapst","GB/T22712-2008","台",2,"340热轧","2023-04-27"]
[29,6000300251,"变频器风扇","4715MS-23T-B50","230V~AC，50/60Hz,15/14W","GB/T22712-2008","台",2,"340热轧","2023-04-27"]
[30,6100900135,"接线盒","M2QA315L4A","长53cm宽35cm高20cm，材料HT100","JB/T10634-2006","个",5,"340热轧","2023-04-27"]
[31,6000300246,"变频器冷却风机","FP-105EX-S1-B","正方形，尺寸：150*150*50（mm);孔距122mm;AC220V；50Hz；0.22A;38W","GB/T22712-2008","台",5,"340热轧","2023-04-27"]
[32,6000300247,"励磁变压器冷却风机","GFD450/106-510","风量：510m3/h；220V；50Hz；38W；转速:1400r/min;3.5KG","GB/T22712-2008","台",10,"340热轧","2023-04-27"]
[33,6100900050,"控制柜","2000*800*800;标准",null,null,"台",1,"340热轧","2023-04-27"]
[34,6100500353,"时间继电器","SK4-220d；0.1～3S","通电延时型空气延时头；延时动作时间0.1～3S；触头额定电流：0.95A主触头触点形式：双断电；工作条件：周围空气温度-50℃—+40℃，24小时的平均值不超过+35℃；空气的相对湿度为不超过50%；安装地点海拔不超过2000M；","GB14048.4-2010","只",30,"340热轧","2023-04-28"]
[35,7500500115,"喷标机 油漆过滤器","62.5L-LPH-SL-100-N2",null,"JB/T8679-1998","件",10,"89油管热处理","2023-04-27"]
[36,6100500382,"中间继电器","JZX-22F/4Z","AC220V，3A，4开4闭，14脚，无底座","GB/T14048.1-2006","只",20,"物流中心","2023-04-27"]
[37,6300300148,"PLC模块","1756-IF8;AB",null,null,"块",2,"219厂部","2023-04-27"]
[38,6400300053,"接近开关","LJ18A3-8-J/EZ AC90-250V",null,"GB/T14048.10-2008","只",3,"检验检测中心","2023-04-27"]
[39,6100500044,"时间继电器","H3Y－2PYF08A DC24V 0.5？1S",null,"GB/T 14598.1-2002","只",5,"检验检测中心","2023-04-27"]
[40,6100500075,"中间继电器","RJ25-CL-D24 DC24V RU2S","IEC61810-1","IEC61810-1","只",5,"检验检测中心","2023-04-27"]
[41,6400300202,"接近开关","FBM-30D20P1-D3","工作电压10-30VDC;感应距离20mm;PNP型;电感式传感器;齐平安装;全金属圆柱形带螺纹外壳;外形尺寸30mm;常开模式;3线式",null,"个",10,"89油管车丝委外","2023-04-27"]
[42,6200200876,"伺服驱动器","A06B-6117-H304","输入：283-339V ~9.5KW；输出：240V；输出电流：L axis 6.5A，M axis 6.5A ，N axis 13A","EN50178 UL508C","块",1,"检验检测中心","2023-04-27"]
[43,6400600516,"行车超载限制器","QCX-HL（5T）","工作电压AC380V，工作方式：常闭","TSG Q7014-2008","个",1,"检验检测中心","2023-04-27"]
[44,6200300094,"箱式电阻炉","炉膛尺寸(深×宽×高)：400×200×160mm","1、最高温度：1400℃，，长期工作温度：≤1350℃；2、电源及功率：AC380V/10KW；3、炉膛尺寸(深×宽×高)：400×200×160mm；4、测温：铂铑（S分度号）热电偶+精密数显程序控温仪；5、控温：可控硅移相调压+智能PID调节+程序升降温，控温精度：±1℃；6、发热元件：硅碳棒。","JJF1376-2012","台",1,"检验检测中心","2023-04-27"]
[45,6300100123,"CPU模块 AB","1769-L33ER","电压24V DC，防护等级IP54,2 MB Memory,Dual Ethernet Port - SD Card Supported - USB","IEC61508","只",1,"89油管热处理","2023-04-27"]
[46,6400400165,"旋转编码器","FS2-6815-C1024BM-05L","工作电压5VDC，输出电流≦60mA，输出高电压≧2.5V，输出低电压≦0.3V","Q/HZJD12—2019","个",1,"检验检测中心","2023-04-27"]
[47,4100500404,"按钮开关","D16LMR1-1AB","焊接端子，圆形，安装孔径16mm，1开1闭，接触电阻15mΩ，无锁复归型，额定功率250VAC 5A，24VDC 6A","CCC/CE      JBT 3907-1999","个",20,"检验检测中心","2023-04-27"]
[48,6000300245,"空气-水冷却器","BCZ-250-Z900-2；热交换容量250kw","冷却风机2台，每台15kw；进水量9.7L/S;风量8.6M3/S;最高进水温度33度，最高出水温度40度；装进出水温度显示和风温显示，进出水压力显示；安装漏水检测装置。侧面须有积水排水孔。","JB/18992-1999","台",1,"219厂部","2023-04-27"]
[49,6400600517,"位移传感器","RHM0550MD631P102","MTS 24V  550mm长  Profibus协议  附件：磁环1个，6针公、6针母插头各1个","GB/T28857-2012","支",1,"219厂部","2023-03-28"]
[50,5700100181,"滑块","HGW55HA","下锁式；末端密封垫片；","THK","件",6,"89热轧","2023-04-27"]
[51,6200200885,"交流伺服驱动器","KND SD310-30","工作电压AC220V","JB/T 10184-2014","台",1,"检验检测中心","2023-03-14"]
[52,6100900083,"BCM数字式吸盘控制装置","BCM 140A 220BS","140A  220V","GB/T3235-1999",2,"台","炼钢厂部","2023-04-27"]
[53,6200200410,"数字式调压调速装置","BCCH150A 380BS","容量150A 升降","GB/T3235-1999",1,"台","炼钢厂部","2023-04-27"]
[54,6200200632,"调压调速装置","THYROMAT 10BCCT150A","380BSZ;容量150A;平移","GB/T3235-1999",1,"台","炼钢厂部","2023-04-27"]
[55,6200200411,"数字式调压调速装置","BCCT200A","380BS GB/T3235-1999 容量200A 平移","GB/T3235-1999",1,"台","炼钢厂部","2023-04-27"]
[56,6200200853,"调压调速装置","THYROMAT 10BCCT30A 380BNZ-A","供电电压380-415v;3相50Hz;控制电压220v;单相50Hz;额定电流30A;平移机构应用","GB/T3235-1999",1,"台","炼钢厂部","2023-04-27"]
[57,6200200854,"调压调速装置","THYROMAT 10BCCH500A 380BPZ-A","供电电压380-415v;3相50Hz;控制电压220v;单相50Hz;额定电流500A;起升机构应用","GB/T3235-1999",1,"台","炼钢厂部","2023-04-27"]
[58,4100600069,"报警灯","8WD4 400-1AB","DIN VDE0660 T200;BA15d;电源等级230VAC/DC;红色;最大功率5w","IEC EN60947-5-1",6,"只","炼钢厂部","2023-04-28"]
[59,6100100221,"24V电源模块140V1","BM108.0","24VDC EV   B.M. ELETTRONICA","GB14048",2,"块","180热轧","2023-04-28"]
[60,6100600291,"电容","SKC 3M3-35B-1","10.5A/3300 350V","IEC  60831",15,"只","炼钢厂部","2023-04-28"]
[61,6100600292,"熔断器","170M5258","660V;400A;2KN/110","GB/T13539 IEC 60270",4,"只","炼钢厂部","2023-04-28"]
[62,6200200752,"变频器","PowerFlex 753；20F11NC043JA0NNNNN  AB","输入电压：400V交流 输入频率：三相，47-63HZ：输出电压：0-400V 输出电流：43A 输出频率：三相，0-400HZ 一般负载：22KW","IEC61800",1,"台","180热轧","2023-04-28"]
[63,6200200884,"操作面板","E82ZBC","Id:00417192;Prod;4500275960;Ser;0584;适用伦茨E82EV系列变频器","GB/T12668",2,"块","炼钢厂部","2023-04-28"]
[64,6200300095,"中频炉感应线圈","LZH-200-350","线圈连接端面至线圈外径总长度775mm，线圈内径380mm，功率300Kw，配连接水管卡簧，焊接部位不能漏水，材料必须采用紫铜管","JB/T2977-1992",2,"只","219厂部","2023-04-28"]
[65,6300600076,"行车遥控发射接收器","F24-12S   一发一收   控制电压AC36V","防护等级IP65 186*61*51 遥控距离100米  11个单速按钮","GB/T22084.2-2008",1,"套","炼钢厂部","2023-04-28"]
[66,6400600522,"压力传感器","ISE30A-01-D","SUP 12-24VDC  CLASS2 40mA MAX\n\nOP.PRESS -0.1-1.0MPa","GB/T15478-1995",4,"只","89热轧","2023-04-28"]
[67,6100900134,"检修电源箱","400*500*200；带电器元件","安装方式：户内壁挂明装；电源箱材料：304不锈钢 δ=1.5mm。电器元件清单及要求：1、4P 125A 漏电塑壳断路器1个； 2、3P 63A断路器2个； 3、3P 32A 断路器2个； 4、2P 16A 断路器1个； 5、2P 10A 断路器1个； 6、63A 5极 AC380V工业插座插头2套； 7、32A 5极 AC380V 工业插座插头2套； 8、16A 3极 AC220V工业插座插头1套； 9、16A  AC36V工业插座插头1套； 10、380/36V 300VA 变压器1台； 11、 PE母排一根。要求以上元器件采用国产优质品牌产品并按附图成套安装好，电源指示灯、电缆等符合电气一般设计规范，执行标准：GB7251.1-2013。","审核图纸","台",50,"炼钢厂部","2023-04-28"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2023年2月电气备件采购项目        项目编号：HGJY-G2023015"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}