{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":60,"n_cols":11,"rows_kept":60,"merged":[[0,0,0,10],[1,0,1,10],[57,0,57,6],[58,0,58,6],[59,0,59,6]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2023年3月液压缸公开招标采购项目                                         项目编号：HGJY-G2023020"]
["序号","资材编号","资材名称","规格型号","技术参数","单位","数量","交货时间","使用部门","含税单价(元)","生产厂家\n"]
[1,5900100005,"平面磨床横向油缸","行程大于1100mm","行程大于1100mm；适用于MQ7140-GM卧轴矩台平面磨床","台",2,"2023-05-30","检验检测中心"]
[2,5900100006,"可移动夹紧虎钳油缸","90*400","90*400；用于G4240/50卧式带锯床","个",2,"2023-05-30","检验检测中心"]
[3,7201300023,"液压缸","Z0224.13.02.01.00","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",2,"2023-05-30","219厂部"]
[4,7200400108,"夹具液压缸","HSGK-50-130","缸径 D=50，杆径28; 工作压力：P=18Mp;工作行程：S=130","套",2,"2023-05-30","89油管热处理"]
[5,7200600198,"液压油缸(二)","02680014DR5005ME013-21","32Kg：参照图纸技术要求","件",5,"2023-05-30","89热轧"]
[6,7200600197,"液压油缸(一)","02680014DR5005ME013-12","20Kg：参照图纸技术要求","件",4,"2023-05-30","89热轧"]
[7,7200100346,"液压缸","02680014DR5005ME035-41","按CD250B50/36-235A10/01CADMA标准制造，带防尘罩","台",2,"2023-05-30","89热轧"]
[8,7200100053,"液压缸","CD250B125/70-125A10/02CADMA","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",2,"2023-05-30","219厂部"]
[9,7201300033,"液压缸耳环","GAK22",null,"件",8,"2023-05-30","管加工厂部"]
[10,7200600044,"炉盖提升缸","140/80-470","缸径Φ140,杆径Φ80,行程470 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力25MPa 活塞及活塞杆采用V型组合耐高温密封 工作介质水乙二醇液压油","台",1,"2023-05-30","炼钢厂部"]
[11,7200600226,"钢包加盖横移液压缸（三)","90/60-800","缸径Φ90,杆径Φ60,行程800;工作环境温度≤200℃;工作压力25MPa;试验压力31.5MPa;活塞及活塞杆采用V型组合密封;工作介质水乙二醇液压油;配GAS50耳环;图号:GBJG-HGL-02-4","台",1,"2023-05-30","炼钢厂部"]
[12,7200600032,"浇注液压缸","90/45-115","配进口密封 缸径Φ100,杆径Φ50,行程170 工作环境温度-20℃~120℃ 工作压力20MPa,试验压力30MPa 活塞及活塞杆采用V型组合耐高温密封 工作介质水乙二醇液压油","台",3,"2023-05-30","炼钢厂部"]
[13,7201300017,"液压缸 三位活塞杆","WG10525-03","42CrMn","件",6,"2023-05-30","340热轧"]
[14,7200600111,"液压缸","PBA03CL00000 63/45-125","缸径Φ63,杆径Φ45,行程125 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",4,"2023-05-30","340热轧"]
[15,7200100276,"液压缸;","PBA03CN00000;80/56-225","缸径Φ80,杆径Φ56,行程225 工作环境温度-20℃~70℃ 工作压力16MPa,试验压力20MPa 活塞密封为格莱圈，活塞杆采用V型组合密封","台",3,"2023-05-30","340热轧"]
[16,7200400001,"C型转子翻车机摘钩液压缸","HSGL01-40/20-1101-80/305","带耳环，密封材质：聚氨酯+丁晴橡胶，工作压力25MPa","台",2,"2023-05-30","原料工段"]
[17,7200100056,"液压缸","CD250B63/36-25A10/02CGDMA","缸径Φ63,杆径Φ36,行程25 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"2023-05-30","340热轧"]
[18,7200600228,"液压缸","Z0745.04.03.03G","100/70-1185;耐压等级25MPA；耐高温；带GAS50耳环。","台",2,"2023-05-30","180厂部"]
[19,7200200037,"液压缸","02690005DR5006ME044-9","CD250E100/56-135A10/01CGDMA L10=269 额定压力25MPa JB/T 5000","台",1,"2023-05-30","180热轧"]
[20,7200200058,"液压缸","YG63/35-25","额定压力25MPa JB/T 5000","台",1,"2023-05-30","180热轧"]
[21,7200600151,"液压缸","268.23SB0081-17;CD250B125/90-200A10/01CADMA+GAS60改;","耐30兆帕高压，密封为进口件，位移传感器灵敏度不得有误，带耳环GAS60","台",1,"2023-05-30","180管加工热处理"]
[22,7200100420,"液压缸","CD250E100/56-280A10/01CADMA;L10=385;配耳环GAS50(带锁紧螺钉)","带GAS50球铰耳环.  L10=385；","台",2,"2023-05-30","180管加工热处理"]
[23,7200100086,"液压缸","CD250E100-56-320B10-01CADMT","L10=380 额定压力25MPa JB/T 5000","台",2,"2023-05-30","180管加工热处理"]
[24,7200100277,"液压缸","CD250E63/45-1000A10/02CADMA L10=260","压力等级：25MPa,采用进口密封，连接螺栓12.9级，带球铰耳环","台",2,"2023-06-30","720厂部"]
[25,7200400027,"液压缸","CD250B50/36-340A10/011CADMAC02",null,"台",3,"2023-06-30","340管加工热处理"]
[26,7200400025,"液压缸","CD250B50/28-325A10/02CGDMA","06.457-6","台",2,"2023-06-30","340管加工热处理"]
[27,7200100206,"液压缸","CD250E100/56-340A10/01CADMA;","L10=405，压力21MPa","个",1,"2023-07-30","340管加工热处理"]
[28,7200100216,"液压缸","CD250A50/36-200A10/01CADMA",null,"台",4,"2023-07-13","180管加工热处理"]
[29,7200100366,"液压缸","CD250B125/70-25010/01CADMA","活塞密封：DAS组合密封圈125*100*25.4*6.35","台",2,"2023-04-30","219厂部"]
[30,7200100445,"液压缸","CDH1MP5/80/56/705.0A11B1CSDBWW 活塞杆与耳环整体制作",null,"台",2,"2023-04-30","720厂部"]
[31,7200400055,"液压缸","CD250B100/70-345A10/011CADMAC02",null,"台",2,"2023-07-30","89油管热处理"]
[32,7200400076,"液压缸","CD250E125/70-340A10/01CADMA370",null,"台",1,"2023-07-30","340管加工热处理"]
[33,7200500047,"液压缸","Z0224.12.03.01 80/56-205 进口密封","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",3,"2023-07-30","219厂部"]
[34,7200500082,"液压缸","YG100X200HL-00","缸径100mm，耐压等级20MPa","件",2,"2023-05-29","180管加工水压"]
[35,7200500086,"液压缸","CDH1MP5/50/36/175A1/B1NAE*WW","缸径：50；杆径36；行程：175；带耳环","台",10,"2023-04-30","180热轧"]
[36,7200600015,"包盖旋转缸","80-56-595","缸径Φ80,杆径Φ56,行程595 工作环境温度-20℃~140℃ 工作压力25MPa,试验压力32.5MPa 活塞及活塞杆采用V型组合耐高温密封 伸缩防护套耐温150度 工作介质聚酯抗燃液压油","台",2,"2023-06-13","炼钢厂部"]
[37,7200600081,"液压缸","2500.080.278-1 80/56-225","缸径Φ80,杆径Φ56,行程225 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",2,"2023-07-30","340热轧"]
[38,7200600095,"液压缸","HSGK01-100/55E*400","缸径Φ100,杆径Φ55,行程400 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"2023-07-30","340热轧"]
[39,7200600135,"引锭杆存放液压缸","125/70-490","96Kg","台",2,"2023-07-30","炼钢厂部"]
[40,7200600150,"中间辊道液压缸","63/45-1000","进口密封 中间铰接式油缸 缸径Φ63,杆径Φ45,行程1000 工作环境温度-20℃~140℃ 工作压力14MPa,试验压力21MPa 活塞及活塞杆采用V型组合密封 伸缩防护套耐温150度 工作介质水乙二醇液压油","台",2,"2023-07-30","炼钢厂部"]
[41,7200600162,"液压缸","HYZ02345","直径90/80-130","台",3,"2023-07-30","89热轧"]
[42,7200600191,"液压缸;","WG11471改;1.MFL.009.00;63/36-650","缸径Φ63,杆径Φ36,行程650 工作环境温度-20℃~70℃ 工作压力16MPa,试验压力20MPa 活塞密封为TPM248185-63*47*18.3*6.4，活塞杆采用格莱圈和U型密封","台",2,"2023-07-30","340热轧"]
[43,7200600192,"液压缸;","WG11470改;1.MFL.010.00;63/36-650","缸径Φ63,杆径Φ36,行程650 工作环境温度-20℃~70℃ 工作压力16MPa,试验压力20MPa 活塞密封为TPM248185-63*47*18.3*6.4，活塞杆采用格莱圈和U型密封","台",2,"2023-07-30","340热轧"]
[44,7200600206,"液压缸","YF0176-23P","CD250E50/36-220A10/01CADMA;L10=200,带与位移传感器953AC40230MXXSX相配的磁环；不带传感器","台",3,"2023-05-30","89热轧"]
[45,7200600207,"液压缸","PB16Y000G","缸径80杆径56行程234压力等级25MPa","台",2,"2023-06-13","89热轧"]
[46,7200600213,"水冷式液压缸","125/90-380","中间铰接式;带水冷外壳;带缓冲;工作环境温度-20℃~150℃;工作压力15MPa;试验压力25MPa;活塞及活塞杆采用V型组合密封;工作介质聚酯抗燃液压油;附图","台",2,"2023-04-30","炼钢厂部"]
[47,7200600215,"液压缸组件","Z0202.03.02.03.00g1-7","油缸CD250E80/56-115A10/01CGDMA;L10=200;带耳环、铜套、碰块等附件","台",2,"2023-05-30","89热轧"]
[48,7201300014,"液压缸球铰耳环","CGAK35",null,"件",10,"2023-06-13","180热轧"]
[49,7201300030,"水平夹液压缸活塞杆1","HM-CG63/36-650-1",null,"件",10,"2023-06-13","340热轧"]
[50,7201300031,"水平夹液压缸6活塞杆2","HM-CG63/36-650-2",null,"件",10,"2023-06-13","340热轧"]
[51,7201300032,"水平夹液压缸活塞杆","HM-CG63/36-650-3",null,"件",10,"2023-06-13","340热轧"]
[52,7201300057,"液压缸球铰耳环","GAS90",null,"件",2,"2023-06-13","340管加工热处理"]
[53,7501800047,"液压缸耳环","GAK80","带80关节轴承","件",2,"2023-04-30","340管加工热处理"]
[54,7502000050,"液压缸耳环","GAK28",null,"件",8,"2023-06-13","89热轧"]
["投标人：                         （盖单位公章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日  期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2023年3月液压缸公开招标采购项目                项目编号：HGJY-G2023020"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位公章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日  期：      年      月      日                "]