{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":38,"n_cols":13,"rows_kept":38,"merged":[[0,0,0,8],[1,0,1,12],[34,0,34,8],[35,0,35,8],[36,0,36,8],[37,0,37,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2023年3月机械配件采购项目                     项目编号：HGJY-G2023025"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,7502500103,"离心高温风机转子组","Y6-30-11NO19.4F；1700.02转子组","含叶轮、轴、轴承、轴承座，总重1820Kg；叶轮工作温度120-260℃；正常使用寿命五年","套",1,"JB/T8689-1998","高辅工段","2023-04-29"]
[2,7001200098,"高压泵 泵底阀","H42X-2.5 Q/12","DN200","只",3,"Q/12 NJ3583-2001","340管加工热处理","2023-04-29"]
[3,5501200082,"烧结机17#、18#翻板阀；未部风箱翻板阀","FF1400-00",null,"套",1,"审核图纸","烧结","2023-04-29"]
[4,5719700002,"PP袋式污水过滤袋","180*810-150微米--2号；","过滤精度：150μm；过滤面积：0.5㎡；最大流量：40m3/h ；袋口固定环：镀锌钢圈","只",50,"GB12625-1990","管加工厂部","2023-04-29"]
[5,5501400007,"烧结;成品仓振动给料机","QZS-80-130F 不带电机；面宽800mm，长1300mm","铆焊","台",4,"JB/T8096-2013","烧结","2023-04-29"]
[6,7502400138,"机床切削液专用混配器","Master Mix M-10","配比浓度0%~20%，流量38升/分，进水口1/2英寸，出水口3/4英寸，水压：2bar~4bar","套",2,"Q/MT 005-2016","管加工厂部","2023-04-29"]
[7,7502400141,"加药搅拌轴及叶轮","750-32","搅拌轴：304不锈钢材质，直径32mm,长度：1200mm，实心；三叶叶轮：不锈钢材质，内孔Φ32mm，外直径Φ750mm，厚度6mm","套",2,null,"能源厂部","2023-04-29"]
[8,7001200297,"五柱塞往复泵;柱塞","5XND-315-0203-D","直径60;材质：锻38CrMoAl;原装厂家：成都西南水泵厂","件",5,"GB/T5015-2003","180管加工热处理","2023-04-29"]
[9,7501300094,"波纹膨胀节","复式通用型，DN1200","DN1200，工作温度250℃；工作压力：0.1MPa；补偿量：轴向50mm，横向70mm；介质：煤气；波纹管材质316L","件",1,"GB/T12777-1999","高炉","2023-04-29"]
[10,7001200290,"五柱塞往复泵;出水阀座","5XND-315-0106","材质：3Cr13;原装厂家：成都西南水泵厂","件",10,"GB/T5015-2003","180热轧","2023-04-29"]
[11,7001200291,"五柱塞往复泵;进水阀座","5XND-315-0104","材质：3Cr13;原装厂家：成都西南水泵厂","件",10,"GB/T5015-2003","180热轧","2023-04-29"]
[12,7001200286,"五柱塞往复泵;锥阀","5XND-315-0105","材质：3Cr13;原装厂家：成都西南水泵厂","件",20,"GB/T5015-2003","180热轧","2023-04-29"]
[13,5500800015,"旋风除尘输灰机","DS100T-AZ","16Mn DS100T-AZ 含机壳.轴.轴承座、带防爆电机、减速机、螺旋叶片(耐磨合金 厚度12mm).，电机型号YB3-200L-4,30KW,转速1470r/min,电机轴直径110 搅拌叶片采用高铬抗磨铸铁，硬度HRC≥50壳体采用16Mn优质板材焊接而成 板厚12mm，焊缝采用坡口焊接 搅拌轴采用40Cr轴头和厚壁缝钢管焊接制作，喷水管材质采用1Cr18Ni9Ti 金属构件等应进行除锈，内表面采用防锈底漆两道，外表面采用防锈底漆两道，面漆两道。","套",1,null,"高炉","2023-05-15"]
[14,5900100004,"带锯机夹钳","行程大于800mm，挡板高大于600mm","行程大于800mm，挡板高大于600mm，包含横梁，同步齿轮、齿条；适用于GB4280C双立柱卧式带锯床","套",1,"JB/T4318","检验检测中心","2023-04-29"]
[15,7502100045,"SAE法兰焊接组件","DSFS6002/1.4571","接管材质：不锈钢","只",15,"ISO7169-1998","89热轧","2023-04-29"]
[16,7502100046,"SAE法兰焊接组件","DSFS3003/1.4571","接管材质：不锈钢","只",10,"ISO7169-1999","89热轧","2023-04-29"]
[17,5702000065,"注水阀","ZSF127H","装配件，86kg","件",1,"审核图纸","89油管热处理","2023-04-28"]
[18,7001600001,"气动开关蝶阀","Z011-A-10-400","对夹式;通径400;压力1MPa","台",1,"GB/T8100-2006","炼钢厂部","2023-04-29"]
[19,7101600204,"气动开关蝶阀","Z011-A-10-300","对夹式;通径300;压力1MPa","台",1,"GB/T8100-2006","炼钢厂部","2023-04-29"]
[20,5602600071,"火焰切割机","F274C068D-0","切割圆坯规格φ220-φ330","套",1,"审核图纸","炼钢厂部","2023-05-29"]
[21,7100300441,"多功能水泵控制阀","JD745X-25","DN400,PN2.5Mpa，长度996mm，膜片疲劳弯曲：200万次无破损，最低动作压力：≤0.05MPa，缓闭时间：3 ～ 120S（可调节），水锤峰值：≤1.5倍水泵出口额定压力，水泵最高反转速度：≤1.2倍水泵额定转速，阻力损失：比旋启式止回阀减少约31%，阀体铸钢件，阀杆材质不锈钢1Cr18Ni9Ti2Gr13，主阀板座材质不锈钢，膜片材质金属网+天然橡胶","台",1,"CJ/T167-2002","高炉","2023-04-29"]
[22,7001200345,"五柱塞往复泵;连杆组套","5XND-315-0208","连杆和连杆盖组件，材质：锻45#;原装厂家：成都西南水泵厂","套",5,"GB/T5015-2003","340管加工热处理","2023-06-26"]
[23,7001200346,"五柱塞往复泵;十字头销","5XND-315-0206","材质：35CrMoA;原装厂家：成都西南水泵厂","根",5,"GB/T5015-2003","340管加工热处理","2023-06-26"]
[24,7001200347,"五柱塞往复泵;连杆衬套","5XND-315-0207","材质：ZCuSn10Pb1;原装厂家：成都西南水泵厂","只",5,"GB/T5015-2003","340管加工热处理","2023-06-26"]
[25,7102000082,"U型弹止阀","DZF4DN32-1","\"1、型号：DZF-3 DN25，组焊件，材质：Q235\n2、钢球内孔与卡座内孔要求同心，钢球在插入喷枪时要检验是否滚动灵活，不能卡阻\n3、法兰孔成90°方向\"","个",20,"审核图纸","高炉","2023-04-27"]
[26,7501300101,"波纹管膨胀节","SP-CS0702","三波波纹管，含法兰及拉杆，材质316L，厚度1.2mm，耐压0.4Mpa，带配套插销紧固件","套",1,"GB/T14525-1993","高炉","2023-05-12"]
[27,5501200135,"烧结机单辊破碎机;限矩型永磁耦合器","YCX1-0090/8","最大转速/rpm;740;传递功率/kW;90;额定转矩/N.m;1161.5;外形尺寸/mm;Φ550×241;设备重量/kg;120","套",1,"Q/320192MGNT001-2018","烧结","2023-05-12"]
[28,5501300058,"环冷机;隔振型永磁耦合器","YCL2-0015/6","最大转速/rpm;990;传递功率/kW;7.5;额定转矩/N.m;72.3;外形尺寸/mm;Φ330×93;设备重量/kg;50","套",2,"Q/320192MGNT001-2018","烧结","2023-04-29"]
[29,5900100003,"合金粒度检测过筛机","KMHA-0202","入料粒度；≤0-75mm；筛面倾角：0-10°；处理量：30-40t/h；出料粒度：筛孔10-50mm；10*28；配电机2台型号：YZO50-6；4kw；380V；筛板材质：聚氨酯","台",2,null,"物流中心","2023-04-29"]
[30,4201700136,"洗地吸干机","SK50/50","额定功率980W，水箱容积50L清水/50L污水，电瓶持续工作时间：3-5小时，清洗宽度：51cm，吸水宽度：75cm，噪音：小于70db，最大爬坡度：5%，清洁效率：2200平米/h，最大喷水量：2.6L/min，净重：80kg，吸水电机功率：450W，刷盘电机功率：500W，最小转弯半径：75cm，行车方式：手推","台",1,"EN60335-2-72","检验检测中心","2023-04-29"]
[31,7001200085,"高压泵 液压缸","APT245-105-S02-01-01-01",null,"台",2,"JB/T10205-2000","管加工厂部","2023-04-29"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2023年3月机械配件采购项目               项目编号：HGJY-G2023025"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":4,"n_cols":1,"rows_kept":4,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8]],"flags":["formulas_cached_only"]}
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]