{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":69,"n_cols":12,"rows_kept":69,"merged":[[0,0,0,11],[1,0,1,11],[65,0,65,8],[66,0,66,8],[67,0,67,8],[68,0,68,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2023年3月电气备件采购项目                    项目编号：HGJY-G2023026"]
["序号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家"]
[1,6100600106,"快熔","NGTC2  1000V/400A",null,"GB/T13539 IEC 60270","个",12,"180热轧","2023-04-30"]
[2,4100400065,"堵油型铜接线鼻子","*","25mm2","GB/T 14315-2008","只",50,"720厂部","2023-04-30"]
[3,6400400018,"绝对编码器","CE65M Nr:110-02904 Sn0621 11-27vDC pruif Nr.30253 6404 TR公司 D-78647","Schritte/Umdrehung Prog.(Max:4096) Umdrehung Prog.(Max:4096) Schnittstelle/Code SSI/Prog:Stebel.Nersion 2293 AN00 Ausgangspege1 RS422 option Trwinprong:Spannung:11-27vDC pruif Nr.30253 06404 绝对值型 金属外壳 外形尺寸∮65mm SSI输出 符合标准DIN EN 61000-6-4，DIN EN 61000-6-2",null,"只",2,"219厂部","2023-07-30"]
[4,6300700010,"操作面板","TP177A 6AV6 642-0AA11-0AX1 德国IEC61508","input:24V","德国IEC61508","块",1,"340热轧","2023-04-30"]
[5,6100500380,"时间继电器","H3YN-2 TIMER","AC200-230V ;50/60HZ;8针","GB14048.5","只",20,"180厂部","2023-04-30"]
[6,6100500353,"时间继电器","SK4-220d；0.1～3S","通电延时型空气延时头；延时动作时间0.1～3S；触头额定电流：0.95A主触头触点形式：双断电；工作条件：周围空气温度-50℃—+40℃，24小时的平均值不超过+35℃；空气的相对湿度为不超过50%；安装地点海拔不超过2000M；","GB14048.4-2010","只",20,"340热轧","2023-04-30"]
[7,6100600174,"熔断器","RN2-10KVA","0.5A",null,"只",12,"炼钢厂部","2023-04-30"]
[8,6100500367,"中间继电器","C10-A10FX","24VDC;带座;10A 250V AC1;10A 30V DC1;RELECO","JBT 56288-1999","只",30,"炼铁厂部","2023-04-30"]
[9,6400400049,"增量编码器","DKS40-E5J01000 带弹性联轴器9402 8*8 SICK","增量型 金属外壳 脉冲数1024 侧向电缆直接 10 V ... 30 V 供电，符合标准DIN EN 61000-6-4，DIN EN 61000-6-2","EN61000-6-2","只",2,"720厂部","2023-04-30"]
[10,6100300074,"断路器","DZ47-60,2P 20A","Ue:690V.50/60Hz","GB14048.2-2001","只",20,"340热轧","2023-04-30"]
[11,6100600035,"熔断器","RT28-32 2A",null,null,"只",4,"能源厂部","2023-04-30"]
[12,6600100392,"定量给料机","GM—BSC22—S02","使用准确度±0.5%;皮带宽度800mm;流量0-25t/h;配CFC-2000型控制仪表和SEW变频电机减速机;三路4-20mA信号输出;采用DUB2高精度数字式称重传感器和LE627测速传感器;50Kg/m*2m1根;下置式并带安装附件","GB/T7721-2007","套",2,"炼铁厂部","2023-04-30"]
[13,6000200465,"真空断路器","3AH4305-4 Ur=36KV/Isc=31.5KA/Ir=2000A/屏柜NX-40.5 带小车 德国IEC947","德国IEC947","德国IEC947","台",1,"炼钢厂部","2023-04-30"]
[14,6400500902,"枪内专用线","ADE-LDRX-QNX","配测温探头，长度：1.6m",null,"套",1,"炼铁厂部","2023-04-30"]
[15,6400500903,"枪外专用线","ADE-LDRX-QWX","长度：25m，12芯+视频线",null,"套",1,"炼铁厂部","2023-04-30"]
[16,6100900050,"控制柜","2000*800*800;标准",null,null,"台",1,"340热轧","2023-04-30"]
[17,6100600291,"电容","SKC 3M3-35B-1","10.5A/3300 350V","IEC  60831","只",15,"炼钢厂部","2023-04-30"]
[18,6100600292,"熔断器","170M5258","660V;400A;2KN/110","GB/T13539 IEC 60270","只",4,"炼钢厂部","2023-04-30"]
[19,6200200884,"操作面板","E82ZBC","Id:00417192;Prod;4500275960;Ser;0584;适用伦茨E82EV系列变频器","GB/T12668","块",2,"炼钢厂部","2023-04-30"]
[20,4100600069,"报警灯","8WD4 400-1AB","DIN VDE0660 T200;BA15d;电源等级230VAC/DC;红色;最大功率5w","IEC EN60947-5-1","只",6,"炼钢厂部","2023-04-30"]
[21,6300600076,"行车遥控发射接收器","F24-12S   一发一收   控制电压AC36V","防护等级IP65 186*61*51 遥控距离100米  11个单速按钮","GB/T22084.2-2008","套",1,"炼钢厂部","2023-04-30"]
[22,6200200752,"变频器","PowerFlex 753；20F11NC043JA0NNNNN  AB","输入电压：400V交流 输入频率：三相，47-63HZ：输出电压：0-400V 输出电流：43A 输出频率：三相，0-400HZ 一般负载：22KW","IEC61800","台",1,"180热轧","2023-04-30"]
[23,6100100221,"24V电源模块140V1","BM108.0","24VDC EV   B.M. ELETTRONICA","GB14048","块",2,"180热轧","2023-04-30"]
[24,4100300047,"内制编码器拉绳开关","JX-LS-DZ","电压：AC220V,通讯方式：CAN，硬接点数量：2常开2常闭，触点容量：DC24/15A-380/10A,复位方式：手动复位，编码设置：0-254，设置方式：红外遥控，显示方式：跳动提示，材质：铝压铸","JB/T  10960-2010","个",16,"炼铁厂部","2023-04-30"]
[25,6600200863,"取温取压探头组件","FPI6.151.194","探杆长度1700mm;材质不锈钢;带涂层","HJ76-2017","套",1,"炼铁厂部","2023-04-30"]
[26,6600200864,"电加热探杆","35*1700","探杆长度1700mm;材质不锈钢;220V-400W","HJ76-2017","只",1,"炼铁厂部","2023-04-30"]
[27,6600200865,"加热盒气体室","FPI5.814.476","CEMS-2000.  V4.0用;光程800mm","HJ76-2017","台",1,"炼铁厂部","2023-04-30"]
[28,6100500075,"中间继电器","RJ25-CL-D24 DC24V RU2S","IEC61810-1","IEC61810-1","只",5,"检验检测中心","2023-04-30"]
[29,6300500240,"UPS","HTM6006-30M","容量6KVA：输入电压380VAC±25％输入频率50/60Hz±10%，输出电压：220VAC±1％输出频率50/60Hz±0.5，切换时间0ms，后备时间0.5小时。主机内置输入输出隔离变压器，采用三旁路模式（静态、维修、应急）",null,"套",1,"219厂部","2023-04-30"]
[30,5700100181,"滑块","HGW55HA","下锁式；末端密封垫片；","THK","件",6,"89热轧","2023-04-30"]
[31,6400600522,"压力传感器","ISE30A-01-D","SUP 12-24VDC  CLASS2 40mA MAX\n\nOP.PRESS -0.1-1.0MPa","GB/T15478-1995","只",4,"89热轧","2023-04-30"]
[32,6200300095,"中频炉感应线圈","LZH-200-350","线圈连接端面至线圈外径总长度775mm，线圈内径380mm，功率300Kw，配连接水管卡簧，焊接部位不能漏水，材料必须采用紫铜管","JB/T2977-1992","只",2,"219厂部","2023-04-30"]
[33,4000200363,"35KV穿墙套管","CWC-35/1000A","35KV/1000A;尺寸：L:950\\L1：790\\L2：422\\L3：12\\d1:16\\d2:30\\a:200","JB/DQ2553-1989","只",12,"能源厂部","2023-04-30"]
[34,4100400277,"35KV冷缩电缆终端头","WLS-35/1.2","120-185mm2","GB/T 11017.3","套",6,"炼钢厂部","2023-04-30"]
[35,6300700072,"综合显示大屏","BCD4P-AN2P-176","VOITAGE:100-240VAC/50-60HZ","Q/IBRF7-2013","台",1,"炼钢厂部","2023-04-30"]
[36,4100600070,"永磁碰撞式安全门装置器","INCHI-CMS/D1A","额定电流6A;工作电压110-380V","QYQJ0308001-2013","台",10,"炼钢厂部","2023-04-30"]
[37,6100300300,"断路器","CM3-225M/33202;200A","额定工作电压 AC690V/400V；额定绝缘电压800V;额定频率50HZ/60HZ;额定电流200A;瞬时脱扣整定电流12In","IEC60947-2 GB14048.2","个",1,"180热轧","2023-04-30"]
[38,6400400169,"编码器","EB50B8-P4AR-1024 ADT201","5-30Vdc;Ser-Nr.:YD182779/2;ELCO",null,"只",1,"180厂部","2023-04-30"]
[39,6400600524,"位移传感器","CHMM0260S00201P8",null,null,"只",1,"720厂部","2023-04-30"]
[40,6400400156,"编码器","TVI50T-09BK0R6TN-01024","Part No.:187367-0012;Ser.No.:4 000 000/4 133 275;厂家:P+F","DIN 32878-1993","个",1,"340热轧","2023-04-30"]
[41,6400600115,"激光测距仪","SICK DME3000-111P No.1018063","外形:矩形 外壳材质:金属 检测模式/感应类型:光电测距型 供电范围:18-30DC 感应范围:0.2-30m 分辨率1mm Led显示 按键设置 输出:模拟量/mA/V 1PNP/NPN 接线方式：m12插头 防护等级:IP65","Q/RG2003-2013","台",2,"89油管车丝委外","2023-04-30"]
[42,6300200183,"KOYO输出模块","T1K-16TR","Outputs Per Module：16；Output Type： Relay Form A (SPST) normally open；Commons Per Module：4, 4pts. / common (isolated)","IEC 1000–5–1&2 /IEC 1131–4.","个",1,"检验检测中心","2023-04-30"]
[43,6300200184,"KOYO输入模块","T1K-16ND3","Inputs Per Module：16 (sink / source)；Input Current (Typical)： 4mA @ 12VDC, 8.5 mA @ 24VDC；Operating Voltage：12–24 VDC；Input Impedance： 2.8 kΩ","IEC 1000–5–1&2 /IEC 1131–4.","个",1,"检验检测中心","2023-04-30"]
[44,6300200185,"KOYO输出模块","T1H-EBC100","Module Type：Ethernet Slave； Communications：100Base-T Ethernet； Auto-configuring： I/O type/position automatically identified during power-up","IEC 1000–5–1&2 /IEC 1131–4.","个",1,"检验检测中心","2023-04-30"]
[45,6300400093,"KOYO电源模块","T1K-01DC","Input Voltage Range：12/24 VDC (10.8 - 26.4 VDC)； Maximum Power：20W； Maximum Inrush Current： 10A","IEC 1000–5–1&2 /IEC 1131–4.","个",1,"检验检测中心","2023-04-30"]
[46,6100300282,"户外防雨智能光控开关","ZYT26GK","\"五种光控模式感光范围可调；系统延时0~ 10分钟；PC阻燃材料；电源电压90~250VAC/DC50Hz/60Hz；照度范围0 .5Lux~5KLx；环境温度-10~50°C (但不凝霜)；环境湿度<85%PH25°C；防护等级IP55\n\n\n\n\n\n\n\n\"","NB/T 10290-2019","只",10,"物流中心","2023-04-30"]
[47,6400200106,"光栅","E02M-Q32L67-6X-H1151-0.5","发射端，发射端，供电电压;10-30VDC 距离：67mm TURCK","IEC61508","只",2,"89油管车丝委外","2023-04-30"]
[48,6200200890,"直流步进电机驱动器","Q2HB44MA","驱动电压：DC12-40V；最高反应频率200Kpps；供电：DC12-40V","JJG1140-2017","个",2,"检验检测中心","2023-04-30"]
[49,6400300243,"接近开关","J18-A8H","圆柱形，直径18mm，交流二线制，AC220V，常闭NC，感应距离8mm","GB/T 14048.10-2016","个",10,"检验检测中心","2023-04-30"]
[50,6200200401,"平移控制板","1050TCS",null,"GB/T3235-1999","块",2,"炼钢厂部","2023-04-30"]
[51,6100600019,"高压保险","RN2-35 0.5A",null,"GB9816-2008","只",10,"炼钢厂部","2023-04-30"]
[52,4000400026,"换气扇","APB25","220V","GB/T13380-2007","台",2,"能源厂部","2023-04-30"]
[53,6400600128,"流量开关","FCT-G1/2A4P-AP8X-H1141","FCT-G1/2A4P-AP8X-H1141","GB50397-2008","只",4,"340热轧","2023-04-30"]
[54,4000200190,"电刷","J164-Z","25*32*60",null,"只",30,"炼铁厂部","2023-04-30"]
[55,6100500250,"中间继电器","DZ52-22","220V",null,"只",30,"720厂部","2023-04-30"]
[56,6300600048,"比例阀电源板","VT-VSPA2-50-10/T5",null,"GB/T14048.10-2008","块",2,"340热轧","2023-04-30"]
[57,6400300126,"终端接头","订货号312705","五针",null,"只",3,"720厂部","2023-04-30"]
[58,6300200104,"前连接器","1756-TBCH","AB","IEC61508","只",1,"炼铁厂部","2023-04-30"]
[59,6300500068,"光纤","光纤 LWL Formkabel lsatz FSH",null,null,"根",3,"180厂部","2023-04-30"]
[60,6400200012,"对射冷探","M100/MV100-RT//76a 95/103","10-30VDC:检测距离 20m：信号输出 PNP","JB/T6475-1992","只",6,"180厂部","2023-04-30"]
[61,4100500380,"按钮开关","LAY16","φ22","JB/T 3907-1999","只",10,"检验检测中心","2023-04-30"]
[62,6400300123,"限位开关","LXJM1-8108","240v:5A:IP64",null,"只",15,"219厂部","2023-04-30"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2023年3月电气备件采购项目        项目编号：HGJY-G2023026"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}