{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["一、开标一览表","二、商务 技术偏离"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"一、开标一览表","index":0,"n_rows":46,"n_cols":11,"rows_kept":46,"merged":[[0,0,0,10],[1,0,1,5],[1,6,1,10],[42,0,42,10],[43,0,43,10],[44,0,44,10],[45,0,45,3]],"flags":["formulas_cached_only"]}
["开  标  一  览  表"]
["项目名称：2023年4月-2024年4月探伤备件年标采购项目",{"$nulls":5}," 项目编号：HGJY-G2023039"]
["序号","物料编码","物料描述","规格描述","技术参数","单位","数量","交货日期","含税单价（元）","生产厂家","备注"]
[1,5701700065,"12通道组合横向探头","HC120-H12-F5","2.5MHz9*12F60","只",2,"以订单为准",null,null,"需求量以订单为准"]
[2,6400500807,"超声波 纵横向双晶斜探头","蝙蝠5P 10*12*2 K1，纵向和横向","5MHz，尺寸10X12，K1，两个接头Q9，纵横向两个方向可以同时检测，附合格证 附性能测试报告","只",37,"以订单为准",null,null,"需求量以订单为准"]
[3,6400500806,"超声波 纵向双向斜探头","蝙蝠5P 10*12*2 K1，纵向双向","5MHz，尺寸10X12（mm)，K1，两个Q9接头，纵向两个方向可以同时检测，附合格证 附性能测试报告","只",26,"以订单为准",null,null,"需求量以订单为准"]
[4,6400500234,"超声波探伤仪","HS600","HS600附合格证 附性能测试报告","台",4,"以订单为准",null,null,"需求量以订单为准"]
[5,6400500336,"超声测厚仪 测厚探头","CTS-30A","5Z10FG-HC","只",66,"以订单为准",null,null,"需求量以订单为准"]
[6,6400500592,"超声探伤机;纵向探头橡皮线卡","313351",null,"只",60,"以订单为准",null,null,"需求量以订单为准"]
[7,6400500063,"检测探头","EMT-Z002","武汉华宇一目检测装备有限公司 附合格证","只",4,"以订单为准",null,null,"需求量以订单为准"]
[8,6400500255,"探伤机 超声信号线","SVT-UTSL Ⅱ-690",null,"根",395,"以订单为准",null,null,"需求量以订单为准"]
[9,6400500254,"探伤机 超声信号线","SVT-UTSL I-690",null,"根",180,"以订单为准",null,null,"需求量以订单为准"]
[10,6400600295,"探伤机 横向漏磁探头总成","DHCH244.48",null,"套",8,"以订单为准",null,null,"需求量以订单为准"]
[11,6400600294,"探伤机 横向漏磁探头总成","DHCH219.1",null,"套",8,"以订单为准",null,null,"需求量以订单为准"]
[12,6400600297,"探伤机 横向漏磁探头总成","DHCH339.7",null,"套",6,"以订单为准",null,null,"需求量以订单为准"]
[13,6400600298,"探伤机 横向漏磁探头总成","DHCH368",null,"套",6,"以订单为准",null,null,"需求量以订单为准"]
[14,6400600296,"探伤机 横向漏磁探头总成","DHCH273",null,"套",6,"以订单为准",null,null,"需求量以订单为准"]
[15,6400500118,"探伤机 漏磁耐磨块","EMT-Z002","武汉华宇一目检测装备有限公司 附合格证","块",25,"以订单为准",null,null,"需求量以订单为准"]
[16,6400500023,"探伤机 喷枪","PILOT SIGNIER 1.0mm","附合格证","件",5,"以订单为准",null,null,"需求量以订单为准"]
[17,6400500131,"探伤机 探头连接线","RG316","长度10000mm 附合格证","根",72,"以订单为准",null,null,"需求量以订单为准"]
[18,6400500031,"探伤机 特斯拉计","HT201","附合格证，校准证书","台",8,"以订单为准",null,null,"需求量以订单为准"]
[19,6400500033,"探伤机 荧光磁粉","1KG/瓶","HLY-20 附合格证","瓶",2430,"以订单为准",null,null,"需求量以订单为准"]
[20,6400500034,"探伤机 圆柱直筒万向球跟踪轮","HLM10-45","HLM10-45 附合格证","件",30,"以订单为准",null,null,"需求量以订单为准"]
[21,6400500834,"探伤机：16通道横伤探头","HC360-H16-F2.5-2","2.5MHz9X12X16;附测试性能报告","只",3,"以订单为准",null,null,"需求量以订单为准"]
[22,6400500833,"探伤机：8通道组合探头","HC360-FC8-F5-2","复合晶片5C12X12X8;附测试性能报告","只",3,"以订单为准",null,null,"需求量以订单为准"]
[23,6400500832,"探伤机：M通道纵伤探头","HC360-ZM-F2.5-2","2.5MHz12.5X14X10,F80;附测试性能报告","只",3,"以订单为准",null,null,"需求量以订单为准"]
[24,5701800017,"探伤机：测厚探头NCS-WRD06-F2.5","测厚探头NCS-WRD06-F2.5",null,"个",8,"以订单为准",null,null,"需求量以订单为准"]
[25,6400500737,"探伤机：横向漏磁探头总成","DHCH323","国产化直径323mm，带探头镶座, 两端带耐磨块，2个通道","套",6,"以订单为准",null,null,"需求量以订单为准"]
[26,6400500867,"探伤机：横向探头","HC360-H16-F2.5","2.5MHz  9*12  16.5度","只",2,"以订单为准",null,null,"需求量以订单为准"]
[27,6400500343,"探伤机;超声水蘘皮","*",null,"块",50,"以订单为准",null,null,"需求量以订单为准"]
[28,5721300001,"探伤机;超声探鞋悬挂杆子","3970210010",null,"根",4,"以订单为准",null,null,"需求量以订单为准"]
[29,6400600367,"探伤机;漏磁探头","JJTZ-16T   3358310010  SHOE ASSY，AMALOG 16CH MILL","长度200mm, 两端带耐磨钉，16个通道","只",2,"以订单为准",null,null,"需求量以订单为准"]
[30,6400500611,"探伤机;喷枪","PILOT SIGNIER 0.8mm",null,"只",4,"以订单为准",null,null,"需求量以订单为准"]
[31,6400500671,"探伤机；退磁机；","YSKTZ-30;","壁厚16的钢管，退磁后剩磁不高于10GS","套",1,"以订单为准",null,null,"需求量以订单为准"]
[32,6400500831,"探伤机;斜伤探头11°","HY365-X-F2.5-11°TS15HYHL2","8 14x12 2.5MHZ 不聚焦 Q9 附合格证/校准证书","个",2,"以订单为准",null,null,"需求量以订单为准"]
[33,6400500690,"探伤机;周向磁化线圈;","CXT-24000AT-ZHXQ-500","适用设备型号：CXT-24000AT","套",1,"以订单为准",null,null,"需求量以订单为准"]
[34,6400500866,"探伤机;纵向探头","HC360-Z10-F2.5","2.5MHz  12.5*14F80","只",2,"以订单为准",null,null,"需求量以订单为准"]
[35,5701000067,"探伤机平台升降机","SGT30L0-0-24-0-Ⅰ-S;E9608222;国产化","减速比1:24，适用设备DS2000,审核图纸","台",4,"以订单为准",null,null,"需求量以订单为准"]
[36,6400500199,"探伤机气阀Solenoid Valve","19789","Fosto","台",20,"以订单为准",null,null,"需求量以订单为准"]
[37,6400500053,"荧光磁粉","SVT-20","500目","Kg",100,"以订单为准",null,null,"需求量以订单为准"]
[38,6000400045,"周向磁化线圈","CXT-20000AT-ZHXQ-500","2.24直径双绕","套",2,"以订单为准",null,null,"需求量以订单为准"]
[39,6000400046,"纵向磁化线圈","CXT-20000AT-ZQXQ-260-120","2.24直径双绕   上海宇光","套",3,"以订单为准",null,null,"需求量以订单为准"]
["注：1、投标报价含税，税率13%                                                                                     \n2、生产厂家要求全称填写准确无误"]
["投标人：（盖单位章）"]
["法定代表人或其委托代理人：（签字或盖章）"]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离","index":1,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2023年4月-2024年4月探伤备件年标采购项目   \n项目编号：HGJY-G2023"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位公章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]