{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":51,"n_cols":13,"rows_kept":51,"merged":[[0,0,0,8],[1,0,1,12],[47,0,47,8],[48,0,48,8],[49,0,49,8],[50,0,50,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2023年5月机械备件采购项目                     项目编号：HGJY-G2023053"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,7502400138,"机床切削液专用混配器","Master Mix M-10","配比浓度0%~20%，流量38升/分，进水口1/2英寸，出水口3/4英寸，水压：2bar~4bar","套",2,"Q/MT 005-2016","管加工厂部","2023-06-26"]
[2,7102000049,"切割氧止回阀","DZH-A4",null,"只",5,"JB/ZQ4595-2006","炼钢厂部","2023-06-26"]
[3,7102000050,"预热氧止回阀","DZH-G(SH)",null,"只",5,"JB/ZQ4595-2006","炼钢厂部","2023-06-26"]
[4,7102100017,"疏水器","BS19H-16-40",null,"只",4,null,"烧结","2023-06-26"]
[5,5500300110,"全封闭型钢制拖链架","TLE125Ⅲ-250x300x5200","250x300x5200 材质：铝合金组件","套",1,"JB/T12471-2015","高炉","2023-06-26"]
[6,7500200005,"高粘度真空净油机;GZL-200","GZL-200","工作电压380V，总功率65KW","台",1,null,"180厂部","2023-06-26"]
[7,7001200098,"高压泵 泵底阀","H42X-2.5 Q/12","DN200","只",3,"Q/12 NJ3583-2001","340管加工热处理","2023-06-26"]
[8,7001200296,"五柱塞往复泵;挡水板","5XND-315-0213","材质：聚四氟乙烯;原装厂家：成都西南水泵厂","件",30,"GB/T5015-2003","340管加工热处理","2023-06-26"]
[9,7001200294,"五柱塞往复泵;柱塞套","5XND-315-0202-D","材质：2Cr13;原装厂家：成都西南水泵厂","件",10,"GB/T5015-2003","340管加工热处理","2023-06-26"]
[10,7502400146,"高压泵 缸盖下","A-45/20.02-08",null,"件",10,"GB/T13320","720厂部","2023-06-26"]
[11,7001200287,"五柱塞往复泵;中塞","5XND-315-0103","材质：2Cr13;原装厂家：成都西南水泵厂","件",5,"GB/T5015-2003","340管加工热处理","2023-06-26"]
[12,7001200346,"五柱塞往复泵;十字头销","5XND-315-0206","材质：35CrMoA;原装厂家：成都西南水泵厂","根",5,"GB/T5015-2003","340管加工热处理","2023-06-26"]
[13,7001200347,"五柱塞往复泵;连杆衬套","5XND-315-0207","材质：ZCuSn10Pb1;原装厂家：成都西南水泵厂","只",5,"GB/T5015-2003","340管加工热处理","2023-06-26"]
[14,7001200295,"五柱塞往复泵;填料环乙","5XND-315-0212-D","材质：聚四氟乙烯;原装厂家：成都西南水泵厂","件",20,"GB/T5015-2003","89热轧","2023-06-26"]
[15,7001200078,"高压泵阀座","APT245.105-100.01-03",null,"只",3,"GB/T5272-1985","89油管热处理","2023-06-26"]
[16,7001200079,"高压泵阀芯","APT245.105-100.01-04",null,"只",3,"GB/T5272-1985","89油管热处理","2023-06-26"]
[17,7001200120,"高压泵 锥阀","W8-65BI",null,"只",10,"GB/T8558-1997","340管加工热处理","2023-06-11"]
[18,7001200121,"高压泵 锥阀座","W9-65AI",null,"件",10,"GB/T8558-1997","340管加工热处理","2023-06-11"]
[19,4100400141,"型材切割机","J3G3400","功率2.2KW","台",3,"GB14807-1993","高炉/炼钢/340","2023-06-27"]
[20,5719700002,"PP袋式污水过滤袋","180*810-150微米--2号；","过滤精度：150μm；过滤面积：0.5㎡；最大流量：40m3/h ；袋口固定环：镀锌钢圈","只",50,"GB12625-1990","管加工厂部","2023-06-26"]
[21,7502500103,"离心高温风机转子组","Y6-30-11NO19.4F；1700.02转子组","含叶轮、轴、轴承、轴承座，总重1820Kg；叶轮工作温度120-260℃；正常使用寿命五年","套",1,"JB/T8689-1998","高辅工段","2023-06-26"]
[22,5602600071,"火焰切割机","F274C068D-0","切割圆坯规格φ220-φ330","套",1,"审核图纸","炼钢厂部","2023-06-26"]
[23,7102000082,"U型弹止阀","DZF4DN32-1","\"1、型号：DZF-3 DN25，组焊件，材质：Q235\n2、钢球内孔与卡座内孔要求同心，钢球在插入喷枪时要检验是否滚动灵活，不能卡阻\n3、法兰孔成90°方向\"","个",20,"审核图纸","高炉","2023-06-26"]
[24,5602600065,"单倍尺割枪","LDG-16","割枪总长1200;枪体1035;切割氧管接口DG1\";预热氧管接口DG1/2\";燃气管路接口DG3/4\";冷却水管接口DG1/2\"","把",5,"GB5108-1985","炼钢厂部","2023-06-26"]
[25,5722600122,"锯床带轮","锯床G4240/50上用，安装孔径38；5级变速","适配皮带B1295Li;","件",2,"JB/T 4318.4-2002","180热轧","2023-06-26"]
[26,5709500067,"线性导轨滑座","SHS65LV8ZZHH","SHS65LV8ZZHH ;末端密封垫片;带油嘴。","件",6,"HTK","340热轧","2023-06-26"]
[27,7500300030,"板式不锈钢冷却器","BR0.23-1.0-16","16m2;压力1.6MPa;板片材料304;厚度1.0;丁晴橡胶;水口DN65,同侧","台",1,"JB/T4715-1992","炼钢厂部","2023-06-26"]
[28,5900100004,"带锯机夹钳","行程大于800mm，挡板高大于600mm","行程大于800mm，挡板高大于600mm，包含横梁，同步齿轮、齿条；适用于GB4280C双立柱卧式带锯床","套",1,"JB/T4318","检验检测中心","2023-06-26"]
[29,6200300098,"炉门密封件","SX2-18-14TP-LM","含炉门保温棉、陶瓷杆、炉门锁；炉门方形档火砖500mm*500mm*50mm","套",1,"GB/T 9452-2012","检验检测中心","2023-06-26"]
[30,7100100268,"氧气二级减压阀","WH-ZZC-16B（自立式）","进口压力0.2MPa;DN50;法兰式/L=230;D=165;D0=125;H=430","只",1,"GB/T1226-2001","炼钢厂部","2023-06-26"]
[31,7100100269,"氧气一级减压阀","1788B（调压器）","进口压力0.28MPa;DN25;内螺纹/A=3.31\";B=4.69\";C=1.60\";D=6.84\"","只",1,"GB/T1226-2001","炼钢厂部","2023-06-26"]
[32,5300400270,"双向可逆皮带机校正器（槽式）","JHYJZP650AD-B   带宽650","露天双向可逆，包胶花纹主辊D159/d133×250，主托辊辊面衬胶采用复合聚氨脂材料，具有防冻、防滑、防脱落及耐磨性能，且满足当地气候温度，托辊具有防尘、防水，动作灵敏可靠，无噪音，调偏幅度大，带宽650，长1030×宽350×高360；不损伤皮带，表面胶层硬度不得低于60～70°(邵氏A型硬度)，质保期三年，质保期内无需更换任何配件。","个",2,"ZL202020201838.8","烧结","2023-06-26"]
[33,7502500109,"循环风机进出口软连接","\"进口软连接2880*890 L=300;\n出口软连接1980*1640 L=300；\"","材质：防火硅胶布；配套风机：AII 6850-1120；工作压力小于等于10000pa","套",1,"JB/T12235","能源厂部","2023-06-26"]
[34,7501300096,"筛下软连接","TTHBS-350-85-75","材质：帆线橡胶","套",2,"Q/LMJ016-2007","高辅工段","2023-06-26"]
[35,5501000072,"烧结筛筛板","TTHBS-350-2","单层双面悬臂棒条    材质：55CrSi","套",4,"JB5015-1985","高辅工段","2023-06-26"]
[36,5502000016,"无尘散料装车机","SZJ500 50m3/h","标准件 GB12625-1990螺旋机外壳厚度≥5mm,叶片厚度大于8mm水平螺旋长度4.8米，垂直螺旋长度1.2米，螺旋宽度550mm,高度520mm,电机转速1440r/min","台",1,"GB12625-1990","高辅工段","2023-08-11"]
[37,5300700001,"120t铁水罐车 车轮对","带轴箱",null,"套",3,"TB/T 1463-2015","物流中心","2023-07-12"]
[38,5300700010,"120t铁水罐车：侧架","侧架总长2300mm","材质2G230-450，铁路专用，两导框中心距1400mm，轴箱处导框宽度424mm","件",3,null,"物流中心","2023-06-12"]
[39,5300700003,"121t铁水罐车 摇枕","29221",null,"条",2,null,"物流中心","2023-07-12"]
[40,5300700009,"铁水车车钩总成","13#上作用车钩","含车钩、缓冲器、钩尾框、前从板、钩尾销","套",1,"TB/T1595-1996","物流中心","2023-06-26"]
[41,5300300712,"机车车钩钩舌","13#",null,"付",10,"TB/T2943.1-2007","物流中心","2023-06-11"]
[42,5300700012,"铁水走行车;上下芯盘","430×380mm","材质为2G230-450，借用铁路转8转向架下心盘，心盘内径305mm","套",12,null,"物流中心","2023-06-26"]
[43,7502500002,"轴流风机","125FZY2-S",null,"台",20,"GB/T 13933-2008","180热轧","2023-06-11"]
[44,6000200795,"轴流风机","EG-4A-4；400mm","0.46KW，380V，1400r/min","台",1,"JB/T 10562-2006","高辅工段","2023-06-27"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2023年5月机械备件采购项目     项目编号：HGJY-G2023053"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":4,"n_cols":1,"rows_kept":4,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8]],"flags":["formulas_cached_only"]}
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]