{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["一、开标一览表","二、商务 技术偏离"],"read":"whole","date_system":"1900"}

{"sheet":"一、开标一览表","index":0,"n_rows":44,"n_cols":11,"rows_kept":44,"merged":[[0,0,0,10],[1,0,1,10],[41,0,41,10],[42,0,42,10],[43,0,43,10]]}
["开  标  一  览  表"]
["项目名称：2023年6月-2024年5月五金日杂年标采购项目                                                                              项目编号：HGJY-G2023070"]
["序号","物料编码","物料描述","规格描述","技术参数","单位","数量","交货日期","含税单价（元）","生产厂家","备注"]
[1,4000700090,"一吨包装袋","装载量1吨",null,"件",2600,"以订单为准",null,null,"需求量以订单为准"]
[2,4000200040,"阀控密封铝酸电池","GFM300 CHAMPION","2V  300AH","只",108,"以订单为准",null,null,"需求量以订单为准"]
[3,4600100060,"防尘口罩","9502V+KN95","折叠式带阀","只",80000,"以订单为准",null,null,"需求量以订单为准"]
[4,3163100002,"高温喷号涂料","JR-100",null,"Kg",4300,"以订单为准",null,null,"需求量以订单为准"]
[5,8700800058,"RIHON利合牌微晶弹性抛光轮","SC80-300mm*50mm*32mm","材料硬度14P、抛光轮颜色：蓝色；原材料：微晶刚玉。性能：切削力强、粉尘少","个",500,"以订单为准",null,null,"需求量以订单为准"]
[6,4201700099,"纤维抛光轮","外径*厚度*中心孔：300mm*50mm*33mm","材料硬度等级：14P","块",2500,"以订单为准",null,null,"需求量以订单为准"]
[7,4600100059,"防尘口罩","9501V+KN95","折叠式带阀","只",80000,"以订单为准",null,null,"需求量以订单为准"]
[8,3301000054,"液体聚合氯化铝","PAC","氧化铝(AL2O3)的质量分数≥ 9.0%; 盐基度40-90%;密度(20oC)/(g/cm3)≥ 1.12;水不溶物的质量分数≤ 0.2%;pH(1%水溶液)3.5-5.0;砷(As)的质量分数 ≤ 0.0002%; 铅(Pb)的质量分数≤0.001%;镉(Cd)的质量分数≤0.0002%; 汞(Hg)的质量分数≤0.00001%六价铬(Cr+6)的质量分数≤0.0005%","吨",174,"以订单为准",null,null,"需求量以订单为准"]
[9,4600100025,"马头牌肥皂","200克",null,"块",54600,"以订单为准",null,null,"需求量以订单为准"]
[10,3301000055,"切削液","Master马思特 TRIM  SC310，每桶量：204L","水溶液推荐使用浓度： 3.0% - 10.0%","桶",21,"以订单为准",null,null,"需求量以订单为准"]
[11,4200700029,"角向磨光机","GWS6-125","GWS6-125","台",467,"以订单为准",null,null,"需求量以订单为准"]
[12,4600100058,"炼铁阻燃工作服","白色",null,"套",500,"以订单为准",null,null,"需求量以订单为准"]
[13,4600100017,"防护面屏安全帽支架","BD173B",null,"个",2850,"以订单为准",null,null,"需求量以订单为准"]
[14,4600100016,"防护面屏","SE-173A",null,"块",3130,"以订单为准",null,null,"需求量以订单为准"]
[15,4300600061,"应力环盒子进气出气口接头","T-400-1-4","PTFE材质，硫化氢腐蚀；包含公扣母扣，连接1/4英寸气管，一端是1/4NPT外螺纹连接，另外一端是1/4英寸卡套连接","套",385,"以订单为准",null,null,"需求量以订单为准"]
[16,5300800023,"送样专用三轮电动车","车身尺寸：3130*1110*1380，箱体尺寸：1600*1100*260","技术参数：功率1000w,电瓶45A;车速≤25km/h;带驾驶室；把式","台",11,"以订单为准",null,null,"需求量以订单为准"]
[17,3400100067,"过滤器填充料；无烟煤滤料","直径2~4mm","密度为1.57g/cm3。盐酸可溶率不应大于0.81%；","吨",62.92,"以订单为准",null,null,"需求量以订单为准"]
[18,4600100041,"耳塞1110子弹型","（两只要有线连接）",null,"付",27000,"以订单为准",null,null,"需求量以订单为准"]
[19,4600100010,"带嘴型防尘口罩","（3M3200型面具及3700型承接座）",null,"套",1600,"以订单为准",null,null,"需求量以订单为准"]
[20,6700100104,"X荧光光谱仪专用分析试剂","X荧光光谱仪专用分析试剂 67Li2B4O7：33LiBO2 有效期内，带有效证书，无水解，无结块变质AR1000g",null,"瓶",120,"以订单为准",null,null,"需求量以订单为准"]
[21,3300600037,"铁屑","1mm≤粒度≤4mm","要求干燥、无油","吨",10,"以订单为准",null,null,"需求量以订单为准"]
[22,4000100139,"LED配电房专用灯","BD-A95;","30W;220-240V;斑点照明","盏",800,"以订单为准",null,null,"需求量以订单为准"]
[23,4000400159,"车丝拧接机防护专用砂布","静电植砂ELECTRO COATED：    230*280（9in*11in)","230*280（9in*11in)","张",37000,"以订单为准",null,null,"需求量以订单为准"]
[24,4201700017,"角磨片","125*6*22；NO:1669161256",null,"片",17500,"以订单为准",null,null,"需求量以订单为准"]
[25,4000300077,"钢丝绳用铝套管","A型;","直径14mm","只",6000,"以订单为准",null,null,"需求量以订单为准"]
[26,7501100510,"卡套","T-400-SET","材质：特氟龙，与1/4英寸硫化氢气管相接的前后卡套","套",800,"以订单为准",null,null,"需求量以订单为准"]
[27,3301000009,"亚硝酸钠","（工业用)",null,"吨",7,"以订单为准",null,null,"需求量以订单为准"]
[28,3301000026,"锯床专用切削液","HJ-Y01；5Kg/桶",null,"桶",1100,"以订单为准",null,null,"需求量以订单为准"]
[29,4400400044,"稀土丝","直径2.1mm","主要元素:铈(Ce)99.98、镧（La）65.79","Kg",280,"以订单为准",null,null,"需求量以订单为准"]
[30,4201200034,"冲击试验机缺口拉刀","QCS-Y-2T;V/U型;W18Cr4V;HRC65-70;54齿;GB/T229",null,"个",8,"以订单为准",null,null,"需求量以订单为准"]
[31,6700400213,"英思特朗150吨拉伸机平板夹具","英思特朗1500KN万能试验机;专用拉伸夹具平钳口;5-25mm,一套共上下左右四块","适用于5-25mm，专用拉伸夹具平钳口","套",4,"以订单为准",null,null,"需求量以订单为准"]
[32,4200200007,"电动扳手",6906,null,"台",12,"以订单为准",null,null,"需求量以订单为准"]
[33,6600200727,"HXFQ-6S型焦炭反应性及反应后强度测定仪焦炭反应器","HXFQ-6S-FYQ","反应器耐高温合金钢，材质为GH3044,内径80mm±1mm,反应管壁厚不小于1.5mm，拖料筛片直径78±1mm，其上均匀钻3mm圆孔，孔间距5mm，筛片厚度1.5mm","套",7,"以订单为准",null,null,"需求量以订单为准"]
[34,4201700064,"园锥磨头","直径20*30",null,"只",32500,"以订单为准",null,null,"需求量以订单为准"]
[35,6700400155,"硫化氢实验堵头","非标，配M10试样",null,"只",210,"以订单为准",null,null,"需求量以订单为准"]
[36,4200700034,"酷刚玉砂轮片","230*6*22",null,"片",1100,"以订单为准",null,null,"需求量以订单为准"]
[37,4200700028,"角向磨光机","GWS6-100",null,"台",161,"以订单为准",null,null,"需求量以订单为准"]
[38,4300500029,"同步齿形带","BD114MGT-2520 USA278*26",null,"根",6,"以订单为准",null,null,"需求量以订单为准"]
["注：1、投标报价含税，税率13%                                                                                     \n2、生产厂家要求全称填写准确无误"]
["投标人：（盖单位章）"]
["法定代表人或其委托代理人：（签字或盖章）"]

{"sheet":"二、商务 技术偏离","index":1,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]]}
["   （二）商务/技术偏离表"]
["项目名称：2023年6月-2024年5月五金日杂年标采购项目                                                                              项目编号：HGJY-G2023070"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位公章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]