{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":73,"n_cols":12,"rows_kept":73,"merged":[[0,0,0,11],[1,0,1,11],[69,0,69,8],[70,0,70,8],[71,0,71,8],[72,0,72,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2023年6月电气备件采购项目                    项目编号：HGJY-G2023080"]
["序号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家"]
[1,6100300293,"万能式断路器","DW15-2500","额定电压1140v，50hz，额定电流2500A，额定极限短路分断能力25KA,额定运行短路分断能力20KA,长延时0.7-1In，0.4s瞬时3-6In，欠压脱口器分励脱口器储能电动机电压均为交流220v；断路器尺寸需与现有使用的一致。原厂家：浙江正泰电器股份有限公司","GB14048.2","台",1,"219厂部","2023-08-26"]
[2,6400200106,"光栅","E02M-Q32L67-6X-H1151-0.5","发射端，发射端，供电电压;10-30VDC 距离：67mm TURCK","IEC61508","只",2,"89油管车丝委外","2023-08-26"]
[3,6200200896,"AB PF755逆变器功率单元大风机","SK-R1-FAN1-F8","750系列通用PF750,Inv,Kit,Heatsink Fan,Frame 8","E0.967X","套",2,"219厂部","2023-08-26"]
[4,6200200895,"AB PF755逆变器主板小风机","SK-R1-FAN2-F8","750系列通用PF750,Internal Stir Fans With Tray,Frame 8","E0.967X","套",2,"219厂部","2023-08-26"]
[5,6400600531,"位移传感器","CI43-6-1BR08T10300SA4201A","量程300mm；电源24VDC;输出4-20mA，测量起始端以外保持4mA输出；超出测量末端保持20mA输出。8米屏蔽电缆直接；带磁环。Q/JT01-2011",null,"只",5,"219厂部","2023-08-26"]
[6,6200100099,"磨床走刀控制器（含直流调速驱动功能）","MJK-508Y-14","15-16脚接两线直流电机    两组供电电压12V  24V","GB50034-2004","块",2,"219厂部","2023-08-26"]
[7,6300500275,"通信模块","GRM300-TTO","DC 12~24V 12W 2个RS485 1个RS232 3个网口","DTL645","套",2,"219厂部","2023-08-26"]
[8,5300700016,"铁水车加盖：地面控制柜","LC8921-II/型","交流380伏","JB/T2785-2010","个",2,"物流中心","2023-08-26"]
[9,6300100129,"CPU模块","1756-L81E","1756-L81E","IEC61508","块",2,"219厂部","2023-08-26"]
[10,4000300229,"电缆桥架盖板","2000mm*400mm*1.5mm（长*宽*厚）","材质：镀锌钢板","GB/T 5117-1995","米",20,"219厂部","2023-08-26"]
[11,6000400083,"石灰活性度测定仪搅拌器","HD-571JBQ","搅拌器转速250～300r/min，搅拌浆杆：Φ6×250mm，材质：哈氏合金;搅拌叶片：0.5×10×60mm。","YB/T 105-2014","个",1,"检验检测中心","2023-08-26"]
[12,6200200912,"高温散热风扇","4650Z","230V、50Hz、115mA、2800r/min、19W","GB/T4706.27-2008","个",1,"检验检测中心","2023-08-26"]
[13,4200700105,"充电式吹风机","DCQF28(B型)","最大输出功率350W,吹吸两用，18V/4.0Ah锂电池两组，充电器一个，集尘袋 吹风管","GB3883.1-2005","台",3,"89油管车丝委外","2023-08-26"]
[14,6100900157,"操作台","1000*800*780mm","柜内PLC模块及导轨自供。","审核图纸","个",1,"89油管车丝委外","2023-08-26"]
[15,6000300263,"穿孔机主电机冷却器","GLSK-D15-2-250","换热功率250kW,风量123/s,水量35，进水温度35℃，出风温度40℃，工作水压0.1-0.4MPa,风机型号Y160M1-2/15kW 2台","审核图纸","台",2,"89油管车丝委外","2023-08-26"]
[16,6600300048,"全电子式电动执行器","LSDZ-U-1000","AC220V 输入输出4-20mA 配伺服控制器","JB/T8219-1999","台",1,"180厂部","2023-08-26"]
[17,6100600035,"熔断器","RT28-32 2A",null,null,"只",4,"能源厂部","2023-08-26"]
[18,6400200013,"对射式光电开关","OM30-EVP6 ELCO JT 2-30s/1499","外形:圆柱型 外壳材质:金属 检测模式/感应类型:对射式（接收器） 供电范围:10-30VDC 感应范围:0-25m 输出形式:PNP 输出特性:常开1点，常闭1点 接线方式:导线输出连接 防护等级:IP67","JT 2-30s/1499","只",16,"管加工厂部","2023-08-26"]
[19,4100400156,"铜接线鼻子","C240-16",null,null,"只",50,"炼钢厂部","2023-08-26"]
[20,6100600246,"熔断器","RSF-5G","AC1000V;1800A;BC100KA;长城熔断器","GB13539 IEC 60269","只",12,"180厂部","2023-08-26"]
[21,4000200298,"暗开关三联","10A250V",null,"GB15092．1-2003","只",10,"340热轧","2023-08-26"]
[22,6300700072,"综合显示大屏","BCD4P-AN2P-176","VOITAGE:100-240VAC/50-60HZ","Q/IBRF7-2013","台",1,"炼钢厂部","2023-08-26"]
[23,6400400055,"绝对编码器","RSP02-58-13+12-3-B-W1-DS","Profibus-Dp总线型绝对值型多圈编码器 主体尺寸:φ58 安装方式:φ36夹紧法兰，轴长20MM 10-30VDC供电 圈数:4096/单圈位置数:8192","IEC60947-5-1","只",3,"720厂部","2023-08-26"]
[24,6100300301,"真空断路器触头","JYN1-35","额定电流1600A;额定电压40.5KV;含动触头骨架、开口3毫米全铜28片镀银","GB/T21706-2008","只",4,"炼钢厂部","2023-08-26"]
[25,6100500246,"中间继电器","K22E","AC220V",null,"只",20,"炼钢厂部","2023-08-26"]
[26,6000300259,"力矩电机控制器","TMA-4B;20A","工作电压三相交流380V,±10％;频率50-60Hz;调节范围0-380V;不平衡率±3％","GB14048.4-2003","只",1,"炼钢厂部","2023-08-26"]
[27,6400300245,"接近开关","JKL28-M4B3B","电感式:金属外壳:M16圆柱型带螺纹:电源电压10...30VDC 200mA:检测距离2mm:三线制 pnp输出一常开:接插式:配M12标准插头线:油缸用:耐压500bar","GB/T 70.1-2000","只",10,"炼钢厂部","2023-08-26"]
[28,4100700194,"二极管","MD 200A/1600V","电流200A;耐压2000V","GB/T18904-2002","个",10,"炼钢厂部","2023-08-26"]
[29,6100600294,"熔断器","RS96B-200A/500V","圆柱型;电流200A;耐压500V","GB13539.1","个",30,"炼钢厂部","2023-08-26"]
[30,6100600295,"熔断器","RS96B-160A/660V","圆柱型;电流160A;耐压660V","GB13539.1","个",30,"炼钢厂部","2023-08-26"]
[31,6100600296,"熔断器","RS96B-100A/660V","圆柱型、电流100A;耐压660V","GB13539.1","个",30,"炼钢厂部","2023-08-26"]
[32,6100900140,"开关盒","200*150*120","长*宽*高：200mm*150mm*120mm；防水等级：IP67，硅胶密封条；内置安装好导轨","GB7251.1-1997","个",10,"720厂部","2023-08-26"]
[33,6200200904,"伺服驱动器","ASD-B3-7543-M","7.5KW,输入400vac,B3系列,CANOPEN通讯","IEC60130","台",2,"720厂部","2023-08-26"]
[34,6400100043,"热金属检测器","HMD4-4ZC1","电源DC24V，输出24VDC高电平，负载能力>100mA，响应时间 接点＜20ms 电平与隔离＜2ms，检测温度550℃～1400℃，检测距离0.2m～8m，外壳形式 带冷却，功耗≤5W，保护  直流输入极性保护，电平输出短路及过载保护，带红光瞄准，灵敏度可调节，有电源及信号工作指示，可自检",null,"台",2,"340管加工热处理","2023-08-26"]
[35,7500300031,"散热器","OR-250","长780mm；直径：139mm；进出油口：6分；进出水口：6分；内部铜管冷却，工作压力：1MPa；换热量：60L","JB/T4715-1992","台",1,"烧结","2023-08-26"]
[36,6200200899,"制动电阻","3kW/18R","配CS710-4T30GB变频器，电阻值:18R,制动功率:3kW","IEC61800","台",2,"炼铁厂部","2023-08-26"]
[37,6300400095,"24V电源","DRP-240-24","INPUT:AC 100-240V 3.5A 50/60HZ  OUTPUT:DC 24V 10A","IC947","台",2,"炼铁厂部","2023-08-26"]
[38,6200200900,"PLC-通讯模块","CM-1243-5","CM-1243-5 PROFIBUS DP-MASTER","IEC97-1991","块",2,"炼铁厂部","2023-08-26"]
[39,6200200901,"HY多功能控制器","HY505","AC 220V",null,"台",1,"炼铁厂部","2023-08-26"]
[40,6400500911,"A/D板卡","HK-6210-4","4路4-20mA，PCI插口","GB/T26225-2010","个",1,"炼铁厂部","2023-08-26"]
[41,6100600303,"-/110 T型微型开关指示器（快速熔断器）","170M6201","额定电流：1400A;弧前焦耳积分1250000；1000V时总焦耳积分：6000000；功率损耗：150；1100V;BUSSMANN","GB/T 23521-2009","个",10,"340热轧","2023-08-26"]
[42,6100600304,"微动开关","170H0235","T型指示器类型，配一个常开触点和常闭触点，额定电流2A，额定电压250V；6.3*0.8mm接线片","GB/T 23521-2009","个",10,"340热轧","2023-08-26"]
[43,6200200903,"冷却风机","W2E200-HH38-06","带反馈点，225*225*80mm，风量：925/1030M3/h,103050/60HZ,60/80W;230V；Ebmpapst","GB/T22712-2008","台",3,"340热轧","2023-08-26"]
[44,6300700076,"工业无线遥控器","F21-E1B;带发射器、接收器","AC/DC 12V-72V;接收频率灵敏度≥-110dBm;发射频率输出功率≤4dBm",null,"套",4,"180热轧","2023-08-26"]
[45,4000200037,"短接片","280-402","WAGO","GB/T15887-1995","包",10,"180热轧","2023-08-26"]
[46,4100400289,"电缆桥架","50*25*2200；（宽*高*长mm）","材质：镀锌钢板，配盖板，厚度0.8mm","GB/T 5117-1995","件",15,"能源厂部","2023-08-26"]
[47,6200200898,"变频器","NZ200-22G/30P-4  22KW","输入电压3PH AC380V±5%;输入电流46A;输出功率22KW;容量37KVA;输出电流45A;过载能力（60s）67.5A",null,"台",1,"180热轧","2023-07-27"]
[48,6400300246,"耐高温行程开关","JDHK-3GL","浇铸全封闭滚臂型;触头1NO/1NC;5A/AC 220V;耐热温度550℃;防护等级;IP67标准","JB/T 5553-2006","个",30,"炼钢厂部","2023-07-12"]
[49,6400400172,"编码器安装支架","Angled flange 9203","编码器安装支架，配RVI58N-011BER61T-10000编码器使用",null,"块",4,"340管加工热处理","2023-08-26"]
[50,6200200908,"电抗器","OCL-0120-EISC-E58UC","功率：45KW;额定电流：120A；电感0.06mH;压降：1%；绝缘等级F级；规格：D*H*W:195*165*165mm，D1*W1：150*88mm；a*b:8*15mm；材质Cu;重量：9kg;品牌：EAGTOP","GB/T1094.6-2011","台",2,"340热轧","2023-08-26"]
[51,6400600415,"激光测距仪","DIMETIX-DAN-30-150","DIMETIX；订货号：500634；  工作电压：12...30 VDC；  自然表面量程：0.05...~100 m；   激光、红色可见光； 典型精度 @ 2s：± 3 mm； 模拟量输出，可编程, 0/4...20 mA；",null,"台",1,"炼钢厂部","2023-08-26"]
[52,6200300109,"霍尔电源","HR1603","输出信号直流0-10V","JB/T 7490-2007","台",1,"炼钢厂部","2023-07-12"]
[53,6400600534,"霍尔传感器","HV100","测量电压0-2500V;输出电流0-50mA;电源电压±15V;额定输入/输出有效值电流10mA/50mA","JB/T 7490-2007","台",1,"炼钢厂部","2023-07-12"]
[54,6100900149,"KP检查板","CHK-1706","供电24V;16路检测回路;1路保护输出","JB/T 7490-2007","块",1,"炼钢厂部","2023-07-12"]
[55,6100900150,"脉冲板","MB2-1406","2路磁环脉冲;原副边耐压10KV","JB/T 7490-2007","块",1,"炼钢厂部","2023-07-12"]
[56,6100900151,"脉冲板","MB3-1406","3路磁环脉冲;原副边耐压10KV","JB/T 7490-2007","块",1,"炼钢厂部","2023-07-12"]
[57,6100900155,"三合一变压器板","5KA-1306A","电流以及保护信号取样;5A/0.1A","JB/T 7490-2007","块",1,"炼钢厂部","2023-07-12"]
[58,4100700153,"声光报警器","TGSG-06D","220V",null,"台",10,"炼钢厂部","2023-08-26"]
[59,6000300253,"多合一智能电动机转子控制器","RSC1-M1-500R2-3","转子额定开路电压≤AC500v;用于三相交流电动机3段转子电阻器的控制","GB/T3235-1999","台",1,"炼钢厂部","2023-07-12"]
[60,6100900145,"多功能智能控制板","MFCHARGE","输入电压AC/DC110~245V;AO输出DC12V; 0~10V;DI输入;6输入;DO输出;6输出","GB/T16261-1996","块",1,"炼钢厂部","2023-07-12"]
[61,6100900146,"主控板","MFMC-200","输入电压AC/DC;110~245V;AO输出DC12V; 0~10V;DI输入;12输入;DO输出：8输出","GB/T16261-1996","块",1,"炼钢厂部","2023-07-12"]
[62,6100900147,"智能脉冲控制板","QLWKV3009","输入电压AC220V;输出;脉宽调制10路;AI输入;1路;DI输入;2路;DO输出;1路","GB/T16261-1996","块",1,"炼钢厂部","2023-07-12"]
[63,6000300262,"电机保护器","SOCK-DZS1","AC245V;保护功能;过流、欠电流、缺相、不平衡、堵转;0-100A","GB/T14598.18-2012","台",5,"炼钢厂部","2023-07-12"]
[64,6200100093,"变频器","MD480T37GB","37KW","EN61800-3","台",3,"720厂部","2023-06-27"]
[65,6100300302,"固定式断路器","HD4s-40.5MX-1600A-25kA","额定电压40.5KV;额定频率50Hz;额定电流1600A;3秒热稳定电流（有效值）25kA;额定动稳定电流（峰值）63kA;额定短路开断电流25kA;额定短路关合电流63kA;辅助电源电压;控制回路DC220V;储能电机DC220V;合闸时间55-67ms;分闸时间33-45ms;燃弧时间＜15ms;合闸弹跳时间≤2mS;机械循环寿命10000次;电气循环寿命符合E2级规定;ABB","GB1984-2001","台",1,"炼钢厂部","2023-08-26"]
[66,6200200906,"变频器","C200-044 00135 A 5.5KW","I/P 380-480V, 50-60HZ , 3ph , 16.3A ;O/P 0-480V, 0-550HZ ,3ph ,13.5A;S/N:8978528025;By Control Techniques",null,"台",1,"180热轧","2023-07-27"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误\n3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2023年6月电气备件采购项目        项目编号：HGJY-G2023080"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}