{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":17,"n_cols":13,"rows_kept":17,"merged":[[0,0,0,8],[1,0,1,12],[13,0,13,8],[14,0,14,8],[15,0,15,8],[16,0,16,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2023年6月阀门采购项目                     项目编号：HGJY-G2023081"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,7102000088,"止回阀","H41H-16C;DN100","1.6MPa","台",2,"GB/T3452.1-1992","89热轧","2023-07-27"]
[2,7101800276,"高压球阀","QJH-25wl","31.5MPa","只",4,"GB/T9065.2-2010","高炉","2023-07-27"]
[3,7102500014,"电动扇形阀","F943X-2.5","0.25MPa，DN1600，适用温度300℃，适用介质：煤气、烟气等，配防爆型电动装置；配两端法兰、金属垫片及螺栓","套",1,"GB/T6901-1993","能源厂部","2023-07-27"]
[4,7102000083,"多功能水力阀","JD745SH-16","DN125;PN16;阀轴材质不锈钢;阀板阀体为铸钢;介质;工业新水;带进出口配对法兰及连接件、密封件;接管外径φ133mm","只",1,"GB/T3452.1-1992","炼钢厂部","2023-07-27"]
[5,7100100011,"弹簧式安全阀","SFA42Y-320,Pg32MPa,Dg25mm",null,"只",2,"GB/T12241","180管加工热处理","2023-07-27"]
[6,7101600240,"电动耐磨尘气蝶阀","D941W-2.5C","介质;含尘烟气;规格DN3700mm;L=500mm;工作压力-7000Pa t≤100℃;电动执行器驱动、带电动执行机构;N=5.5kW/380V;电动阀要求具备阀位反馈功能、不带现场操作箱、可远程控制或就地控制;带过力矩保护及开、关到位保护装置;带进出口配对法兰及连接件、密封件","台",3,"GB/T12238-2008","炼钢厂部","2023-07-27"]
[7,7100100270,"安全阀","A48Y-16C-80；","铸造；压力等级0.6~1.0Mpa；整定压力0.6Mpa","台",1,"GB/T12243-2005","高炉","2023-07-27"]
[8,7100100271,"不锈钢减压阀","Y43W-25P-DN150","DN150通径，材质：不锈钢,进口压力12∽16公斤压力，出口压力8公斤压力","台",1,"GB/T12244-2006","高炉","2023-07-27"]
[9,5500500046,"煤气切断阀","D944P-0.5 DN1600","公称压力0.05Mpa，阀体材质Q235B","台",1,"JB/T 11597-2013","高炉","2023-07-27"]
[10,7102300005,"电动敞开式插板阀","CCF944X-0.5","适用介质：高炉煤气，公称压力：0.05MPa，公称通径：DN2000mm，介质温度<=300摄氏度，阀体材料：Q235","台",1,"TS2710C28-2011","高炉","2023-07-27"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误\n3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2023年6月阀门采购项目           项目编号：HGJY-G2023081"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":4,"n_cols":1,"rows_kept":4,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8]],"flags":["formulas_cached_only"]}
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]