{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":45,"n_cols":13,"rows_kept":45,"merged":[[0,0,0,8],[1,0,1,12],[41,0,41,8],[42,0,42,8],[43,0,43,8],[44,0,44,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2023年6月机械备件采购项目                     项目编号：HGJY-G2023082"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,5900100004,"带锯机夹钳","行程大于800mm，挡板高大于600mm","行程大于800mm，挡板高大于600mm，包含横梁，同步齿轮、齿条；适用于GB4280C双立柱卧式带锯床","套",1,"JB/T4318","检验检测中心","2023-07-27"]
[2,5704800005,"高压泵;齿轮","JAJ60/178-10","45# 3.8Kg","件",7,"审核图纸","89油管热处理","2023-08-11"]
[3,7502500106,"屋顶通风机","DWT-I-7","底座尺寸1000*1000mm，风罩直径1220mm，电机 三相380V 转速960，功率1.5Kw，风量12500-17500m3/h","台",2,"JB/T2977-1992","219厂部","2023-07-27"]
[4,7001300004,"清洗泵","型号：OD2N1-3X24","功率4KW；扬程216m","台",1,"GB/T26135-2010","219厂部","2023-07-27"]
[5,5300700017,"铁水车加盖总装配","120吨","L C81505.01","套",2,null,"物流中心","2023-07-27"]
[6,5300700018,"铁水车加盖总装配","45吨位","L C81102.01","套",2,null,"物流中心","2023-07-27"]
[7,7101600203,"气动开关蝶阀","Z011-A-10-250","对夹式;通径250;压力1MPa","台",3,"GB/T8100-2006","炼钢厂部","2022-09-18"]
[8,7502400138,"机床切削液专用混配器","Master Mix M-10","配比浓度0%~20%，流量38升/分，进水口1/2英寸，出水口3/4英寸，水压：2bar~4bar","套",2,"Q/MT 005-2016","管加工厂部","2022-09-26"]
[9,7101800139,"气动球阀","DN80 ANSI 300 ASMEB16.5","铸钢 F30，CL300，AIR TO CLOSE，ASTM A479，TYPE316，TFM-1600","只",2,null,"高辅工段","2023-07-27"]
[10,5500800013,"星形卸灰阀","YXD-570","570*570 高度600 带电机 铸钢 GB16490-1996 工作温度450℃，介质：高炉瓦斯灰，壳体材质：Q235，叶轮材质：不锈钢，叶轮与壳体间隙30丝，轴密封采用石墨盘根，扎三圈，便于更换，带电机、减速机电动机型号 YKF2-100L1-4 电压 380V，电流 5.09 轴伸端轴承 6206-2RS 功率2.2KW 减速机型号 XLD4-2B","套",3,"GB16490-1996","高炉","2023-07-27"]
[11,5501200134,"柔性翻板式新型双层卸灰装置","JYXF300×1800","\"驱动方式：下阀板分别由单个独立液压缸驱动；液压站（含滤油器+缓冲装置）：电机功率：2.2KW   厂家：节能高效电机\n油泵：康百世齿轮泵   ；密封件材质：橡胶软密封（耐温200℃）；工作压力：16Kpa～20Kpa；物料堆重比：2.2t/m3；漏风率：≤0.05%\"","套",2,"审核图纸","烧结","2023-07-27"]
[12,5601500004,"钢包烘烤器主烧嘴","FY-HGQ-01","出厂前烧嘴砖需要完成低温烘烤","套",1,"审核图纸","炼钢厂部","2023-07-27"]
[13,5601500005,"钢包烘烤器点火烧嘴(长明火烧嘴)","FY-HGQ-02","不锈钢","套",1,"审核图纸","炼钢厂部","2023-07-27"]
[14,5500500034,"离心通风机","NGP300A","540m3/h,全压2156Pa;电机0.75Kw;2900r/min","台",1,"GB/T14048","高辅工段","2023-07-27"]
[15,6400100035,"免烘烤型连续测温管","HFC-G-IV-C-1100-95B","测 量 范 围:800～1800℃;测量不确定度:±3℃;测温管寿命:≥30小时;响应时间:热态响应时间≤ 75s","根",30,null,"炼钢厂部","2023-07-27"]
[16,5603200037,"滤袋","Φ130×7000;花板孔直径138mm","PTFE+覆膜+防油防水处理","条",200,"GB12625-1990","炼钢厂部","2023-07-27"]
[17,5705200032,"袋式除尘器滤袋","DM85.5 直径130*1800","覆膜涤纶针刺选毡","件",120,"GB12625-1990","180热轧","2023-07-27"]
[18,7001200253,"高压泵 直通体","(79)20A-ZZTM36.30.12-01",null,"件",10,"JB/T9872-2000","340管加工水压","2023-07-27"]
[19,5705300022,"带锯机","G4250/85",null,"台",1,"JB/T4318.4-2002","180热轧","2023-07-27"]
[20,6400600470,"点火电极","ZHLJ1SFSV 400N-300","L=650MM   陶瓷+不锈钢芯","根",10,"GB/T26800-2011","180管加工热处理","2023-07-27"]
[21,6400600471,"检测电极","ZHLJ1SFSV 400N-300-1","L=650MM 陶瓷+不锈钢芯","根",10,"GB/T26800-2011","180管加工热处理","2023-07-27"]
[22,6400600472,"点火电极","ZHLJSFSV  190N-250/185M","L=400MM 陶瓷+不锈钢芯","根",10,"GB/T26800-2011","180管加工热处理","2023-07-27"]
[23,6400600473,"检测电极","ZHLJ2SFSV 190N-250/185M-1","L=400MM 陶瓷+不锈钢芯","根",10,"GB/T26800-2011","180管加工热处理","2023-07-27"]
[24,6400600474,"点火电极","HHLJ1SCEM190LN-200/135M","L=400MM 陶瓷+不锈钢芯","根",10,"GB/T26800-2011","180管加工热处理","2023-07-27"]
[25,6400600475,"检测电极","HHLJSCEM190LN-200/135M-1","L=400MM 陶瓷+不锈钢芯","根",10,"GB/T26800-2011","180管加工热处理","2023-07-27"]
[26,5721100003,"G4225带锯床 导向头总成","导向头总成,含合金导向块.耐磨合金键.轴承","G4225","只",4,"JB/T4318.4-2002","180管加工热处理","2023-07-27"]
[27,7001200011,"高压泵 除磷环喷嘴紫铜垫","*",null,"只",50,"JB/T9872-2000","340热轧","2023-08-11"]
[28,5501000051,"焦丁筛聚氨酯筛板（15）","1310*320*30开孔（15mm）","包含整套焦丁筛所用聚氨酯HPM筛板和聚氨酯HW12接料筛板。堵孔率小于10%（非接料区），筛分效率大于90%，使用寿命大于9个月，筛面不用人工清理。","套",1,null,"高辅工段","2023-07-27"]
[29,5501000072,"烧结筛筛板","TTHBS-350-2","单层双面悬臂棒条    材质：55CrSi","套",2,"JB5015-1985","高辅工段","2023-07-27"]
[30,5501000078,"槽下环保筛激振器","TTXY-160","通轴管式激振器，采用稀油润滑，无需配备润滑站和供油系统，注油和放油采用管式，注油和放油均在外边操作，轴承采用中美合资品牌TWB振动专用轴承，激振器轴的材料为40Cr，调质处理220 HBW～250 HBW","套",2,"GB11349.2-1989","高辅工段","2023-07-27"]
[31,7501300106,"金属补偿器","DN300;PN6;L180","附结构图:3#VD-SSJ-03","件",2,"GB/T12777-2019","炼钢厂部","2023-07-12"]
[32,7501300107,"金属补偿器","DN250;PN10;L260","附结构图;3#VD-SSJ-04","件",2,"GB/T12777-2019","炼钢厂部","2023-07-12"]
[33,7501300108,"金属补偿器","DN300;PN10;L180","附结构图;3#VD-SSJ-05","件",2,"GB/T12777-2019","炼钢厂部","2023-07-12"]
[34,7501300109,"金属补偿器","DN400;PN10;L250","附结构图;3#VD-SSJ-06","件",2,"GB/T12777-2019","炼钢厂部","2023-07-12"]
[35,7501300110,"膨胀节","DN900;PN10;L400","附结构图;3#VD-SSJ-07","件",2,"GB/T12777-2019","炼钢厂部","2023-07-12"]
[36,7501300113,"法兰式伸缩节","DN150，介质：瓦斯灰，温度≤500℃","总长380，伸缩量±40，总行程340-420mm；设计额定压力PN16，短时上限压力PN25，瞬时上限压力PN40。额定耐温300度，上限温度500度；法兰连接，顶部法兰是DN150PN10，底部法兰是DN200PN16的。","件",2,"GB/T 12465-2017","高炉","2023-07-12"]
[37,4200700104,"拉丝机(自带拉丝轮)","SIN-FF-120×100","1.1400瓦可调速；二级齿轮传动，2.额定频率：50Hz;  额定电压：220V； 输入功率：1400W； 额定转速：693-3800r/min;  抛光轮尺寸：120×100mm","台",10,"CNS 11155-1984","180热轧","2023-07-27"]
[38,5501200134,"柔性翻板式新型双层卸灰装置","JYXF300×1800","\"驱动方式：下阀板分别由单个独立液压缸驱动；液压站（含滤油器+缓冲装置）：电机功率：2.2KW   厂家：节能高效电机\n油泵：康百世齿轮泵   ；密封件材质：橡胶软密封（耐温200℃）；工作压力：16Kpa～20Kpa；物料堆重比：2.2t/m3；漏风率：≤0.05%\"","套",2,"审核图纸","高辅工段","2023-07-27"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误 \n3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2023年6月机械备件采购项目       项目编号：HGJY-G2023082"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}