{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":35,"n_cols":13,"rows_kept":35,"merged":[[0,0,0,8],[1,0,1,12],[31,0,31,8],[32,0,32,8],[33,0,33,8],[34,0,34,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2023年7月机械备件采购项目                    项目编号：HGJY-G2023115"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,5900100004,"带锯机夹钳","行程大于800mm，挡板高大于600mm","行程大于800mm，挡板高大于600mm，包含横梁，同步齿轮、齿条；适用于GB4280C双立柱卧式带锯床","套",1,"JB/T4318","检验检测中心","2023-07-28"]
[2,7001300004,"清洗泵","型号：OD2N1-3X24","功率4KW；扬程216m","台",1,"GB/T26135-2010","219厂部","2023-07-28"]
[3,7502300063,"不锈钢扇形喷嘴","70代码5.2MM孔径","4分外丝，孔径5.2毫米，角度65","个",150,"GB/T3098.6-2000","89热轧","2023-09-26"]
[4,7101600238,"双法兰蝶阀","F012-K1 DN800","阀体材质:球墨铸铁GGG-40;阀板材质:不锈钢1.4408:阀杆材质:2Cr13:阀座密封材质:EPDM:连接方式:双法兰:法兰连接标准;EN1092 PN10:阀板工作压力:3bar:执行机构:EB20.1-SYD 双作用气功:限位开关:SBU 机械式:电磁阀;ASCO DC24V","只",1,"EN 1092","炼钢厂部","2023-09-26"]
[5,5500500034,"离心通风机","NGP300A","540m3/h,全压2156Pa;电机0.75Kw;2900r/min","台",1,"GB/T14048","高辅工段","2023-09-26"]
[6,7001200011,"高压泵 除磷环喷嘴紫铜垫","*",null,"只",50,"JB/T9872-2000","340热轧","2023-09-26"]
[7,7501300113,"法兰式伸缩节","DN150，介质：瓦斯灰，温度≤500℃","总长380，伸缩量±40，总行程340-420mm；设计额定压力PN16，短时上限压力PN25，瞬时上限压力PN40。额定耐温300度，上限温度500度；法兰连接，顶部法兰是DN150PN10，底部法兰是DN200PN16的。","件",2,"GB/T 12465-2017","高炉","2023-09-26"]
[8,4200700104,"拉丝机(自带拉丝轮)","SIN-FF-120×100","1.1400瓦可调速；二级齿轮传动，2.额定频率：50Hz;  额定电压：220V； 输入功率：1400W； 额定转速：693-3800r/min;  抛光轮尺寸：120×100mm","台",10,"CNS 11155-1984","180热轧","2023-09-26"]
[9,5400300039,"双罐煤气冷凝水排水器","XG－100L，带沉降过滤功能","介质：高炉煤气，工作压力：300Kpa，工作温度≤100℃，罐体材质Q235B，厚度12mm，小罐进口阀DN100PN16，小罐排污阀DN50PN25，大罐排水阀DN50PN25，大罐排污阀DN50PN25，阀门均为不锈钢球阀，做耐压试验，试验压力1Mpa无泄漏","套",1,"GB6222","高炉","2023-09-26"]
[10,7501300111,"方形法兰不锈钢补偿器","1400*980","Pn1.0MPa;介质:高温煤气;工作温度：≤300℃;材质：316L;轴向位移69mm;","套",1,"审核图纸","高辅工段","2023-09-26"]
[11,5501400037,"烧结环保筛激振器","HBZZ-40-6","单轴座式激振器，采用润滑脂润滑，轴承采用中美合资品牌TWB振动专用轴承，激振器轴的材料为40Cr，调质处理220HBW~250HBW；轴承型号：22216CA/W33","台",2,"GB11349.2-1989","烧结","2023-09-26"]
[12,5501400034,"烧结;A2筛筛板(二)","HBS2050(TTHBS-450-1)-b","上层棒条直径16mm，长度270mm，间距25mm；下层棒条直径16mm，长度320mm，间距16mm；棒条材质HBZL-5CrSiV；棒条布置角度16°","件",1,null,"烧结","2023-09-26"]
[13,5501400035,"烧结;A3筛筛板(三)","HBS2050(TTHBS-450-1)-c","上层棒条直径9mm，长度260mm，间距6mm；下层棒条直径7mm，长度210mm，间距4mm；棒条材质HBZL-5CrSiV；棒条布置角度15°","件",1,null,"烧结","2023-09-26"]
[14,5501400036,"烧结;A1筛筛板(一)","HBS2050(TTHBS-450-1)-a","上层棒条直径16mm，长度270mm，间距16mm；下层棒条直径13mm，长度320mm，间距12mm；棒条材质HBZL-5CrSiV；棒条布置角度18°","件",1,null,"烧结","2023-09-26"]
[15,5501600018,"离线筛弹簧","ASY0189F1","60SiMn GB13781-1992","只",12,"GB13781-1992","原料工段","2023-10-11"]
[16,5501800031,"全自动焦炭机械制球机筛片","KX-01",null,"件",1,"审核图纸","炼铁厂部","2023-09-26"]
[17,5400300027,"低氮天燃气烧嘴","SFSV   600N-300,  功率500KW","嘴前压力在于5KPA","套",2,"GB/T 35073-2018","180管加工热处理","2023-09-26"]
[18,5400300028,"低氮天燃气烧嘴","SFSV   400N-300, 功率360KW","嘴前压力在于5KPA","套",2,"GB/T 35073-2018","180管加工热处理","2023-09-26"]
[19,5400300029,"低氮天燃气烧嘴","SFSV   190N-250/185M","功率180KW，  嘴前压力在于5KPA","套",2,"GB/T 35073-2018","180管加工热处理","2023-09-26"]
[20,5600500023,"炉壁陶瓷碳枪芯","HG45C-001","带DN40法兰;长1500mm","件",30,"审核图纸","炼钢厂部","2023-09-26"]
[21,7101500103,"电动阀门装置","ADOK-40B","DN250;电源AC380V;环境温度-30℃~+80℃;频率50/60Hz;开闭时间30Sec;额定电流0.25A 扭矩400N·M","台",5,"JB/T8219-1999","炼钢厂部","2023-09-26"]
[22,6600300182,"电动开关阀HV107","DN40,PN25","公称压力：2.5MPa，通径40mm，温度197℃，阀体材质：ZG230-450,滤芯材质OCr 18Ni 9,带配套电动执行机构","台",1,"TS-2743018-2022","能源厂部","2023-09-26"]
[23,6600300183,"进气阀线性执行器","T5110010","\"行程：0-160mm\n电压：110V AC\n反应时间；2-5s\"","个",1,"JB/T8219-1999","能源厂部","2023-09-26"]
[24,7500300033,"风冷换热器","JD6-AC380V","风机功率0.75Kw;风机电压AC380V;风叶直径500mm;工作压力15bar;流量180L/min;工作介质68#脂肪酸脂液压油;附外形尺寸图","台",4,"JB/T4715-1992","炼钢厂部","2023-09-26"]
[25,5704000033,"线性导轨滑座","SHS55V2QZKKHHC1","JB/T7940-1999","件",30,"JB/T7940-1999","180热轧","2023-09-26"]
[26,5500500048,"助燃空气燃烧阀","DN1100，QZ741Y","通径：φ1100，工作压力0.45Mpa，介质：热空气，工作温度≤450℃，启闭时间≤12S，启闭压差：10Kpa，泄漏率≤3%，明杆楔式单向闸板闸阀，阀体及密封面：铸钢件，密封面堆焊硬质合金，阀盖：铸钢件，阀板及密封面：铸钢件，密封面堆焊硬质合金，阀杆：304不锈钢，阀杆采用动、静双层密封，密封材料采用粉末冶金环的迷宫环组，紧固件为8.8级，法兰密封面采用包覆式金属密封圈2片，带甘油润滑装置、成套紧固件及液压缸","台",1,"\"GB/T12238-2008\n\"","高炉","2023-09-26"]
[27,5500700004,"复膜防静电滤袋","直径130*6000","材质：涤纶/涤纶防静电基布 克重：500g/m2,厚度：2.0mm,透气量15m3/m2.min,经向拉力：>1100N/5×20cm,纬向拉力：>1200N/5×20cm，经向伸长：<35%，纬向伸长<55%，使用温度：≤130℃.","件",300,"HJ/T327-2006","高辅工段","2023-10-11"]
[28,5502000011,"低压脉冲袋式除尘器;骨架","直径124*5930","标准件 GB13871-1992","只",200,null,"高辅工段","2023-09-26"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2023年7月机械备件采购项目                    \n项目编号：HGJY-G2023115"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}