{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":64,"n_cols":12,"rows_kept":64,"merged":[[0,0,0,11],[1,0,1,11],[60,0,60,8],[61,0,61,8],[62,0,62,8],[63,0,63,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2023年8月电气备件采购项目                    项目编号：HGJY-G2023131"]
["序号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家"]
[1,6400200101,"激光测距仪安装支架","BEF-GH-DME;No.2015229","订货号No.2015229，SICK DME3000配套安装支架","IEC60947-5-1","件",2,"89油管车丝委外","2023-09-26"]
[2,6400600053,"传感器","LT600MQ21LU2X3-H1141","配附件","GB/T14048","只",1,"89油管车丝委外","2023-09-26"]
[3,6100300068,"断路器","DZX2-100 3P 80A","IEC 60898 额定电压400V 额定电流80A","IEC 60898","只",5,"检验检测中心","2023-09-26"]
[4,4000200074,"矩形瓷瓶","直径75*高95mm",null,"GB50300-2001","套",30,"物流中心","2023-09-26"]
[5,6400200028,"反光镜","H50",null,"GB/T14048","块",30,"89油管车丝委外","2023-09-26"]
[6,4100400172,"端子排","281-904;端板;281-329",null,"IEC947-7-1","节",400,"219厂部","2023-09-26"]
[7,6100100061,"控制变压器","BK-150","380V /36V GB/T18494.1-2001","GB/T18494.1-2001","台",3,"219厂部","2023-09-26"]
[8,6400300049,"接近开关","JLXK1-111","AC380V DC220V:5A:防护等级：IP62","JB/T 5553-2006","只",100,"89油管车丝委外","2023-09-26"]
[9,4100400086,"集电刷刀片","*","200A","CB/T 3668-1995","块",50,"物流中心","2023-09-26"]
[10,6300200030,"PLC模块I/O模块","接口模块 CI522A",null,null,"块",1,"340热轧","2023-09-26"]
[11,4000300246,"导轨","TS15","宽15MM;长1000MM;U型导轨;表面镀锌",null,"米",30,"180热轧","2023-09-26"]
[12,6200200327,"可控硅","MDC130A-16",null,"GB/T14315-2008","只",5,"180热轧","2023-09-26"]
[13,6100300069,"断路器","DZ158-100/3P","3P 100A","GB17701-2008","只",20,"炼钢厂部","2023-09-26"]
[14,4100500077,"开关箱","500*600*200","（未配任何开关）","GB7251.1","个",5,"180热轧","2023-09-26"]
[15,4100400173,"端子排","WAGO279-901；","100节/根","IEC947-7-1","根",2,"180热轧","2023-09-26"]
[16,6100600243,"熔断器","NGTC00;32A","1000V;50KA","GB13539 IEC 60269","个",9,"180热轧","2023-09-26"]
[17,6100600299,"快速熔断器","NGTC2 aR280A","RSM-1000;690V","GB13539 IEC60269","个",6,"180热轧","2023-09-26"]
[18,6100900007,"不锈钢仪控箱","HYYKX-600A1","CNS13551-1995","CNS13551-1995","套",2,"180热轧","2023-09-26"]
[19,4000400030,"开口型铜接线鼻子","适用于电缆 35mm2",null,"GB/T 14315-2008","只",50,"能源厂部","2023-09-26"]
[20,4100400218,"开口铜接线鼻子","100A，GB/T 14626",null,"GB/T 14626","只",50,"能源厂部","2023-09-26"]
[21,4100400221,"开口铜接线鼻子","150A，GB/T 14626",null,"GB/T 14626","只",50,"能源厂部","2023-09-26"]
[22,6400600064,"传感器 接插件","BCC-M425-0000-1A-004-PX0334-030","插头带LED灯 AWM 22AWG 80℃ 300V","GB/T26846-2011","只",20,"180热轧","2023-09-26"]
[23,6100500067,"中间继电器","CA-E31Q5N(3NO+1NC)",null,"GB/T22387—2008","只",10,"340管加工热处理","2023-09-26"]
[24,6300100129,"CPU模块","1756-L81E","1756-L81E","IEC61508","块",2,"219厂部","2023-09-26"]
[25,6100900158,"变频器柜","MD880-01S-0673-4-SG-CT","含变频器MD880-01S-0673-4-SG；进线断路器NSX800F TMD 800 3P3D F，熔断器HDLRT0-1000+熔芯 800A，制动单元MDBUN-200-T，EtherNet卡HETN-10，柜体GGD 800*2200*600","EN61800-3","套",2,"219厂部","2023-09-26"]
[26,6100200007,"电动隔离开关 合闸机构","3DC1026-5E 德国IEC947","额定工作电压36KV 额定电流2000A 控制电压AC220V 辅助触点4NO+4NC","德国IEC947","套",1,"炼钢厂部","2023-09-26"]
[27,6000200465,"真空断路器","3AH4305-4 Ur=36KV/Isc=31.5KA/Ir=2000A/屏柜NX-40.5 带小车 德国IEC947","德国IEC947","德国IEC947","台",1,"炼钢厂部","2023-09-26"]
[28,6100500246,"中间继电器","K22E","AC220V",null,"只",20,"炼钢厂部","2023-09-26"]
[29,6000400014,"电磁阀线圈","防水02-310122 DC24V",null,"GB/T14048","只",2,"340管加工热处理","2023-09-26"]
[30,6200200899,"制动电阻","3kW/18R","配CS710-4T30GB变频器，电阻值:18R,制动功率:3kW","IEC61800","台",2,"炼铁厂部","2023-09-26"]
[31,6000300253,"多合一智能电动机转子控制器","RSC1-M1-500R2-3","转子额定开路电压≤AC500v;用于三相交流电动机3段转子电阻器的控制","GB/T3235-1999","台",1,"炼钢厂部","2023-09-26"]
[32,6100900145,"多功能智能控制板","MFCHARGE","输入电压AC/DC110~245V;AO输出DC12V; 0~10V;DI输入;6输入;DO输出;6输出","GB/T16261-1996","块",1,"炼钢厂部","2023-09-26"]
[33,6100900146,"主控板","MFMC-200","输入电压AC/DC;110~245V;AO输出DC12V; 0~10V;DI输入;12输入;DO输出：8输出","GB/T16261-1996","块",1,"炼钢厂部","2023-09-26"]
[34,6100900147,"智能脉冲控制板","QLWKV3009","输入电压AC220V;输出;脉宽调制10路;AI输入;1路;DI输入;2路;DO输出;1路","GB/T16261-1996","块",1,"炼钢厂部","2023-09-26"]
[35,6200100093,"变频器","MD480T37GB","37KW","EN61800-3","台",3,"720厂部","2023-09-26"]
[36,6100300302,"固定式断路器","HD4s-40.5MX-1600A-25kA","额定电压40.5KV;额定频率50Hz;额定电流1600A;3秒热稳定电流（有效值）25kA;额定动稳定电流（峰值）63kA;额定短路开断电流25kA;额定短路关合电流63kA;辅助电源电压;控制回路DC220V;储能电机DC220V;合闸时间55-67ms;分闸时间33-45ms;燃弧时间＜15ms;合闸弹跳时间≤2mS;机械循环寿命10000次;电气循环寿命符合E2级规定;ABB","GB1984-2001","台",1,"炼钢厂部","2023-09-26"]
[37,6000201084,"高频电源冷却风机","W2E250—HL06-01","AC 230V  50Hz  0.66A  127W","JB/T10391-2002","台",10,"炼铁厂部","2023-09-26"]
[38,6100900160,"变频控制柜","柜体尺寸：宽*深*高为800mm*600mm*2150mm;","风机水泵负荷；每台变频器柜为2台功率为75Kw风机水泵提供动力；具体配置：2套进线电源开关；带配套进出线电抗器；2套变频器型号为：MD480T55G-PLUS（品牌为汇川）；变频器与AB公司Logix5000PLC通过EIP通讯卡进行通讯（型号：MD500-EN1）；供货方负责变频控制柜及与PLC的现场通讯调试","GB/T12668.2-1989","套",3,"340管加工热处理","2023-09-26"]
[39,6400600177,"温度继电器","ETS388-5-150+TFP100+S.S+ZBE08+ZBM300","测量范围0-100℃ 精度等级正负1% 4个开关量输出带换向触点，1个模拟输出4-20mA 耐振，耐冲击",null,"只",2,"180厂部","2023-09-26"]
[40,4000200367,"AC380V 63A工业插头","插头：NTC1-563P6H/415V   ；63A 5极 ；电压等级415VAC",null,"GBT 11918-2014","个",20,"340热轧","2023-09-26"]
[41,4000200368,"AC380V 63A工业插座","插座：NTC1-563AS6H/415V；63A 5极；电压等级415VAC",null,"GBT 11918-2014","个",10,"340热轧","2023-09-26"]
[42,4000200369,"AC220V 16A工业插头","插头：NTC1-316P6H/250V;16A 3极;电压等级250VAC",null,"GBT 11918-2014","个",20,"340热轧","2023-09-26"]
[43,4000200370,"AC220V 16A工业插座","插座：NTC1-316AS6H/250V ；16A 3极；电压等级250VAC",null,"GBT 11918-2014","个",10,"340热轧","2023-09-26"]
[44,4000200371,"AC36V工业插头","插头;CEE-012 ；电压等级36VAC，",null,"GBT 11918-2014","个",20,"219厂部","2023-09-26"]
[45,4000200372,"AC36V工业插座","插座：CEE-312；16A；电压等级36VAC",null,"GBT 11918-2014","个",5,"219厂部","2023-09-26"]
[46,4000300255,"电缆桥架盖板","2000mm*100mm*1.5mm（长*宽*厚）","材质：镀锌钢板","GB/T 5117-1995","米",40,"180热轧","2023-09-26"]
[47,4000300256,"电缆桥架盖板","2000mm*200mm*1.5mm（长*宽*厚）","材质：镀锌钢板","GB/T 5117-1995","米",40,"180热轧","2023-09-26"]
[48,4100400292,"电缆桥架","50*50*1.0  宽*高*厚   单位：mm","材质：镀锌钢板，线槽与盖板同长，配相应数量的连接板和螺丝","GB/T 5117-1995","米",100,"219厂部","2023-09-26"]
[49,4100400293,"电缆桥架","100*75*1.0   宽*高*厚  单位：mm","材质：镀锌钢板，线槽与盖板同长，配相应数量的连接板和螺丝","GB/T 5117-1995","米",100,"219厂部","2023-09-26"]
[50,4100400296,"工业航空插头","NTC1-532P6h/415V插头","5芯:额定电流:32A,额定电压415V:防护等级：IP44;厂家:浙江正泰","GB/T 11918.1","个",20,"340热轧","2023-09-26"]
[51,5100300084,"抱闸电控箱","EXE800一2E","输入交流380V；\n输出直流65V；启动12V;维持\n瞬间启动电流36A,功率2500W;\n维持电流6.7A,功率100W\"","JB14048.11","台",1,"340热轧","2023-09-26"]
[52,6000300265,"电机抱闸整流器","RH555","555V ;2A;输入380V,输出直流220V；UHT","GB3859-93","个",3,"180热轧","2023-09-26"]
[53,6100100224,"中频炉变压器","ZP-300-BYQ","功率300千瓦，变比20：2  电压1200伏，中频谐振电流1500安  尺寸800x500x450mm 水压≥0.3MPa","GB/T18494.1-2001","台",1,"219厂部","2023-09-26"]
[54,6200200920,"功率单元","HD9MS-A069-0080-500010","01290141","GB/T14315-2008","台",1,"能源厂部","2023-09-11"]
[55,6400600554,"激光测距传感器","O1D100-O1DLF3KG","18...30 DC，量程10 m   2 个开关输出；可将其中一个编程为4-20mA输出，使用寿命 [h]50000   安装附件：M12 5Pins输出插头或者插头线","IEC 61131-2","只",1,"219厂部","2023-10-26"]
[56,6400600555,"传感器7针插头","No.560701+530029 D70  带25米线","No.560701+530029 带线25米线; MTS 灰数据（-） 粉红数据（+） 黄时钟（-） 绿时钟（-） 棕+24VDC(-15/+20%) 白电源地 M16mm连接器接口。","IEC60176-2-106-2011","根",5,"180热轧","2023-09-26"]
[57,6400600079,"内置式位移传感器","BTL5-S172-M0500-B-KA05","检测长度500mm 配磁环","GB/T28857-2012","只",2,"炼钢厂部","2023-09-26"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误\n3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2023年8月电气备件采购项目     项目编号：HGJY-G2023131"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}