{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":43,"n_cols":13,"rows_kept":43,"merged":[[0,0,0,8],[1,0,1,12],[39,0,39,8],[40,0,40,8],[41,0,41,8],[42,0,42,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2023年8月机械备件采购项目                    项目编号：HGJY-G2023134"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,5708000005,"带锯机;夹紧装置滑座(油缸端);G4240/60","*",null,"件",1,"JB/T4318.4-2002","219厂部","2023-10-26"]
[2,5704000016,"线性导轨","LINEAR GUIDESHS55V2QZKKHHC1+1500LSF690143MFL",null,"件",2,null,"180热轧","2023-10-26"]
[3,5100100425,"离心水泵六爪弹性圈","IS100-65-200","外径110，内径50，六爪弹性水泵弹性体","只",10,"JB/T7511-1994","能源厂部","2023-10-26"]
[4,6200100084,"16夹头","LD45(DJ)-010119","材质铬锆铜CrZrCu；重量0.72KG","对",5,"审核图纸","180热轧","2023-10-26"]
[5,5711300039,"紧定套","H3144","组件 GB/T9160 1-93","套",5,"GB/T9160","340热轧","2023-10-11"]
[6,7102200003,"遥控浮球阀用浮球和导阀","G1/2",null,"台",2,"QB/T1199-1991","180管加工热处理","2023-09-26"]
[7,5900100004,"带锯机夹钳","行程大于800mm，挡板高大于600mm","行程大于800mm，挡板高大于600mm，包含横梁，同步齿轮、齿条；适用于GB4280C双立柱卧式带锯床","套",1,"JB/T4318","检验检测中心","2023-10-26"]
[8,6600400005,"吸尘器","科乐C-0419,水过滤 干湿两用",null,"台",1,"GB4706.1-1998","检验检测中心","2023-10-26"]
[9,7001200011,"高压泵 除磷环喷嘴紫铜垫","*",null,"只",50,"JB/T9872-2000","340热轧","2023-10-26"]
[10,5501400036,"烧结;A1筛筛板(一)","HBS2050(TTHBS-450-1)-a","上层棒条直径16mm，长度270mm，间距16mm；下层棒条直径13mm，长度320mm，间距12mm；棒条材质HBZL-5CrSiV；棒条布置角度18°","件",1,null,"烧结","2023-10-26"]
[11,5501600018,"离线筛弹簧","ASY0189F1","60SiMn GB13781-1992","只",12,"GB13781-1992","原料工段","2023-10-11"]
[12,5600500023,"炉壁陶瓷碳枪芯","HG45C-001","带DN40法兰;长1500mm","件",30,"审核图纸","炼钢厂部","2023-10-26"]
[13,6000200375,"轴流风机","T35-14.2-4","固定式 不带支架 电机功率7.5Kw","台",2,"GB/T13274-1991","炼钢厂部","2023-10-26"]
[14,6600300183,"进气阀线性执行器","T5110010","\"行程：0-160mm\n电压：110V AC\n反应时间；2-5s\"","个",1,"JB/T8219-1999","能源厂部","2023-10-26"]
[15,5704000033,"线性导轨滑座","SHS55V2QZKKHHC1","JB/T7940-1999","件",30,"JB/T7940-1999","180热轧","2023-10-26"]
[16,7502500043,"轴流风机","BSFT-300","AC220V;0.55Kw;配10米风管手提式；防爆","台",1,"GB/T11800-2008","能源厂部","2023-10-11"]
[17,5500300119,"（新）开口机送进装置","SLYZ1000-0314","含送进马达；马达型号：6K-490；","台",1,"JB/T12471-2015","高炉","2023-10-26"]
[18,5501000069,"槽上卸矿车","K103Tr","皮带宽度：1000mm；最大输送能力：600t/h；最高带速：2m/S；皮带托辊直径：Φ108；小车皮带斜面：12°；有打滑检测装置；有跑偏检测装置；有防堵料检测装置；蜗杆减速机型号：MNAT97-YEI11-4P-163.64-M3-B-270；总计重量约12吨","台",1,null,"高辅工段","2023-09-11"]
[19,5500700004,"复膜防静电滤袋","直径130*6000","材质：涤纶/涤纶防静电基布 克重：500g/m2,厚度：2.0mm,透气量15m3/m2.min,经向拉力：>1100N/5×20cm,纬向拉力：>1200N/5×20cm，经向伸长：<35%，纬向伸长<55%，使用温度：≤130℃.","件",300,"HJ/T327-2006","高辅工段","2023-10-11"]
[20,5502000011,"低压脉冲袋式除尘器;骨架","直径124*5930","标准件 GB13871-1992","只",200,null,"高辅工段","2023-09-26"]
[21,5501800024,"整套圆盘（不含减速机）","PDX25HLS","定量圆盘给料系统，盘面直径2500，硬齿面回转轴承QND900.25AZ，底架组装件,盘面及附属密封、管路螺栓等，不包括减速箱及减速箱润滑系统。","套",1,null,"原料工段","2023-09-26"]
[22,7101800253,"三通球阀","KH3K-DN32-SAE420-112A-L-06","DN32;31.5MPa","只",2,"GB/T9065.2-2010","检验检测中心","2023-09-26"]
[23,7101800078,"高压球阀","BKH-10S-1123",null,"只",8,"GB/T9065.2-2010","89热轧","2023-09-26"]
[24,5300300877,"软化水处理机","DLSCLR2","2吨","台",1,"GB/T12688.2-1989","物流中心","2023-09-26"]
[25,5603200031,"布袋","V350-4400;玄武复合","耐高温滤袋","条",250,"GB12625-1990","炼钢厂部","2023-09-26"]
[26,7001500003,"罗茨真空泵","DDR40000（2030144）","极限压力0.03Pa;抽速40000m3/h;转速Max3600r/min;功率37Kw;带电机","台",1,"Q/SOEU17-2007","炼钢厂部","2023-09-26"]
[27,7101300021,"对夹式蝶阀密封内衬","适用于Z011-A-PN6-DN350蝶阀","材质：EPDM","件",1,"GB/T8100-2006","炼钢厂部","2023-09-26"]
[28,7101300022,"对夹式蝶阀密封内衬","适用于Z011-A-PN16-DN250蝶阀","材质：EPDM","件",5,"GB/T8100-2006","炼钢厂部","2023-09-26"]
[29,7101300023,"对夹式蝶阀密封内衬","适用于Z011-A-PN16-DN300蝶阀","材质：EPDM","件",1,"GB/T8100-2006","炼钢厂部","2023-09-26"]
[30,7101300024,"法兰蝶阀密封内衬","适用于F012-K1 DN800蝶阀","材质：EPDM","件",2,"GB/T8100-2006","炼钢厂部","2023-09-11"]
[31,7101600218,"气动开关蝶阀","Z011-A-PN16-DN300","阀体材质:球墨铸铁GGG-40;阀板材质;不锈钢1.4408;阀杠材质;2Cr13;阀座密件;EPDM;连接方式;对夹;阀板工作压力;16bar","只",3,"GB/T8100-2006","炼钢厂部","2023-09-26"]
[32,7501300120,"复式轴向波纹补偿器","FL600-2150","DN600;PN0.25MPa;工作介质：高炉煤气；温度≤250℃;补偿器材质：INCOLOY825 ；两侧波纹管：3+3波，（三层波纹），每层厚度0.8mm，；内衬管表面有5mm厚陶瓷耐磨涂层。两侧波纹管+中间连接管；单侧补偿器长度300mm，一侧波纹管法兰连接，总长2150mm。","只",15,"GB/T12777-1999","高辅工段","2023-09-26"]
[33,7501300121,"大拉杆波纹补偿器","FL1800-0.25-250-5150","DN1800;PN0.25MPa;补偿量250mm；L=5150mm;介质：高炉煤气；工作温度≤250℃;补偿器材质：INCOLOY825；波纹管：3+3波，三层波纹成型，单层厚度δ≥0.8mm。","只",1,"GB/T12777-1999","高辅工段","2023-09-26"]
[34,7502500114,"酸雾净化塔配套风机","LXBF4-4.5#-4BP","聚丙烯防腐蚀离心风机；电机功率4KW AC380V，风量：2250-7470m3/H；风机风压：2001-1315Pa，安装方式：卧式，安装额定频率：50 Hz；冷却方式：IC411；防护等级：IP54；绝缘等级：F；环境温度：-15 ~ 40℃","台",1,"GB18613-2012","检验检测中心","2023-09-26"]
[35,5400300040,"3#线淬火炉均热段烧嘴","BSPG125HLR","150kw;功率调节比1:10；燃烧室：烧嘴砖：嘴前最低压力：3.5Kpa；燃气温度：常温；嘴前空气最低压力3.5Kpa；空气温度：约430℃","套",18,"审核图纸","180管加工热处理","2023-10-26"]
[36,5722600120,"锯床导向臂","导向臂长535，上宽110，下宽75","G4240/50锯床专用","台",2,"JB/T 4318.4-2002","180管加工热处理","2023-10-26"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2023年8月机械备件采购项目         项目编号：HGJY-G2023134"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}