{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["一、开标一览表","二、商务 技术偏离"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"一、开标一览表","index":0,"n_rows":71,"n_cols":11,"rows_kept":71,"merged":[[0,0,0,10],[1,0,1,10],[68,0,68,10],[69,0,69,10],[70,0,70,10]],"flags":["formulas_cached_only"]}
["开  标  一  览  表"]
["项目名称：2023年10月-2024年9月照明器具备件年标采购项目          项目编号：HGJY-G2023153"]
["序号","物料编码","物料描述","规格描述","技术参数","单位","数量","交货日期","含税单价（元）","生产厂家","备注"]
[1,"4000100006","LED泛光灯","NFK3613",null,"只",150,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[2,"4000100007","LED工矿灯","NE-8631","飞利浦照明 额定电压86-260V 额定功率正白光","盏",60,"以订单为准",null,null,"需求量以订单为准"]
[3,"4000100008","LED路灯","LHD-L96WL04","96w 电源效率>90% 平均照度>28LUX","只",50,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[4,"4000100016","安全出口指示灯","(安全出口、左向标示、右向标示、双向标示)GB19261-2009",null,"盏",100,"以订单为准",null,null,"需求量以订单为准"]
[5,"4000100017","安全橡皮行灯","GC30-B","36V 60W 电压等级36V","盏",200,"以订单为准",null,null,"需求量以订单为准"]
[6,"4000100019","厂房照明LED灯","100W","85~265VAC 色温2700K~6500K可选 寿命>50000h","盏",200,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[7,"4000100027","灯具","70W","LED,220V,70W,新曙光","盏",100,"以订单为准",null,null,"需求量以订单为准"]
[8,"4000100028","灯具","HPK518","1*HPI-P400W-BUIC220/50","盏",10,"以订单为准",null,null,"需求量以订单为准"]
[9,"4000100029","灯具","SL170-8U.C2",null,"盏",15,"以订单为准",null,null,"需求量以订单为准"]
[10,"4000100030","灯泡","15W","螺口","只",50,"以订单为准",null,null,"需求量以订单为准"]
[11,"4000100032","灯泡","NTC9210400W",",灯头螺口、E27、400W，海洋王、防振投光灯NTC9210","只",40,"以订单为准",null,null,"需求量以订单为准"]
[12,"4000100034","低压灯泡","60W","36v","只",500,"以订单为准",null,null,"需求量以订单为准"]
[13,"4000100039","电子日光灯架","30W","30W","支",50,"以订单为准",null,null,"需求量以订单为准"]
[14,"4000100046","防尘高顶灯","NGC9810","NGC 9810 A250，220VAC，英制1/2内丝接口","盏",20,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[15,"4000100047","防眩泛光灯","NFC9180","150W","盏",10,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[16,"4000100049","防雨灯头","*","250V","只",100,"以订单为准",null,null,"需求量以订单为准"]
[17,"4000100050","防震型投光灯","NTC9210A-N250","250W 220VAC 支架安装","盏",20,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[18,"4000100051","防震型投光灯","NTK4021","NTK4021","盏",50,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[19,"4000100059","工作灯","FW6580","海洋王,LED防爆泛光灯000.1-2007,LED防爆泛光灯、海洋王","盏",4,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[20,"4000100060","工作行灯","XD-36-60",null,"只",200,"以订单为准",null,null,"需求量以订单为准"]
[21,"4000100061","固态免维护防爆灯","BFC8183","220V","盏",30,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[22,"4000100065","环形吸顶灯","32W",null,"盏",20,"以订单为准",null,null,"需求量以订单为准"]
[23,"4000100066","机床照明灯","FX-JCF20","20W AC85V-220V 防护等级IP65","盏",10,"以订单为准",null,null,"需求量以订单为准"]
[24,"4000100069","节能灯","YPZG","220/26-3U-26W 螺口","盏",100,"以订单为准",null,null,"需求量以订单为准"]
[25,"4000100070","节能灯泡","*","（螺口）,自镇流汞灯、灯头螺口、E27、160W、自整流","只",200,"以订单为准",null,null,"需求量以订单为准"]
[26,"4000100088","螺口吊灯头","*","250V","只",100,"以订单为准",null,null,"需求量以订单为准"]
[27,"4000100090","螺旋节能灯","9W","E27 冷光","只",30,"以订单为准",null,null,"需求量以订单为准"]
[28,"4000100091","螺旋节能灯","18W","E27 暖光","只",50,"以订单为准",null,null,"需求量以订单为准"]
[29,"4000100093","平面节能灯泡","SL85-4U.C","220V 0.39A,节能灯、85W 220V 0.39A、苏州圣路 SL85-4U.C","只",50,"以订单为准",null,null,"需求量以订单为准"]
[30,"4000100096","嵌入式吸顶灯","MQ105-Y13",null,"盏",20,"以订单为准",null,null,"需求量以订单为准"]
[31,"4000100097","强光灯","NTC9230","投光灯 海洋王","套",5,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[32,"4000100109","手提式防爆探照灯","RJW7101/LT","内置电池 可充电型","盏",5,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[33,"4000100110","手提式防爆探照灯","RJW7102","内置电池，可充电型","盏",5,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[34,"4000100111","手提式强光巡检工作灯","IW5500/BH",null,"盏",5,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[35,"4000100114","天棚灯","HNGC996-HP400B-M/TC","220VAC 400W 可选吊环或支架安装","盏",10,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[36,"4000100117","投光灯","HNGT192-HP400/TC","400W220V","盏",30,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[37,"4000100120","微型防爆头灯","IW5130","LED头灯、海洋王","盏",30,"以订单为准",null,null,"需求量以订单为准"]
[38,"4000100123","消防应急照明灯","DYB-3X2/90-002","220V 8W 停电应急照明90分钟","盏",15,"以订单为准",null,null,"需求量以订单为准"]
[39,"4000100139","LED配电房专用灯","BD-A95;","30W;220-240V;斑点照明","盏",200,"以订单为准",null,null,"需求量以订单为准"]
[40,"4000100141","LED日光灯管","*","15W  220V","根",200,"以订单为准",null,null,"需求量以订单为准"]
[41,"4000100143","防爆灯","FGL-L-L150-B1-Z",null,"盏",5,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[42,"4000100149","LED高顶防爆灯","GF9042","100W 220V","盏",15,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[43,"4000100151","多用途泛光灯具","RVP350","HPI-T400W 220V 50HZ SSPCN","盏",5,"以订单为准",null,null,"需求量以订单为准"]
[44,"4000100153","防爆平台灯","BPC8720 150W",null,"盏",30,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[45,"4000100156","车床工作灯","*","2-3节","盏",10,"以订单为准",null,null,"需求量以订单为准"]
[46,"4000100157","LED日光灯管","1200mm长;15W;220V",null,"支",100,"以订单为准",null,null,"需求量以订单为准"]
[47,"4000100163","集成吊顶平板led灯","尺寸600*600；雷士","电压220VAC;功率48W;单驱动；铝合金型材拉丝边框","盏",40,"以订单为准",null,null,"需求量以订单为准"]
[48,"4000100169","LED长臂数控机床工作灯","40F，铝合金材质，长臂，固定底座，灯头开关","功率：5-7/9/12/35W；电压：24V","盏",2,"以订单为准",null,null,"需求量以订单为准"]
[49,"4000100176","一体式LED太阳能路灯","SL-TX-0050hy","灯光通量24001m;色温5700K;光衰1万小时<5%;光效160lm/w;IP66;灯具材质:高端铝合金、电池:3.2v、50Ah,锂电池;控制方式:光控、分时段调光智能控制","套",5,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[50,"4000100177","LED吸顶灯芯灯板","220VAC；24W","圆形；白色；一体化透镜模组；磁铁吸附；光通量2160LM","块",10,"以订单为准",null,null,"需求量以订单为准"]
[51,"4000100178","道路照明路灯杆","102型；灯杆8米","白色；含预埋件；灯杆热镀锌；不含灯具","根",5,"以订单为准",null,null,"需求量以订单为准"]
[52,"4000100194","LED日光灯","CLX-PC40","工作电压220VAC；1.2米40瓦；正白光6500K；光效≥130Lm/w；飞利浦双排芯片；PMMA材质灯罩；一体化底座（含安装卡扣）","套",10,"以订单为准",null,null,"需求量以订单为准"]
[53,"4000100195","LED吸顶灯","CLX-BE36","功率36w；飞利浦芯片；光效≥130Lm/w、智能IC驱动；圆形；白光","套",5,"以订单为准",null,null,"需求量以订单为准"]
[54,"4000100197","软管射灯","220V 10W；15度~45度聚光；明装型；黑壳白光","15度~45度聚光；明装型；220V 10W；黑壳白光","件",10,"以订单为准",null,null,"需求量以订单为准"]
[55,"4000100200","多功能照明灯","SZSW2951","50W～100W 5700K±300K WF2 ≥100000h GB 7000.1 欧司朗光源 IP66","台",10,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[56,"4000100201","天棚照明LED灯","LED 200W 工矿灯","功率(W):200W; 电压:86~265VAC; 光效(Lm/W): 120 ; 色温(K): 6000;显色性:80; 防护等级:IP65; 防腐等级:WF2; 平均寿命(小时):≥50000; 芯片品牌:飞利浦; 驱动品牌:明纬/茂硕","盏",50,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[57,"4000100205","LED顶棚照明灯","HB-JL06-150W","额定电压/频率：85--265VAC/50--60HZ，额定功率：150W（174*1.0W/LED模块），额定电流3.75A，IP等级：IP65，ta：40℃；色温：6000K；RA>80，光效：160lm/w，配光曲线：120°","盏",100,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[58,"4000100208","LED 壁挂防爆泛光灯","100W-LED防爆灯","\"整灯光效:≥140 lm/W；防爆标志:Ex mc nR IIC T4/T6 Gc/Ex tD A22 IP66 T130C ；绝缘等级:I类 ；额定电压:AC220V，50-60Hz色温:5700K； 防护等级:IP66 ；配用光源:LED(OSRAM、CREE)；额定功率:100W\n\"","盏",30,"以订单为准",null,null,"投标须为直供厂家，需求量以订单为准"]
[59,"4000100215","充电照明LED灯","VPU-P60","≤36V;600W；直接195mm，高度80mm；带原装充电器，四档可调档位，续航时长8-48小时；品牌：威浦","盏",20,"以订单为准",null,null,"需求量以订单为准"]
[60,"4100600052","多功能信号灯","MSL4730",null,"盏",5,"以订单为准",null,null,"需求量以订单为准"]
[61,"4000100052","高亮度手电筒","JW7622","LED手电筒、海洋王","只",100,"以订单为准",null,null,"需求量以订单为准"]
[62,"4000100125","袖珍防爆调光手电筒","JW7210",null,"只",30,"以订单为准",null,null,"需求量以订单为准"]
[63,"4000100144","防爆电筒","JW7300",null,"个","6","以订单为准",null,null,"需求量以订单为准"]
[64,"4000100175","强光防爆电筒","SW2102","防爆标志：Exd IIC T6 Gb\n光源：LED\n额定功率：3W\n额定电压：3.7V\n额定容量：2.6Ah\n平均使用寿命:100000h\n连续放电时间：强光≥4h\n                        工作光≥8h\n充电时间：4~6h\n电池使用寿命：1000次循环以上\n防护等级：IP66\n外形尺寸：Φ40x142mm\n重量：205g","件",5,"以订单为准",null,null,"需求量以订单为准"]
[65,"4201700065","警用强光电筒","0",null,"个",30,"以订单为准",null,null,"需求量以订单为准"]
["注：1、投标报价含税，税率13%                                                                                     \n2、生产厂家要求全称填写准确无误"]
["投标人：（盖单位章）"]
["法定代表人或其委托代理人：（签字或盖章）"]

{"sheet":"二、商务 技术偏离","index":1,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2023年10月-2024年9月照明器具备件年标采购项目          \n项目编号：HGJY-G2023153"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位公章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]